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PATCHCROSS（ATV525/625）          

 SERVICE MANUAL
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This manual is general version, the pictures in manual book are 

little difference compared with real part, so please check real part 

accordingly.
SHANDONG ODES INDUSTRY CO., LTD. 

Foreword  

This manual contains such content as introductions on overhaul, maintenance, overhauling program, dismantling, assembling, troubleshooting and service data of ATV525 and ATV625.
	Covered Models

	PATHCROSS ATV 525L/S

	TCROSSER ATV 525L/S

	PATHCROSS ATV 625L

	TCROSSER ATV 625L

	PATHCROSS ATV 625L MUD Version

	TCROSSER ATV 625L MUD Version


This manual will help you know the vehicle beter so that you can assure your customers of fast and reliable service.

This manual hass been prepareed on the basis of the latest specifications at the time of publication. If modifications have been made sine then,   differences may exist between the content of this manual and the actual vehicle.  

Illustrations in this manual are used to show the basic principles of operation and work procedures. They may not represent the actual vehicle exactly in detail. 

Manufacturer reserves the right of no prior notice on product improvement or modification. Repair and maintenance shall be carried out according to actual situation of vehicle. 
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WARNING

	Inexperienced mechanics or mechanics without the proper tools and equipment may not be able to properly perform the services described in this manual.

Improper repair may result in injury to the mechanic and may render the vehicle unsafe for the rider.
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1.1 VEHICLE APPEARANCE

ATV525/ATV625 Vehicle left-hand view 
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	1. Headlight
	2. Front cargo rack 
	3. Display
	4. Auxiliary DC jack

	5. Ignition switch
	6. Front seat
	7. Rear seat back
	8. Rear cargo rack 

	9. Front wheel 
	10. Engine
	11. Rear wheel 
	12. Fuel Tank


ATV525/ATV625 Vehicle right-hand view 
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	1. Tail light 
	2. Muffler 
	3. Shifting lever
	4. Radiator

	5. Rear brake 
	6. Rear shock absorber 
	7. Front shock absorber 
	8. Front brake 


1.2 MARKER INFORMATIVENESS
Numbers of frame (or VIN code), engine and transmission case are major information numbers of a motorcycle. When ordering components or authorizing special services, these numbers are able to assist distributors to serve you better. 

Motorcycle mark information is shown as follows: 
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TYPICAL-ATV525/625 LEFT VIEW (long wheelbase)       TYPICAL-ATV525/625 RIGHT VIEW (long wheelbase)
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TYPICAL
1. PIN/VIN (Vehicle Identification Number on right side/anterior portion on the frame)

2. EIN (Engine Identification Number on left side/top of the crankcase)

1.3 PRECAUTIONS

1.
Do not make engine under operation at a closed place or place with poor ventilation for a long time. 

2.
If engine stops operation, please do not touch it or muffler to avoid burning. 

3.
Due to high corrosiveness, battery fluid may cause burns to skin and eyes. In case of splashing to skin, please clean it with water and contact the doctor immediately. In case of splashing to clothes, please wash it with water immediately. Keep battery fluid far away from children. 

4.
Cooling liquid is toxic. Do not drink it or splash it to skin, eyes and clothes. Once splashing it to skin, please wash it with a lot of soapy water. In case of splashing to eyes, please wash eyes immediately and contact the doctor. In case of drinking cooling liquid, resulting in vomit, please contact the doctor. Keep cooling liquid far away from children. 

5.
Wear proper working suit, boots and hat. If necessary, please wear long-sleeve working suit and gloves for operation.  

6.
Gasoline is highly inflammable. No smoking or firing. At the same time, fire sparks shall be avoided. Vaporized gasoline is explosive as well. Operation shall be carried out at places with good ventilation. 

7.
Battery may produce explosive hydrogen in charging. Please ensure charging at places with good ventilation. 

8.
Use legal parts, lubricating oil and lubricating grease. 

9.
Before overhauling, please clean soil and dust. 

10.
Keep accessories of each part well for correct assembly. 

11.
Replace dismantled gasket, O-ring, piston pin retainer and cotter pin. 

12.
Retainer of rubber ring may be deformed after dismantling. So, please do not use loose and soft retainer. 

13.
Please wash and dry dismantled parts. Use lubricant on the surface of moving parts. For correct installation, please measure data well in dismantling process. 

14.
If do not know length of screw, please install screws one by one to ensure their corresponding depth. 

15.
Pre-tighten bolts and nuts and then tighten them with designated torque from the big to the small and from the inside to the outside. 

16.
Check whether rubber parts are aged. If necessary, replace them. Keep rubber parts far away from grease. 

17.
If necessary, special tools can be used. 

18.
Rotate inside and outside races of bearing to ensure flexibility of balls. 

a) If axial or radial resistance is too large, please replace it. If there is concave-convex on the surface, please use oil for washing. If no effect is achieved with washing, please replace it. 

b) If bearing cannot be clamped tightly in pressing into machine or axle, please replace bearing. 

19.
Please install a side dust proof bearing at correct direction. In installation of open or double-face dust proof bearing, pay attention to that marks of manufacturer shall be outward. 

20.
In cleaning and drying bearing, please keep bearing support still. Before installation, please carry out lubrication with oil or lubricating oil. 

21.
Please correct install elastic retaining ring. Assembling after opening can ensure installation of snap ring into slot. 

22.
After assembly, please check whether all parts are of perfect tightening and flexible movement. 

23.
Brake fluid and coolant may damage shell and plastic and rubber parts. In case of being splashed by them, please use water to wash. 

24.
In installing pipe, please insert them to bottom of connecting pipeline. In installing pipe clamp, please install them to groove if there is. As for pipeline or pipe clamp that cannot be tightened, please replace them. 

25.
Do not mix soil or dust into engine and/or hydraulic braking system. 

26.
Before installation, please clean gasket and spacer of engine shell. Use oil stone to polish scratch of joint face evenly. 

27.
Do not twist or bend too much cable. Twisted or damaged cables may cause inflexible operation. 

28.
In assembling protective caps of parts, insert cap into groove if any. 

1.4 Engine brake-in steps

Though quality material has been used for motorcycle manufacturing and all components are conforming to high quality standard, all components and parts shall subject to brake-in process before engine reaching maximum load. The reason behind this is that cooperation of components has not reached the best status after their assembling. This leads to damping force of engine and unnecessary mechanical loss. The ideal cooperation can be reached after operation for some time. In this case, mechanical loss can be minimized, reaching the best status and bringing the output power to maximum value. As a result, engine performance directly relates to initial maintenance. Regulation of running-in process is shown as follows:

· Please follow the restriction requirements for engine speed in the brake-in period below:

	The first 150km
	Below 5000 rpm

	Till 800km
	Below 5500 rpm

	Till 1600km 
	Below 6500 rpm 

	Above 1600km  
	Below 8500 rpm 


· Do not fully open the accelerator before the reading of the odometer reaching 1000km. 

Attention: the speed shall not exceed 6500 rpm no matter what in brake-in period. 

- During the brake-in period, the engine shall not work at the same speed with the same gear position for a long time. Try to shift gear position and speed to facility running-in of components.

- After 1000km of operation, transmission and crank cases shall be cleaned thoroughly. 

1.5 TIGHTENING TORQUE 

Locking devices (e.g.: locking tabs, elastic stop nuts, self-locking fasteners, etc.) must be installed or replaced with new ones, where specified. If the efficiency of a locking device is impaired, it must be renewed.

In order to avoid a poor assembling, tighten screws, bolts or nuts in accordance with the following recommended torque value:

	Grade
	Torque( N·m)

	
	M6
	M8
	M10
	M12
	M14
	M16

	4.6
	4～5
	10～12
	20～25
	36～45
	55～70
	90～110

	5.6
	5～7
	12～15
	25～32
	45～55
	70～90
	110～140

	6.8
	7～9
	17～23
	33～45
	58～78
	93～124
	145～193

	8.8
	9～12
	22～30
	45～59
	78～104
	124～165
	193～257

	10.9
	13～16
	30～36
	65～78
	110～130
	180～201
	280～330

	12.9
	16～21
	38～51
	75～100
	131～175
	209～278
	326～434


CAUTION: Be sure to use the proper tightening torque for the proper strength grade. Always torque screws, bolts and/or nuts in a crisscross sequence.

2. PERIODIC MAINTENANCE
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2.1 MAINTENANCE SCHEDULE 

In order to maintain the best performance and economical performance of vehicles, suggestions on intervals for necessary regular maintenance are listed. Following maintenance is calculated in km, mile and hour based on firstly appeared data. 

However, keep in mind that if the vehicle isn’t used for a long period of time, the month maintenance intervals should be followed.

Items marked with an asterisk should be performed by a dealer as they require special tools and technical skills.

In case of complicated road conditions, regular maintenance shall be carried for vehicles. 

	ITEM
	ROUTINE
	Whichever

Comes first

[image: image400.png]



	
	INTIAL
	EVERY

	
	
	
	month
	1
	3
	6
	6
	12

	
	
	
	Km

(mi)
	320

(200)
	1,200

(750)
	2,400

(1,500)
	2,400

(1,500)
	4,800

(3,000)

	
	
	
	hours
	20
	75
	150
	150
	300

	Valves*
	● Check vale clearance. 

● Adjust if necessary.
	O
	
	O
	O
	O

	Cooling system
	● Check coolant leakage.

● Repair if necessary.

● Replace coolant every 24 months.
	O
	O
	O
	O
	O

	Seal for 
water pump
	● Check whether water in the breather hose for water pump.
	O
	O
	O
	O
	O

	Spark plug
	● Check condition.

● Adjust gap and clean.

● Replacement every 24 months
	O
	O
	O
	O
	O

	Air filter elements 
	● Clean.
● Replacement every 24 months
	Every 20-40 hours

(More often in wet or dusty areas.)

	Crankcase breather system*
	● Check breather hose for cracks or damage.

● Replace if necessary.
	
	
	O
	O
	O

	Exhaust system*
	● Check for leakage. 

● Tighten if necessary.

● Replace gasket(s) if necessary.
	
	
	O
	O
	O

	Spark arrester
	● Clean.
	
	
	O
	O
	O

	Fuel hose*
	● Check fuel hose for cracks or damage.

● Replacement fuel hose every 48 months
● Replacement fuel filter every 24 months
	
	
	O
	O
	O

	Engine oil
	● Replace (Check oil level every month).
	O
	
	O
	O
	O

	Engine oil filter
	● Replace.
	O
	
	O
	
	O

	Differential oil
	● Check oil level/oil leakage.

● Replacement every 24 months.
	O
	
	
	
	O

	Brake*
	●Check operation/brake pad wear/fluid leakage.

●Brake fluid needs to be above the lowest position.
●Correct if necessary. Replace pads/disk if worn to the limit.
	O
	O
	O
	O
	O

	Brake hoses
	●Check for cracks or other damage, and replace if necessary.
	Every 4 years

	Accelerator lever*
	●Check operation and free play.
	O
	O
	O
	O
	O

	Wheels*
	●Check balance/damage/ run out

●Repair if necessary.
	O
	
	O
	O
	O

	Wheel-hub bearings*
	●Check bearing assemblies for looseness or damage.

●Replace if damaged.
	O
	
	O
	O
	O

	V-belt
	●Check for wear, cracks or other damage, and replace if necessary.
	O
	
	O
	O
	O

	Front and rear Suspension*
	●Check operation and for leakage.

●Correct if necessary.
	
	
	O
	
	O

	Steering system*
	●Check operation and for looseness/Replace if damage.

●Check toe-in/Adjust if necessary.
	O
	O
	O
	O
	O

	Steering knuckle pivots and suspension arms*
	●Lubricate with lithium-soap-based grease.
	
	
	O
	O
	O

	Drive shaft universal joint*
	●Lubricate with lithium-soap-based grease.
	
	
	O
	O
	O

	Engine mount*
	●Check for cracks or damage.

●Correct bolt tightness.
	
	
	O
	O
	O

	Front and rear axle boots*
	●Check operation.

●Replace if damage.
	O
	
	
	
	O

	Stabilizer bushings*
	●Check for cracks or damage.
	
	
	O
	O
	O

	Fittings and fasteners*
	●Check all chassis fittings and fasteners.

●Correct if necessary.
	O
	O
	O
	O
	O

	Battery
	●End connection
	O
	
	O
	O
	O

	Light and steering indication light
	●Operation
	O
	O
	O
	O
	O


2.2 AIR CLEANER

In case of driving in dusty environment, air filter shall be cleaned regularly. It is of great possibility to accelerate wear to engine if there is not filtering element or worn filtering element is used. So, please keep air filter under good conditions all the time. If vehicle is used in dusty area, inspect more frequently than specified in MAINTENANCE SCHEDULE.

If the air cleaner is clogged with dust, intake resistance will be increased, with a resultant decrease in power output and an increase in fuel consumption. never remove or modify any component in the air filter housing. The engine management system is calibrated to operate specifically with these components. Otherwise, engine performance degradation or damage can occur. Check and clean the air filter element in the following manner:

Remove rear seat back, front seat and dash board cover.
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TYPICAL

1. Rear seat back

2. Front seat

3. Air filter service cover
Remove air filter service cover.

Remove air filter housing cover. 
Loosen the clamps and then carefully pull air filter out of the air filter housing.  
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TYPICAL

1. Air filter

2. Clamp

CAUTION: Always wear appropriate skin and eye protection. Chemicals can cause a skin rash and eye injury.

1. Spray the foam filter element inside and out with a good air filter cleaner and follow manufacturer's instructions.

2. Dry the foam element completely. 
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Properly reinstall removed parts in the reverse order of their removal. Pay attention to the seal gasket of air filter housing is not skew.

CAUTION: 1. If liquid /deposits are found, squeeze and dry the foam filter. Replace filter element if damaged.

2. Do not start engine if liquid or deposit is found. If there is oil in the air filter housing, check engine oil level. Oil level may be too high.

3. Inspect the air cleaner element for tears, a torn element must be replaced.

2.3 VALVE CLEARANCE

Excessive valve clearance results in valve noise and insufficient valve clearance results in valve damage and reduced power.

Check the intake and exhaust valve clearances at the distances indicated above and adjust the valve clearances to specification, if necessary.

Valve clearance is to be checked when the engine is cold. The intake and exhaust valve must be checked an adjusted when the piston is at TOP DEAD CENTER (TDC) on the compression stroke.

Remove seats, gear shift lever and air filter service cover.
Remove relevant accessories around an engine, with relevant contents referring to Chapter 5 Vehicle Dismantling.

Remove spark plug cable and spark plug.

Remove the bolts and valve cover.
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TYPICAL

1. 4xM6 bolt
2. Valve cover

Remove the M6 bolts, the big view hole cap and crankshaft position sensor.
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TYPICAL

1. 3xM6 bolt

2. Big view hole cap
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TYPICAL

1. M6 bolt

2. Crankshaft position sensor

Valve clearance of cylinder 

Turn the magneto bolt until mark “T” on magneto flywheel and dot mark on the left crankcase cover are aligned.
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1. Mark “T” on magneto flywheel

2. Dot mark on left crankcase cover

3. Location of crankshaft position sensor

At TDC ignition, the printed marks on the camshaft timing gear have to be parallel to cylinder head base as per following illustration.
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1. Printed marks on camshaft timing gear

2. Cylinder head base

3. Camshaft timing gear
Insert the feeler gauge between the valve stem end and adjusting screw on the rocker arm to check the clearance.

If the valve clearance is out of specification, adjust valves as follows.

	Valve clearance

	Intake
	0.08 to 0.10mm

	Exhaust
	0.08 to 0.10mm


Use mean valve of exhaust/intake to ensure a proper valve adjustment.

Hold the adjustment screw at the proper position and torque the locking nut.

Repeat the procedure for each valve.
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1. Adjustment screw

2. Adjustment nut

3. Feeler gauge

Valve clearance adjuster lock nut:7-8 Nm.
CAUTION: Securely tighten the locknut after completing adjustment.

Install the valve cover, spark plug cable and spark plug, the plug screw and gasket of left crankcase cover and the crankshaft position sensor.

2.4 SPARK PLUG

In case of serious wear or burn to electrode or burn to insulator by spark plug or damage to thread etc., please replace it with new spark plug

In case of carbon deposit, please use proper tools for cleaning. 

Spark plug gap

Use feeler gauge to measure clearance of spark plug. 

In case of exceeding designated range, then adjust the gap.
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Spark plug gap: 0.8-1.0 mm. 

Spark plug heat range

Check the spark plug heat range by observing the electrode color. If the electrode of the spark plug is appearing wet or dark color, replace the spark plug with a hotter type one. If it is white or appearing glazed, replace the spark plug with a colder type one.

Standard type: CR8EKB 

CAUTION: In order to avoiding damaging cylinder cap thread, firstly use hands to tighten spark plug and then use spark plug wrench to tighten cylinder cap with designated torque.
2.5 THROTTLE CABLE PLAY
Before starting the engine, check the throttle handle to ensure the correct operation, and ensure that the throttle handle can be completely restored to the idle position without the external force.

Check the free play and adjust, if needed, press the accelerator to ensure that the movement of the smooth and not sticky buckle back when the check throttle handle correctly. It must run smoothly, fully spring back to the free position.
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From the gate line (support), turn the regulator, regulate the solar term door handle free play.

After adjustment, tighten nut. 

If free play after adjustment cannot reach designated requirement or there is viscosity for throttle valve, replace it with new throttle cable.

2.6 ENGINE OIL

Engine Oil Level Inspection
NOTE: Check level frequently and refill if necessary. Do not overfill. Operating the engine/gearbox with an improper level may severely damage engine/gearbox. Wipe off any spillage.

NOTE: While checking the oil level, visually inspect engine area for leaks.
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LH SIDE OF ENGINE

1. Dipstick

With vehicle on a level surface and engine cold, not running, check the oil level as follows:

1. Move the shift lever to P (Parking) position and apply the brake lock lever.

2. Start and let the engine run at idle for 60s.

3. Stop engine.

4. Remove engine service cover.

Clean around dipstick to avoid foreign particles failing down the hole.

5. Unscrew dipstick then remove and wipe clean it. 

6. Reinstall dipstick, screw in it completely.

7. Remove dipstick and check oil level. It should be near or equal to the upper mark.
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1. MAX

2. MIN

3. Operating range

If the level is between marks, properly tighten dipstick. 

If the level is below the lower mark, add as follow:

- Place a funnel into the dipstick tube to avoid spillage.

- Add a small amount of recommended oil and recheck oil level.

- Repeat the above procedures until oil level reaches the dipstick's upper mark.

NOTICE: Do not overfill. 

Wipe off any spillage.

Oil Change and Oil Filter 

Prior to change the oil, ensure vehicle is on a level surface. Oil and oil filter must be replaced at the same time. Oil change and oil filter replacement should be done with a warm engine.
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WARNING

	The engine oil can be very hot. Wait until engine oil is warm.


CAUTION: Dispose oil and filter as per your local environmental regulations.

1. Ensure vehicle is on a level surface.

2. Start engine and let idle for a few minutes to warm oil.

3. Stop engine. Wait a few minutes to allow oil to flow down to crankcase then check oil level. 

4. Remove dipstick.

5. Raise the vehicle, support it securely. Place a drain pan under the engine drain plug area. 

6. Remove the left foot plate.

7. Clean the drain plug area.

8. Unscrew drain plug to drain out the oil.
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1. Oil drain plug

9. Remove the oil strainer cap, O-ring, oil strainer. Clean oil strainer and then reinstall the assembly with a NEW O-ring. 
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1. M6 Bolt

2. Oil Drain Plug

3. Washer

4. Oil Strainer Cap

5. O-ring

6. Oil Strainer

10. Confirm oil to drain completely from crankcase.

11. Clean the drain plug from metal shavings and residue.

12. Install a new washer on drain plug. Torque drain plug to 30~40 Nm.

13. Remove oil filter component. 
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1. M6 Bolt

2. Oil filter cap

3. O-ring

4. Oil filter

14. Check and clean the oil filter inlet and outlet area for dirt and other contaminations.

15. Apply a NEW O-ring with engine oil and slip onto oil filter cover.

16. Apply engine oil to the seal on open end of the oil filter.

17. Install the oil filter and tighten to the specified torque:9-12Nm.

NOTICE: Pay attention to avoid pinching the O-ring during filter and cover installation.

18. Refill engine with a SAE 10W-40 classification engine oil, Oil change capacity with 2500mL.

19. Check the oil level. Refer to OIL LEVEL VERIFICATION above.

20. Run engine to ensure oil filter and drain plug areas are not leaking.

CAUTION: In order to expand service life of vehicle, please use grade SL standard engine oil conforming to API with its viscosity indication being SAE10W-40. If viscosity of engine does not reach SAE10W-40, make corresponding selection according to drawing.
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2.7 FRONT DIFFERENTIAL OIL

To change the front differential oil, locate the vehicle on a level position and carry out the following steps.

Clean the oil level check plug area and remove the oil level check plug.
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Clean the drain plug area.

Place an oil pan under the front differential case, and then drain oil completely by removing the drain plug.

Tighten the drain plug to 20 Nm. 
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Pour the specified oil (GL-5 80W90) about 230mL by syringe through the oil level check plug hole until the oil over flows.

Tighten the oil level check plug to 20 Nm.

2.8 REAR DIFFERENTIAL OIL

To change the rear differential oil, locate the vehicle on a level position and carry out the following steps.

Clean the oil level check plug area and remove the oil level check plug.
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Clean the drain plug area.

Place an oil pan under the front differential case, and then drain oil completely by removing the drain plug.

Tighten the drain plug to 20 Nm. 

Pour the specified oil (GL-5 80W90) about 230mL by syringe through the oil level check plug hole until the oil over flows.

Tighten the oil level check plug to 20 Nm.
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2.9 STEERING SYSTEM

Keep handlebar in horizontal status on flat ground and check whether the handlebar is loose from four directions (top, bottom, left and right); tighten nut or dismantle steering column for further checking, if any. 

Park vehicle on flat ground and rotate handlebar leftwards and rightwards to check whether it is able to be rotated flexibly. If any stuck, check whether it is caused by installation of main wire ground or other wiring; if not, please check the bottom of steering bar to check whether steering column bearing is damaged.

Park vehicle on flat ground, make sure the tire pressure for right and left tires is same and set to the proper specification, set the front wheels in the straight position, then place a load of 75kg on the seat.
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Measurethe distance A and B of the front wheels and calculate the difference.  

TYPICAL

A: front of front wheel

B: rear of front wheel

Toe-in.: B-A= 5mm

Out of range of toe-in: →Adjust nut of tie rod
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CAUTION: After adjusting toe-in, fist rotate steering wheel from center position to the left and right, to ensure that is the same corner, then slowly run vehicle to see whether its direction can be controlled.

2.10 BRAKING SYSTEM

Check if any brake fluid is leaking out of the pipe joints or the brake fluid reservoir. Apply the brakes firmly for one minute. If there is any leakage, have the vehicle inspected by an authorized dealer.

Test the brakes at slow speed after starting out to make sure they are working properly.
If the brakes do not provide proper braking performance, inspect the brake system.

If needed, have the vehicle inspected by an authorized dealer.
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Brake fluid level

Check brake fluid level by observing upper pump of front brake and upper and lower limit line of rear brake fluid. 

When brake fluid level is lower than lower limit, supplement brake fluid DOT4 in time. 
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Brake pedal adjustment

The brake pedal stroke is 30～40mm. If less than equal 30mm, it will be a hidden dangers, must adjust the brake pin connecting the brake pedal. 
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2.11 GEAR SHIFT

Check the shift lever as to change shift from P to R/N/H/L and reverse smoothly. Also, the meter display is correct.

The shift lever should be vertical when the gear is in neutral. If not, adjust the shift cable and then tighten the nuts of the shift cable.
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2.12 COOLING SYSTEM

To prevent rust formation or freezing condition, always replenish the system with the premixed coolant or with 50% antifreeze and 50% water. Do not use tap water, straight antifreeze or straight water in the system. Tap water contains minerals and impurities which build up in the system. During cold weather, straight water causes the system to freeze while straight antifreeze thickens and does not have the same efficiency. Always use ethylene glycol antifreeze containing corrosion inhibitors specifically recommended for aluminum engines.

Cooling liquid may be reduced by natural evaporation. Regularly check horizontal position of cooling liquid. 

Coolant level verification

Park vehicle at flat ground and check horizontal line of cooling liquid.

Open the front storage box cover.

Remove the water tank cover in the front storage box. 
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Check the level of cooling water in fluid reservoir (auxiliary radiator) is between upper and lower critical levels.
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WARNING

	To avoid potential burns, do not remove the radiator cap or loosen the cooling drain plug if the engine is hot. Never drain or refill cooling system when engine is hot.


Coolant replacement

Park vehicle at flat ground and check horizontal line of cooling liquid.

Remove the front storage box cover and water tank cover. Remove auxiliary tank cover and radiator cover.
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TYPICAL

1. Auxiliary tank cover

2. Radiator cover 

T Partially unscrew coolant drain plug located below water pump housing.

When coolant is drained completely, remove cooling drain plug completely and install a new gasket ring.

Screw the coolant drain bolt and torque it to 10 Nm.
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Unscrew bleed screws on top of thermostat housing.
Fill up the radiator with coolant, when the coolant comes out by the thermostat housing hole, install the bleed screws with its gasket ring and torque to 10 Nm.

Refill coolant tank up to upper-level mark. Install the coolant tank cap and the radiator cap.
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TYPICAL

1. Auxiliary tank cap

2. Radiator cap

Run engine until radiator fan opens then stop engine.

When engine has completely cooled down, recheck coolant level in radiator and coolant tank. Top up if necessary.
2.13 WHEELS

Lift wheels up at horizontal position and ensure no load to each wheel. 

Shake wheels to left and right to see whether their connecting parts are installed tightly and check whether they can be swung. 

No adequate tightening: → tightening 

Swing: → replace rocker arm
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Tire pressure

Improper tire pressure will lower comfort of operation and driving and may lead to wear to side edges of tires. 
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	Front wheel
	Rear wheel

	Rated pressure
	45kPa(0.46kgf/cm2)
	45kPa(0.46kgf/cm2)

	Dimension of tire 
	25×8-12
	25×10~12


Tire thread.                              
When the tire groove decreases to 3 mm (0.12 in) due to wear, replace the tire.  
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2.14 ENGINE COMPRESSION PRESSURE

The compression pressure reading of a cylinder is a good indicator of its internal condition. The decision to overhaul the cylinder is often based on results of a compression test. 

Before measuring cylinder pressure, ensure installation and tightening of cylinder cap bolt with designated torque and reasonable clearance of valve.                                                      

Standard cylinder pressure: 0.9～1.2 Mpa
Too low cylinder pressure may cause the following: 

1. Excessive wear to cylinder;

2. Wear to piston or piston ring;

3. Blockage of piston ring in groove;

4. Close valve seat;

5. Damage to cylinder lining or faults of other parts

Measure engine compression pressure:

1. Warm up engine. 

2. Ensure full charging of battery.

3. Remove the relevant plastic parts and accessories from the outside of the engine

4. Dismantle spark plugs.

5. At spark plug hole, install cylinder pressure meter. 

6. Press button of start for several seconds. Record indication of maximum cylinder pressure.
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2.15 ENGINE OIL PRESSURE
Check the engine oil pressure periodically. This will give a good indication of the condition of the moving parts. The engine oil pressure test should be done with a warm engine 90℃ and the recommended oil.

Remove the relevant plastic parts and accessories from the outside of the engine.

Remove the oil pressure switch wire connector and switch on the right of engine. 

[image: image35.png]| —





Install oil pressure gauge and adapter hose.

Start engine on idle speed. The engine oil pressure should be within the following values.

	Oil pressure
	1600 RPM
	6000 RPM

	Minimal
	70 KPa
	350 KPa

	Nominal
	180 KPa
	420 KPa

	Maximal
	300 KPa
	550 KPa


Remove oil pressure gauge and adapter hose.

Installation oil pressure switch to 12Nm and the oil pressure switch wire connector.
2.16 SUSPENSION SYSTEM

Lubricate both suspension arms with lithium-soap based grease. There are two grease fittings on each suspension arm. Check operation and for leakage. 

Grease fitting location of front suspension arms.
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Use grease gun to grease the suspension pivot nozzles located on the rear steering knuckle, rear A-Arm and sway bar until grease appears at the bushing.
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NOTE: Injection nozzles are symmetrical left and right.
3. ENGINE
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WARNING

	Torque wrench tightening specifications must strictly be adhered to.

Locking devices (e.g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pin, etc.) must be installed or replaced with new ones where specified. If the efficiency of a locking device is impaired, it must be repaired.


When diagnosing an engine problem, always perform a cylinder leak test. This will help pin-point a problem. Refer to the instructions included with your leak tester and to LEAK TEST section for procedures.

Always place the vehicle on level surface.

NOTE: For a better understanding, the many illustrations are taken with engine out of vehicle. To perform the following instructions, it is not necessary to remove engine from vehicle.

Always disconnect BLACK (-) cable from the battery, then RED (+) cable before working on the engine.

Even if the removal of many parts is not necessary to reach another part, it is recommended to remove these parts in order to check them.

When disassembling parts that are duplicated in the engine, (e.g.: valves), it is a strongly recommended to note their position (PTO/MAG side) and keep them as a “group”. If you find a defective component, it would be must easier to find the cause of the failure among it group of parts (e.g.: you found a worn valve guide. A bent spring could be the cause and it will be easy to know which one among the springs is the cause to replace it if you grouped them at disassembly). Also, since used pars have matched together during the engine operation, they will keep their matched fit when you reassemble them together within their “group”.

3.1 ENGINE REMOVAL 
To avoid potential burns, let engine and exhaust system cool down before performing any servicing.

Place vehicle on a work station that will have access to an engine-lifting hoist. Then start with initial preparation of vehicle.

Remove operator’s seat. Disconnect the BLACK (-) cable from battery, then the RED (+) cable.

Drain coolant from engine cooling system. Drain engine oil only if engine overhaul is necessary. To work on gearbox the removal is necessary but do not drain engine oil.
Before remove engine, drain engine oil and coolant.
- Remove CVT air inlet and exhaust pipe.
- Remove shift arm.
- Remove throttle body, water pump inlet hose, coolant outlet hose, oil inlet hose, air inlet hose, cylinder head breather hose, spark plug, crankcase exhaust gas hose. Disconnect crankshaft position sensor, the speed sensor on the gearbox and the gear position switch, starter motor harness, disconnect the oil pressure sensor plug, engine ground harness and disconnect the engine wiring harness from the main harness.
- Disconnect front and rear driveshaft from engine.
- Remove engine mounting bolts on bottom hang brackets and engine rear mounting board.
3.2 VALVE COVER

Removal

-Remove the four M6 bolts of valve cover.
[image: image39.png]



1. 4xM6 Bolt
2. Valve cover

- Remove valve cover and gasket.
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1. Valve cover

2. Gasket
Inspection

Check the gasket on the valve cover if it is brittle, cracked or hard. If so, replace the gasket.

Installation

For installation, reverse the removal procedure.

Torque the bolts for valve cover in a crisscross sequence.

Bolt tightening torque for valve cover: 10~12 Nm.

3.3 TIMING CHAIN TENSIONER

NOTE: Before removal and installation, make sure that the cylinder is set to TDC ignition. Refer to CAMSHAFT.

Tensioner removal
	[image: image41.png]


WARNING

	Never perform this operation immediately after the engine has been turn because the exhaust system can be very hot. Wait until exhaust system is warm or cold.


Remove:

- Lock bolt
- Washer
- Bolt
- Chain tensioner 
- Gasket

[image: image42.png]



1. M6 Lock bolt
2. Washer
3. 2xM6 Bolt
4. Chain tensioner 
5. Gasket

Tensioner Inspection

Check the chain tensioner for cracks or other damages. Replace if necessary.

Check push rod of chain tensioner for free movement by sheet.

Check if washer is brittle, cracked or hard. Replace if necessary.

Check gasket. Replace if broken or worn.

Tensioner Installation

NOTE: Before installing the chain tensioner make sure that the camshaft timing gear can be moved back and forth.
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1. Locking bolt

2. Chain tensioner

3. Bolt

Turn push rod of chain tensioner clockwise to shortest position by sheet.
Install the chain tensioner with gasket to the cylinder block. Tighten the bolt for chain tensioner to 10~12 Nm.

Push out the rod of chain tensioner counterclockwise by sheet, then tighten the lock bolt to 6~8 Nm.

NOTE: Do not forget to place the washer on lock bolt and gasket on the chain tensioner.

3.4 CAMSHAFT TIMING GEAR

Gear Removal

Turn crankshaft to TDC ignition of the cylinder.

Unscrew timing chain tensioner.

Remove the bolt and pressure release valve.
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1. M8 Bolt
2. Pressure release valve
3. 2xM6 Bolt

4. Camshaft timing gear

Remove bolts and camshaft timing gear.

NOTE: Secure timing chain with a retaining wire.

Gear Inspection

Check camshaft timing gear for wear or deterioration. If gear is worn or damaged, replace it as a set (camshaft timing gear and timing chain).

Check pressure release valve for crack or damage. If damaged, replace it.

Gear Installation

For installation, reverse the removal procedure. Pay attention to the following details.

Clean mating surface and threads of camshaft, prior to assemble camshaft timing gear.
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1. Mating surface on camshaft

2.Threads for camshaft screw 

Camshaft timing gear and crankshaft must be at TDC ignition position before installing the timing chain.

CAUTION: Crankshaft and camshaft must be locked on TDC ignition position to place camshaft timing gear and timing chain in the proper position.

Install camshaft timing gear so that the timing gear tabs are located into the flat area of the camshaft.

The printed marks on the camshaft timing gear must be parallel to the cylinder head base. See the following illustration for a proper positioning.
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1. Printed marks on camshaft timing gear

2. Cylinder head base

3. Camshaft timing gear

Tighten the two M6 bolts for camshaft timing gear to 10~12 Nm.

Install pressure release valve and bolt through camshaft timing gear to cylinder.
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1. Pressure release valve 
2. M8 bolt
Apply Loctite 222 on the front 2 teeth of M8 bolt.

Tighten the M8 bolt for pressure release valve to 18~22 Nm.
NOTE: Before installing the bolt adjust the chain tension and check again if marks on the timing gear are parallel to cylinder head base.

3.5 ROCKER ARM

Rocker Arm Removal

Remove:

- Valve cover

- Chain tensioner

- Camshaft timing gear

- Bolt and camshaft retaining plate
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1. Cylinder head

2. Camshaft retaining plate

3. M6 Bolt
- Rocker arm shafts

- Rocker arm assembly (exhaust side and intake side) with adjustment screws and nuts.
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1. Rocker arm shaft

2. Rocker arm (exhaust side)

3. Rocker arm (intake side)

4. Washer

5. Adjustment screw

6. Locking nut

- Washers
CAUTION: Pay attention not to lose washers or drop them into the timing chain compartment.

Rocker Arm Inspection

Inspect each rocker arm for cracks and scored friction surfaces. If so, replace rocker arm assembly.

Check the rocker arm rollers for free movement, wear and excessive radial play. Replace rocker arm assembly if necessary.
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1. Rocker arm (exhaust side)

2. Roller

A- Rocker arm bore diameter

Measure rocker arm bore and shaft diameter. If radial play is out of specification, change the rocker arm assembly.
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	Radial play of rocker arm bore and shaft 

	new
	0.013 to 0.046 mm

	Service limit
	0.046 mm


Measure axial play of rocker arm and cylinder head axial play using a feeler. If axial play is out of specification, change the rocker arm assembly.
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1. Rocker arm 

2. Cylinder head

3. Axial play

	Axial play of rocker arm and cylinder head

	new
	0.04 to 0.46 mm

	Service limit
	0.50 mm


Check adjustment screws for free movement, cracks and/or excessive play.
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1. Free movement of adjustment screw top

Check rock arm shaft for wear or damage, if so, replace parts.

Check washer for wear or damage, if so, replace parts.

Rocker Arm Installation

NOTE: Use the same procedure for exhaust and intake rocker arm.

Apply engine oil on rocker arm shaft.

Install the rocker arm shafts with the cone edge facing inside and use following procedure:

- Insert a rocker arm pin through rocker arm pin bore.

- Install a washer then the proper rocker arm.

- Push in rocker arm shaft until its chamfer reaches the end of rocker arm bore.
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1. Rocker arm shaft 

2. Washer (timing chain side)

3. Washer (spark plug side)

- Place the other washer and push rocker arm shaft to end position.

- Install the camshaft retaining plate.

Tighten the M6 bolt for camshaft retaining plate to 10~12Nm.
3.6 CYLINDER HEAD

Cylinder Head Removal

Drain coolant.

CAUTION: Before removing cylinder head, blow out remaining coolant by air pressure. During cylinder head removal, the remaining coolant in cylinder head could overflow into the engine and a little quantity of coolant could drop into the engine. In this case, the engine oil will be contaminated.
Disconnect: 


- Spark plug wire


- Temperature sensor connector, located at cylinder head

Remove:

    - spark plug


- exhaust pipe spring


- exhaust pipe nuts


- radiator intake hose


- air filter box and throttle body


- chain tensioner


- valve cover and gasket


- camshaft timing gear


- cylinder head bolts M6

 
- cylinder head bolts M10 retaining cylinder head and cylinder to cylinder base.
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1. 4xM10 cylinder head bolt
2. 2xM6 cylinder head bolt
Pull up cylinder head.

Remove:


- chain guide


- cylinder head gasket and scrap it.
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1. Cylinder head

2. Timing chain 

3. Chain guide

4. Cylinder head gasket

Cylinder Head Inspection

Inspect timing chain guide for wear, cracks or other damages. Replace if necessary.

Check for cracks between valve seats and spark plug hole, if so, replace cylinder head.

Check the carbon deposit for spark plug. If so, replace spark plug.

Use clearance gauge to measure clearance of spark plug. 

In case of exceeding designated range, then adjust the gap.
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Spark plug gap: 0.8-1.0 mm 

Check mating surface between cylinder and cylinder head for contamination. If so, clean both surfaces.
Clean oil support through the cylinder head from contamination.
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1. Oil port to lubricate camshaft lobes intake/exhaust

2. Oil supply to camshaft bearing journal timing chain side

3. Oil supply to camshaft bearing journal spark plug side

Check cylinder head for deformation. Measure the flatness of cylinder head using knife straight edge and feeler. If flatness is out of specification, change cylinder head.
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	Flatness of cylinder head

	New
	0 to 0.04 mm

	Service limit 
	0.04 mm


Cylinder Head Installation

NOTE: The cylinder heads are not identical in design. Do not invert the cylinder heads at assembly.

For installation, reverse the removal procedure. Pay attention to the following details.

Ensure dowel pins are in place.
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1. Dowel pin

CAUTION: Chain guide has to be fixed between cylinder and cylinder head.
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1. Chain guide (fixed between cylinder and cylinder head)

2. Chain tensioner guide (mounted in crankcase)

Install a new cylinder head gasket.

NOTE: Do not forget to place the washer on cylinder head M10 bolt. First, torque cylinder head M10 bolts in crisscross sequence to 18~22 Nm, then finish by tightening to 45~50 Nm.

Install cylinder head M6 bolts. Tighten M6 bolts to 10~12 Nm.
Check chain guide for movement.
Tighten spark plug to 20~25 Nm.

3.7 CAMSHAFT
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1. Camshaft of cylinder 

Camshaft Timing Cylinder 

Turn crankshaft until piston is at TDC ignition as follows.

Remove:

  - spark plug cable and spark plug

  - valve cover

  - crankshaft position sensor 

- bolt and big view hole cap
Turn the magneto bolt until mark “T” on magneto flywheel and dot mark on the left cover are aligned.
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1. Mark “T” on magneto flywheel

2. Dot mark on left crankcase cover
3. Location of crankshaft position sensor

NOTE: At TDC ignition, the printed marks on the camshaft timing gear have to be parallel to cylinder head base as per following illustration.
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1. Printed marks on camshaft timing gear

2. Cylinder head base

3. Camshaft timing gear
CAUTION: Crankshaft cannot be locked at cylinder TDC ignition.

Camshaft Removal

Remove:

· spark plug cable and spark plug

   - valve cover (see VALVE COVER above)


- chain tensioner (see CHAIN TENSIONER above)

 
- camshaft timing gear (see CAMSHAFT TIMING GER above)


- camshaft retaining plate
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1. Cylinder head

2. Camshaft retaining plat

3. Bolt

   -rocker arms (see ROCKER ARM above)


   -camshaft.

NOTE: For removal rotate camshaft so that intake/exhaust lobe shows to upper side of cylinder head.
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1. Area for camshaft lobes

2. Camshaft

3. Camshaft retaining

Camshaft Inspection

Check each lobe and bearing journal of camshaft for scoring, scuffing, cracks or other signs of wear.

Measure camshaft base circular runout using the indicator. If runout is out of specification, change camshaft.
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A. Camshaft lobe (exhaust valves)

B. Camshaft lobe (intake valves)

C. Camshaft journal timing chain side

D. Camshaft journal spark plug side
	Camshaft base circular runout

	New 
	0 to 0.02 mm

	Service limit
	0.02 mm


Camshaft Installation

For installation, reverse the removal procedure. Pay attention to the following details.

CAUTION: the camshafts are not identical in design. Do not invert the camshafts during assembly. Any mix-up of the components will lead to engine damage.

Apply engine oil on the camshaft.

Place the camshaft retaining plate in the slot of the camshaft.
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1. Camshaft retaining plate position

2. Slot retaining camshaft 

3. Direction of movement

For other parts, refer to proper installation procedure.

3.8 VALVE SPRING

Valve Spring Removal

Remove:


- rocker arms (see ROCKER ARM above)


- cylinder head (see CYLINDER HEAD above).
Compress valve spring using valve spring compressor clamp and valve spring compressor cup.
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WARNING

	Always wear safety glasses when disassembling valve springs. Be careful when unlocking valves. Components could fly away because of the strong spring preload.


Remove valve cotters.
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1.
Valve spring compressor clamp

2.
Valve spring compressor cup

3.
Valve cotter
Withdraw valve spring compressor, then remove valve spring retainer and valve spring.

Valve Spring Inspection

Check valve spring for visible damages. If so, replace valve spring.

Check force of valve spring for different lengths using tension meter. Replace valves springs if out of specifications.
ATV525 Model
	Force of valve spring at length-22.7 mm

	New 
	530 ± 5% N

	Service limit
	503 N

	Force of valve spring at length-32.5 mm

	New 
	192.7 ± 8% N

	Service limit
	183 N


ATV625 Model
	Force of valve spring at length-25 mm

	New 
	550.4 ± 27 N

	Service limit
	523 N

	Force of valve spring at length-35 mm

	New 
	183.5 ± 14 N

	Service limit
	169 N


Valve Spring Installation

For installation, reverse the removal procedure. Pay attention to the following details.

Colored area of the valve spring must be placed on top.

To ease installation of cotters, apply oil or grease on them so that they remain in place while releasing the spring.

NOTE: Valve cotter must be properly engaged in valve stem grooves.
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1. Position of the spring

2. Valve cotter

After spring is installed, ensure it is properly locked by tapping on valve stem end with a soft hammer so that valve opens and closes a few times.

CAUTION: An improperly locked valve spring will cause engine damage.
3.9 VALVE

VALVE Removal

Remove valve spring, see VALVE SPRING above.

Push valve stem, then pull valves (intake and exhaust) out of valve guide.
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1. Intake valves 

2. Exhaust valve

Remove valve stem seal with Snap-On pliers and discard it. 

Valve Inspection

Valve Stem seal

Always install new seals whenever valves are removed.
Valve

Inspect valve surface, check for abnormal stem wear and bending. 
Valve Stem and Valve Guide Clearance

Measure valve stem and valve guide in three places using a micrometer and a small bore gauge.

Change valve if valve stem is out of specification or has other damages such as wear or friction surface.
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A-Valve stem diameter
ATV525 Model

	Valve stem diameter

	Exhaust valve

	New 
	Φ4.950 to Φ4.965 mm

	Service limit
	Φ4.950 mm

	Intake valve

	New
	Φ4.965 to Φ4.980 mm

	Service limit
	Φ4.965 mm


ATV625 Model

	Valve stem diameter

	Exhaust valve

	New 
	Φ5.45 to Φ5.465 mm

	Service limit
	Φ5.45 mm

	Intake valve

	New
	Φ5.465 to Φ5.48 mm

	Service limit
	Φ5.465 mm


Replace valve guide out of cylinder head if valve guide inner diameter is out of specification or has other damages such as wear or friction surface (see VALVE GUIDE below).
ATV525 Model

	Valve guide inner diameter
(intake and exhaust valves)

	New
	Φ5.00 to Φ5.012 mm

	Service limit
	Φ5.012 mm


ATV625 Model

	Valve guide inner diameter
(intake and exhaust valves)

	New
	Φ5.50 to Φ5.512 mm

	Service limit
	Φ5.512 mm


NOTE: Clean valve guide to remove carbon deposits before measuring valve guide inner diameter.

Valve sealing tape and Seat
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1. Valve seat

2. Exhaust valve 

3. Valve sealing tape (contact surface to valve seat)

Check valve face and seat for burning or pitting, and replace valve or cylinder head if there are signs of damage.

Ensure to seat valve properly. 

Measure valve sealing tape width using a caliper.
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	Valve sealing tape width
(intake and exhaust valves)

	New
	0.85 to 1.15mm

	Service limit
	0.85 mm


NOTE: The location of contact area should be in center of valve seat.

If valve seat contact width is too wide or has dark spots, replace the cylinder head.
Valve installation

For installation, reverse the removal procedure. Pay attention to the following details.

Install a NEW seal valve stem. Make sure valve stem is installed before installing seal.

Apply engine oil on valve stem and install it.

To ease installation of cotters, apply oil or grease on them so that they remain in place while releasing the spring.

After spring is installed, ensure it is properly locked by tapping on valve stem end with a soft hammer so that valve opens and closes a few times.

CAUTION: An improperly locked valve spring will cause engine damage.

3.10 CYLINDER 

Cylinder removal

Remove:

- Chain tensioner (see CHAIN TENSIONER)

- Camshaft timing gear (see CAMSHAFT TIMING GEAR)
- Cylinder head (see CYLINDER HEAD)

- Dowel Pins, gasket and chain guide

Pull out cylinder.

Discard cylinder gaskets.
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1. Cylinder

2. Dowel pin
3. Cylinder gasket

4. Chain guide
Cylinder Inspection

Check cylinder for cracks, scoring and wear, ridge on the top and bottom of the cylinder. If so, replace cylinder.

Measure cylinder bore and if it is out of specifications, replace cylinder and piston rings.
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Measure cylinder bore at 3 recommended positions. 
See the following illustration.

[image: image432.png]RD

RD2

RD1

+

J





1. First measuring of diameter

2. Second measuring of diameter

3. Third measuring of diameter

A. 7mm from cylinder bottom

B. 68mm 
C. 32mm

Distance between measurements should not exceed the service limit mentioned above.

Measure cylinder diameter in piston axis direction from top of cylinder. Take another measurement 90° from first one and compare.
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A. Perpendicular to crankshaft axis

B. Parallel to crankshaft axis
	Cylinder diameter measurement

	Size “A”

	New 
	91 to 91.01 mm

	Service limit
	91.01 mm 

	Size “B”

	New 
	91.01 to 91.02 mm

	Service limit
	91.02 mm


Cylinder Installation

For installation, reverse the removal procedure. Pay attention to the following details.

CAUTION: Always replace cylinder base gasket before installing the cylinder.

Turn magneto bolt. Crank the engine further and position piston at TDC. Then mount cylinder.

Apply engine oil on cylinder bore and also on the band of the piston ring compressor tool.
NOTE: Put timing chain through the chain pit then put the cylinder in place.

NOTE: At installation, do not damage the piston rings.

CAUTION: Chain guide has to be fixed between cylinder and cylinder head.

NOTE: After cylinder is installed, turn crankshaft until piston of cylinder is at TDC ignition and lock crankshaft. Install cylinder head and the other parts in accordance with the proper installation procedures.

3.11 PISTON 

Piston Removal

Remove:


- cylinder head (see CYLINDER HEAD above) 


- cylinder (see CYLINDER above).
Place a rag under piston and in the area of timing chain compartment.

Remove one piston circlip with a needle-nose pliers and discard it.
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NOTE: The removal of both piston circlips is not necessary to remove piston pin.

Push piston pin out of piston.
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1. Piston

2. Piston Pin

Detach piston from connecting rod.

Piston and Pin Inspection

Inspect piston for scoring, cracking or other damages. Replace piston and piston rings if necessary.

Using a micrometer, measure piston at 8 mm perpendicularly (90°) to piston pin.
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	Piston diameter measurement

	Size “I”

	New 
	90.94 to 90.95 mm

	Service limit
	90.94 mm 

	Size “II”

	New 
	90.95 to 90.96 mm

	Service limit
	90.95 mm


The measured dimension should be as described in the following tables. If not, replace piston.

Piston Pin and Piston Pin Bore
Measure the piston pin bore diameter.
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	Piston pin bore diameter

	New
	22.004 to 22.010 mm

	Service limit
	22.010 mm


Using synthetic abrasive woven clean piston pin from deposits.

Inspect piston pin for scoring, cracking or other damages.

Measure piston pin diameter using a micrometer.

Replace piston pin if diameter is out of specifications.

See the following illustration for the proper measurement positions.
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A-Piston pin diameter

	Piston pin diameter

	New
	21.994 to 22.00 mm

	Service limit
	21.994 mm


If piston pin bore and piston pin exceed specified tolerance; replace piston by a new piston or piston pin.
Connecting Rod

Measure inner diameter of connecting rod small end bushing.
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1. Bore gauge

2. Connecting rod
	Connecting rod small end diameter

	New
	22.01 to 22.02 mm

	Service limit
	20.02 mm


Replace connecting rod if diameter of connecting rod small end is out of specifications.

Piston Installation

For installation, reverse the removal procedure. Pay attention to the following details.

Apply engine oil on the piston outer circle.

Insert piston pin into piston and connecting rod.
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1. Piston of cylinder 

2. Mark “IN” on piston 

CAUTION: Mark “IN” on top of piston must show to intake side. Place gap of piston circlip parallel with piston motion.
CAUTION: Always replace disassembled piston circlip(s) by new ones. Place a rag on cylinder base to avoid dropping the circlip inside the engine.
3.12 PISTON RINGS

Ring Removal

Remove:


- cylinder head


- cylinder


- piston pin

- piston rings

Ring Inspection

Inspect ring grooves on piston for scoring, cracking or other damages. Replace piston and piston rings if necessary.

Ring end Gap
Using a feeler gauge measure each ring/piston groove clearance. If the clearance is too large, the piston and the piston rings should be replaced.

To measure the ring end gap, place the ring in the cylinder in the area of 8 to 16 mm from top of cylinder.

NOTE: In order to correctly place the ring in the cylinder, use piston as a pusher.

Using a feeler gauge, check ring end gap. Replace ring if gap exceeds the above tolerance.
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	Ring end gap

	Upper compression ring

	New
	0.20 to 0.40 mm

	Service limit
	0.40 mm

	Lower compression ring

	New
	0.40 to 0.55 mm

	Service limit
	0.55 mm

	Oil scraper ring

	New
	0.20 to 0.70 mm

	Service limit
	0.7 mm


Compression Ring Thickness
Measure compression ring thickness using a caliper. Replace ring if exceeds the above thickness.

	Compression ring thickness

	Upper compression ring

	New
	1.17 to 1.19 mm

	Service limit
	1.17 mm

	Lower compression ring

	New
	1.47 to 1.49 mm

	Service limit
	1.47 mm


Ring Installation

For installation, reverse the removal procedure. Pay attention to the following details.

Clean the ring groove on the piston before ring installation.

NOTE: Install the oil scraper ring first, then the lower compression ring with the word “A” facing up, then the upper compression ring with the word “ATG-V” facing up.
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1. Upper compression ring

2. Lower compression ring

3. Oil scraper ring
CAUTION: Ensure that top and second rings are not interchanged.

The gap of upper compression ring is faced to the intake side. The gap of lower compression ring is faced up to the exhaust side.

NOTE: Use a ring expander to prevent breakage during installation. The oil ring must be installed by hand.

Check that rings rotate smoothly after installation. Space the piston ring end gaps 120 apart and do not align the gaps with the piston pin bore.
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1. DO NOT align gap with piston thrust side axis

2. DO NOT align ring with piston pin bore axis

A.--120°. 

3.13 TIMING CHAIN
Removal of Timing Chain

Remove:

 
- valve cover, chain tensioner and camshaft timing gear (refer to CYLINDER AND HEAD section)


- CVT (refer to TRANSIMISSION)


- Bolt, timing chain guide and tension plate.
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1. Tension plate

2. Bolt

3. Timing chain

Carefully pull the timing chain sideward and down from the crankcase.

NOTE: Mark the operating direction of the timing chain before removal.

Timing Chain Inspection

[image: image438.emf]
NOTE: Check timing chain on camshaft timing gear for excessive radial play.

Check chain condition for wear and teeth condition.

If chain is excessively worn or damaged, replace it as a set (camshaft timing gear and timing chain).

Timing Chain Installation

The installation is essential the reverse of the removal procedure, but pay attention to the following details.

NOTE: Ensure to perform proper valve timing. Lock crankshaft (see CRANKSHAFT) and camshaft at TDC ignition (refer to CYLINDER AND HEAD section).

Install timing chain with camshaft timing gear then, adjust chain tension (refer to CYLINDER AND HEAD section).

CAUTION: Improper valve timing will damage engine components.

3.14 CRANKCASE

Crankcase Dismantling
Remove:


-Front/rear drive shaft (refer to VEHICLE DISMANTING)

-CVT (refer to TRANSIMISSION) and gaskets
  -Starting motor
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1. 2xM6 bolt.
2. Starting motor
- M6 bolts and gearshift switch.
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1. 2xM6 Bolt

2. Gearshift switch

- left crankcase cover (refer to LEFT CRANKCASE COVER)

- gear shift arm

- magneto motor and sprag clutch 
- oil pump


- water pump cover (refer to COOLING SYSTEM section)


- oil filter 
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1. 3xM6 Bolt

2. Oil filter cap

3. O-ring

4. Oil filter


-cylinder head, cylinder and piston (refer to CYLINDER AND CYLINDER HEAD section)


-timing chains and timing chain guides (refer to TIMING CHAIN and TIMING CHAIN GUIDE).

Remove bolts on the right crankcase block. 
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1. 7x M6*60 bolt
2. 2x M8*50 bolt
3. Right crankcase block

Remove bolts on the left crankcase block. 
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1. 8xM6*50bolt

2. 2xM8*50 bolt

3. Left crankcase block

Separate the left/right crankcase block.
Inspection

Check bearing and crankshaft bearing on right crankcase block for wear or damage. Replace if necessary.
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1. Crankshaft bearing 

2. Bearing

3. Right crankcase block.

Installation

The installation is essential the reverse of the removal procedure, but pay attention to the following details.
Apply sealant continuous regular on contact face of left crankcase block.

Do not forget to put dowel pins and O-ring to left crankcase block. Then fit the right crankcase block to left.
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1. 3xDowel pin

2. O-ring

Tighten M6 bolts in crisscross sequence to 10~12 Nm.

Tighten M8 bolts to 18~22 Nm.

CAUTION: Apply oil on the gearshift switch hole before installing. The harness of switch is upward. 

Tighten M6 bolts for gearshift switch to 10~12 Nm.

3.15 GEAR
Removal

Remove right crankcase block (refer to CRANKCASE).

Remove balance shaft, crankshaft and main shaft from the left crankcase block.
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1. Crankshaft

2. Balance shaft

3. Main shaft

4. 4xM8 bolt

5. Active cone

Remove four M8 bolts and active cone.

Remove bolts, washer, spring and steel ball for the shift drum from left crankcase block. 
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1. M14 Bolt

2. Washer

3. Spring

4. Steel ball

Remove shift drum, countershaft, fork and parking brake plate.
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1. Parking brake plate

2. Main shaft

3. Countershaft

4. Fork

5. Shift drum

Inspection

Check crankshaft, balance shaft, main shaft, countershaft, shift drum, bearing and crankshaft bearing for wear or damage. Replace if necessary.

Installation
Install the parking brake plate to the fork shaft.
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1. Parking brake plate

2. Fork

Install main/counter shaft, fork, shift drum to the left crankcase block.
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1. Main shaft

2. Countershaft

3. Shift drum

4. Fork
Install bolts, washer, spring and steel ball to the left crankcase block. Tighten the M14 bolt for shift drum to 28~32 Nm.

NOTE: Install countershaft, fork and shift drum at the same time. Apply thread-locker on the M14 bolt for shift drum before installation. Check shifting smooth or not. Check the steel ball slide smooth or not in the bolt hole.

Install crankshaft and balance shaft to left crankcase block with the marks in a line.
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CAUTION: Apply engine oil on the crankshaft bearing and crankshaft journal. After installation, turn the crankshaft to check the groove on crankshaft and mark on balance shaft in a line or not at TDC position.
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1. Crankcase shaft

2. Balance shaft

3. Groove 

Install M8 bolts and active cone. Tighten bolts for active cone to 18~22 Nm.

1.16 CRANKSHAFT 

Removal

Refer to GEAR.

Inspection

Check each bearing journal of crankshaft for scoring, scuffing, cracks or other signs of wear.

Check woodruff keyway and spline on the crankshaft for wear or damages. 

Replace crankshaft if the gears are worn or otherwise damaged.
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1. Gear

2. Woodruff keyway

3. Spline

Installation

For installation of crankshaft in crankcase reverse the removal procedure. 

1.17 REAR ENWHEEL SHAFT

Removal

Remove right crankcase block. (Refer to CRANKCASE)
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Remove M10 bolt, washer, O-ring, connecting flange at front and rear side of right crankcase block.

Remove the bearing, oil seal, lock nut and rear wheel shaft from the right crankcase block.

Remove M8 blots on the end cover and then remove end cover.

Remove the bearing, oil seal, lock nut and output driven cone from right crankcase block.
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1. 2xM10 bolt

2. Washer

3. O-ring

4. Connecting flange

5. Bearing

6. Oil seal

7. M55 lock nut

8. Right crankcase block

9. Rear wheel shaft

10. Output driven cone

11. Bearing

12. O-ring

13. M65 lock nut

14. Bearing

15. Oil seal

16. End cover

17. 3xM8 bolt

Inspection

Check washer, O-ring, bearing and oil seal for wear or damages. Replace if damaged.
Check driven cone, splines on wheel shaft/connecting flange for wear or damages. Replace if damaged.
Installation

For installation of crankshaft in crankcase reverse the removal procedure. 

3.18 OIL PRESSURE RELIEF
The oil pressure relief is located the left side of engine.
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1. Engine pressure relief
NOTE: The oil pressure relief system works when the oil pressure exceeds 450 kPa (65 psi).

Removal

Remove relief valve cover and pull oil out.
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1. Pressure relief valve cover
2. Spring

3. Steel ball
4. O-ring
Inspection

Inspect spring and O-ring for scoring or other damages.

Check spring for free length.

NOTE: Replace worn or damaged components.

Clean pressure relief valve cover from metal shavings and other contaminations.

Installation

For installation, reverse the removal procedure.

Pay attention to the following details.

NOTE: At installation, always replace the O-ring of the plug screw.

3.19 OIL DRAIN

Prior to change the engine oil, ensure vehicle is on a level surface.

Place a drain pan under the drain plug area.

Clean drain plug area and remove magnetic drain plug with its washer to drain oil.

Remove oil filler including its O-ring.

CAUTION: Pay attention not to lose washer on oil drain plug.

Wait a while to allow oil flow out of gearbox.

[image: image92.png]



1.Bolt

2. Oil drain Plug

3. Washer

4. Oil filter Cap 

5.O-ring

6.Oil filter

Dispose oil as per your local environmental regulations.

Inspection

Oil condition gives information about the teeth condition inside the gearbox.

Clean the magnetic drain plug from metal shavings and dirt. Presence of debris gives an indication of failure inside the gearbox. Check gearbox to correct problem.

Change washer on the magnetic drain plug if damaged.

Replace O-ring if brittle, hard or otherwise damaged.

3.20 CRANKSHAFT POSTION SENSOR

NOTE: The gearbox removal is not necessary to reach the crankshaft position sensor.

Removal

To reach the crankshaft position sensor, remove the engine service cover.

Remove bolt for retaining crankshaft position sensor.
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1. M6 Bolt

2. Crankshaft position sensor

Remove crankshaft position sensor with O-ring.

Installation

For installation, reverse the removal procedure.

Pay attention not to lose O-ring on crankshaft position sensor. Apply oil on the O-ring before installation.
Tighten M6 bolt on crankshaft position sensor to 10~12 Nm.

3.21 LEFT CRANKCASE COVER 

Left Crankcase Cover Removal

Drain engine oil.

Remove breather pipe and big view hole cap and M6 bolt.
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1. 3xM6 Bolt

2. Big view hole cap

Disconnect crankshaft position sensor (CPS) connector and water intake pipe. 

Remove left crankcase cover and bolts.
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1. 2xM6*75 Bolt
2. 16xM6*40 Bolt
3. Left crankcase cover
Pull out left crankcase cover.

Left Crankcase Cover Inspection and Cleaning

Check the oil seal of big view hole cap for cracks or damage. Replace if necessary.
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1. Oil seal

2. Big view hole cap face contacted with left crankcase cover
Check left crankcase cover for cracks or damage. Replace if necessary.

Left Crankcase Cover Installation

For installation, reverse the removal procedure. However, pay attention to the following.

NOTE: At installation replace gasket for left crankcase cover.

Align the left crankcase cover to the dowel pin on the left crankcase block.
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1. Dowel pin

2. Gasket

Tighten M6 bolts on left crankcase cover in a crisscross sequence to 10~12 Nm.
Apply lubricant on the oil seal of big view hole cap. Apply silica gel on the cap face contacted with left crankcase cover.
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1. Big view hole cap 

2. Face contacted with left crankcase cover
Install big view hole cap with air vent upward.

Tighten M6 bolts for big view hole cap to 10~12 Nm.
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1. Air vent

2. 3xM6 Bolt

3.22 GEAR SHIFT ARM

Removal

Remove:

   - Engine service cover and shift lever arm

   - M6 bolts, dowel pin, gear shift mounting cover and gasket.
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1. 3xM6*25 Bolt

2. M6*32 Bolt

3. Dowel pin

4. Gasket

5. Gear shift mounting cover

6. Oil seal

Remove M6 bolt, plate and gear shift arm.
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1. M6*35 Bolt

2. Plate

3. Spring

4. Spline

5. Gear shift arm

Inspection

Check the oil seal for wear or damage. If damaged replace it.

Check spring and spline on the gear shift arm for wear or damage. If damaged replace gear shift arm.

Installation

For installation, reverse the removal procedure. However, pay attention to the following.

Install the bolt through the plate to the left crankcase. Tighten M6 bolt to 10~12 Nm.

CAUTION: Before installation the engine is in neutral. The central of gear shift arm must be aligned.
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Install the dowel pin and gasket. Install the gear shift mounting cover. Tighten M6 bolts to 10~12 Nm.

3.23 MAGNETO STATOR

Stator Removal

Remove left crankcase cover.

Remove stator retaining bolts.

Remove blot, washer and holding strip.

Remove the stator.
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1. Handing strip

2. Magneto stator

3. 3xM6 bolt

4. M6 bolt and washer

Stator Inspection

Check stator condition. If damaged replace it.

Check if stator wires are brittle, bad or otherwise damaged.

For electrical inspection, refer to CHARGING SYSTEM.

Stator Installation

For installation, reverse the removal procedure. However, pay attention to the following.

CAUTION: When installing the stator take care that the cable is in place (guide for wire).

3.24 MAGNETO ROTOR

Rotor Removal

Remove left crankcase cover. Refer to LEFT CRANKCASE COVER above.

Remove gasket and dowel pins.

Remove magneto bolt and magneto rotor shaft sleeve.
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1. Gasket

2. Dowel pin

3. M10 magneto bolt

4. Magneto rotor shaft sleeve

Install magneto tooling into crankshaft to remove magneto rotor.
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1. Magneto tooling
2. Magneto rotor

3. Plate gear

4. Twin gear and shaft

Remove the twin gear, twin gear shaft and plate gear.

Remove the screws for sprag clutch and then remove the sprag clutch.
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1. 6xM8 Screw

2. Sprag clutch

Rotor Inspection

Check inner side of rotor for scratches or other damage.

Check keyway on the rotor for wear or damages.

Check if trigger wheel teeth are bent or otherwise damaged.

[image: image107.png]



1. Rotor with trigger wheel

Check woodruff keyway on the crankshaft for wear or damages. 
Check the teeth on plate gear and bearing for wear or damages. Check the shaft diameter on plate gear. Replace parts as necessary.
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1. Plate gear teeth

2. Bearing

3. Shaft diameter

	Shaft Diameter

	Service limit
	63.295 mm


Rotor Installation

For installation, reverse the removal procedure. However, pay attention to the following.

Install the plate gear with lug boss facing outside to crankshaft.

Clean crankshaft and rotor with pulley flange cleaner.

Note: Do not drop the woodruff key from the crankshaft.

Align the woodruff keyway on the rotor to woodruff key on the crankshaft.

Apply LOCTITE 222 and thread-locker on the front 2 teeth of magneto bolt. Tighten magneto bolt to 50~55 Nm.

Place the small gear facing outside when installing twin gear.

Apply engine oil on hole for the twin gear shaft before installing twin gear.
3.25 SPRAG CLUTCH

Sprag Clutch Removal

Remove left crankcase cover. 

Remove rotor (refer to ROTOR above).
Remove the M8 bolts for sprag clutch and then remove the sprag clutch.
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1. 6xM8 bolt
2. Sprag clutch

Sprag Clutch Inspection

Inspect sprag clutch and wedge on the sprag clutch for wear and damage.
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1. Wedge

2. Sprag clutch

Sprag Clutch Installation

For installation, reverse the removal procedure. Pay attention to the following details.

Apply LOCTITE 263 and thread-locker on threads of sprag clutch bolt. Tighten M8 bolts for sprag clutch to 22~30 Nm.
Mark arrow on the sprag clutch face outside.
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3.26 OIL PUMP

The oil pump is located on the left side of left crankcase block.
Removal 

Remove left crankcase cover.

Remove the bolts and the oil pump cover.
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1. 2xM6 bolt

2. Oil pump cover

Remove retaining rings using an expander. Then remove washers, oil pump gear and bridge gear.
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1. Retaining ring

2. Washer

3. Bridge gear

4. Oil pump gear

Remove oil pump bolts and pull out the oil pump.
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1. 3xM5 bolt

2. Oil pump cap
Inspection

Inspect oil pump, oil pump gear and bridge gear for wear or damage. Replace if damaged.
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1. Outer rotor 

2. Oil pump cap

3. Oil pump shaft

4. Dowel pin
5. Inner rotor

Check inner rotor for corrosion pin holes or other damages. If so, replace oil pump shaft assembly.
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1. Pitting on the teeth

Using a feeler gauge, measure the clearance of inner and outer rotors as shown.
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1. Outer rotor

2. Inner rotor

A.--SERVICE LIMIT:0.25 mm(0.09 in)

If clearance of inner and outer rotors exceeds the tolerance, replace oil pump shaft assembly. Ensure to also check oil pump cover. If damaged, replace the complete oil pump assembly.

If clearance between outer rotor and its bore in crankcase exceeds the tolerance, replace the complete oil pump assembly and/ or the crankcase.

Installation

Install the outer rotor to the rotor hole of left crankcase block.
Put the inner rotor to oil pump shaft. Place dowel pin in the groove on oil pump shaft through hole on the inner rotor.

Install the inner rotor and shaft to shaft hole of the left crankcase.
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1. Outer rotor

2. Inner rotor

3. Dowel pin

4. Oil pump shaft

Tighten the M5 bolts for retaining oil pump cap to 6~9 Nm.

NOTE: The pin groove on the inner rotor faces up the inside

Clean the rotor hole and apply engine oil before installation.

Install the bridge gear to crankcase. Then install washer and retaining ring on the bridge gear shaft.

NOTE: Do not drop the bearing of the bridge gear.
Put dowel pin to oil pump shaft through the hole. Install the oil pump gear, make sure the dowel pin in the groove of oil pump gear. Then install washer and retaining ring on the oil pump shaft.
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1. Dowel pin

2. Groove on oil pump gear

Tighten the M6 bolts for oil pump cover to 10~12 Nm. 

3.27 TRANSMISSION
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Never touch CVT while engine is running. 

Never drive vehicle when pulley cover is removed.

Subcomponent installation and assembly tolerances require strict adherence to procedures detailed.

Never use any type of impact wrench at drive pulley removal and installation.

The clutch assembly is a precisely balanced unit. Never replace parts with used parts from another clutch assembly

These pulleys have metric threads. Do not SAE threads puller. Always tighten puller by hand to ensure that the drive pulley has the same type of threads prior to fully tightening.

3.27.1 REMOVAL
Remove:


-M6 bolts 


-Right crankcase cover and gasket.
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1. Right crankcase cover

2. 8xM6 bolt
3. Gasket
Tighten two M8 bolts to expand the driven pulley. 
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1.Driven pulley 

2. 2x M8 bolt

3. M20 bolt

4. M12 bolt
Remove the M20 bolt from the driven pulley.

Remove the M12 bolt from the driven pulley.

Use CVT drive wheel remove bolt to pull drive pulley out.
	CVT drive wheel remove bolt (P/N 90801014932)
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1. Special tooling 

2. Drive pulley 

3. Belt

4. Driven pulley
Remove the drive pulley and driven pulley from left crankcase block liner.

Remove the belt from pulley.

Unscrew the clamps retaining the intake/exhaust air hoses.

Remove the bolts and shroud.
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1. 3xM6 Bolt

2. Shroud

Remove the bolt and left crankcase block liner.
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1. 4xM6*20 Bolt

2. 4xM6*30 Bolt

3. 4xM6*40 Bolt

4. Left crankcase block liner

Remove the dowel pins and gaskets.
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1. Dowel pin

2. Rear gasket

3. Front gasket

3.27.2 INSPECTION
Belt

Inspect belt for cracks, fraying or abnormal wear. Replace if necessary.
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	Drive belt perimeter

	Service limit
	906.5mm


Drive Pulley

Drive pulley should be inspected annually for wear or damages.

Check drive pulley for cracks and sliding contact surface for excessive wear. Replace it if necessary.

Remove screw, washer and backing plate from the drive pulley.
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1. M12 screw

2. Washer

3. Backing plate

4. Guiding block

5. Drive Pulley 

Check screw, washer and roller for wear or damages. Replace drive pulley if necessary.

Check guiding block on the backing plate for wear or damages. Replace drive pulley if necessary.
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1. Drive pulley

2. Bearing

Check spring, spring stem and bearing on the drive pulley for wear or damages. Replace drive pulley if necessary.

Driven Pulley

The driven pulley face contacted with belt should be inspected annually for wear or damages. Replace sliding sheave if necessary.

Check spring for interference or not. Replace if interfere.
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1. Spring

2. Face contacted with belt

Left Crankcase Block Liner

Clean left crankcase block liner.

Check oil seals for damage. Replace if necessary.
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Check the front/rear gaskets if damaged. Replace if necessary.

3.27.3 INSTALLATION
For installation, reverse the removal procedure. Pay attention to following details.

Tighten M6 bolts for left crankcase block liner to 10~12 Nm.
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1. Word printed on back of belt

2. Drive pulley (front)

3. Driven pulley (rear)

The maximum drive belt life span is obtained when the drive belt has the proper rotation direction. Install it so that the word printed on the back of belt is pointing towards front of the vehicle, viewed from right cover.
Do not apply any lubricant on shaft and pulley.

Clean pulley faces and shaft with dry cloth.

Install drive pulley on crankshaft extension.

Install driven pulley on main shaft extension.

When the driven pulley is blocked, tighten M20 screw to 100-110 Nm. 

To block the drive pulley, torque M12 bolt to 80-85 Nm.

Check the bearing of drive pulley turning smooth. If not, replace or reinstall it.

Remove the two M8 bolt from driven pulley, then run the drive pulley until the belt tension.

Install gasket and right crankcase cover.

Install the center top screw in first.

Tighten the bolts as per following sequence.
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Tighten the M6 bolts to 10~12 Nm. 

3.28 ENGINE INSTALLATION

The engine installation is the reverse of the removal procedure. However, pay attention to the following.

1.
Prior to install engine, inspect condition of engine mounts. If necessary, replace the engine mounts, you can insert a punch in hole of engine mount bushing and push the other bushing out of the housing.

2.
Make sure coolant and oil drain plugs are reinstalled and tight.

Refill engine oil and check the oil level with the dipstick.
4. COOLING SYSTEM

	GENERAL
4-4
	TROUBLESHOOTING
4-4

	MAINTENANCE
4-4
	INSPECTION
4-5

	PROCEDURE
4-5
	


Ordinary Version
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	1. Radiator 
	2. M6 Bolt
	3. Hose Clamp
	4. Inlet Pipe
	5.Outlet Pipe
	6. Hose Clamp

	7.Hose Clamp
	8. M6 Bolt
	9. Lower Radiator Buffer Block
	10. Upper Radiator Buffer Block
	11. Bushing
	12.Harness Clip

	13. M6 Bolt
	14. M6 Nut
	
	
	
	


ATV625 MUD Version
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	1. Radiator 
	2. M6 Bolt
	3. Hose Clamp
	4. Outlet Pipe
	5. Inlet Pipe
	6. Hose Clamp

	7.Auxiliary Water Tank
	8. M6 Bolt
	9. Lower Radiator Buffer Block
	10. Upper Radiator Buffer Block
	11. Bushing
	12.Harness Clip

	13. M6 Bolt
	14. M6 Nut
	15. Auxiliary Water Tank Connecting Bracket
	
	


Cooling System-Engine Components
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	1. M6 Bolt
	2. Thermostat Cover
	3. Thermostat Ass.
	4. Thermostat Base

	5. O-ring
	6. Temperature Sensor of Cooling Fluid
	7. Oil Drain Plug
	8. Washer
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	1. Retaining ring 
	2. Bearing
	3. Oil seal
	4. Mechanism Seal Assy

	5. Water Pump Shaft
	6. Water Pump Impeller
	7. Seal ring
	8. Water Pump Cover

	9. M6 Bolt
	10. Washer
	11. M6 Bolt
	


4.1 GENERAL
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WARNING

	Never start engine without coolant. Some engine parts such as the rotary seal on water pump shaft can be damaged.


Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




1. If cover of radiator is open and temperature of cooling liquid is over 100℃, pressure of cooling liquid will be reduced rapidly and boiled. Vapor injection may cause danger and injuries. After drop of temperature of cooling liquid, use one cloth to cover the cover of radiator and then slowly open the cover. Cooling liquid can only be tested after complete cooling. 
2. Cooling liquid is toxic. Do not drink it or splash it to skin, eyes or clothes. In case of splashing cooling liquid to your eyes, use clean water to wash your eyes completely and contact the doctor. In case of splashing cooling liquid to your clothes, use soapy water to wash it rapidly. In case of drinking cooling liquid, vomit will be caused immediately. Please see the internist physician immediately. Store cooling liquid well and keep it out of reach of children. 
3. Check whether soil of fins is blocked or damaged. Correct curved fins. Use water and compressed air to clean soil. If damaged area reaches 20%, please replace radiator. 

4. Pump overhauling can be carried out before dismantling engine. 

5. Add cooling liquid to water tank. In addition to adding or exhausting cooling liquid, please do not open cover of radiator. 

6. Do not splash cooling liquid to plastic parts. Once splashed, please use clean water for washing. 

7. After dismantling cooling system, check leakage situation of joint. 
4.2 TROUBLESHOOTING

Sharp rise of water temperature 
- Faults of radiator cover 
- There is air in cooling system. 
- Faults of water pump
- Faults of thermostat (thermostat is not open)
- Blockage of radiator tube or cooling tube 
- Damage or blockage to radiator 
- Incomplete cooling liquid
- Failure or faults of fan motor 
No rise or slow rise of water temperature.  
- Faults of thermostat (thermostat is not closed) 

- Faults of line of water temperature display 
Leakage of cooling liquid.
- Faults of water seal 

- Aging, damage or improper sealing to O-ring. 

- Aging, damage or improper sealing to gasket
- Improper installation of pipe or hose
- Aging, damage or improper sealing to pipe and/or hose   
4.3 MAINTENANCE

COOLANT REPLACEMENT
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WARNING

	To avoid potential burns, do not remove the radiator cap or loosen coolant drain plug if the engine is hot.


Recommended Engine Coolant
	Recommended Engine Coolant

	Distilled water and antifreeze solution (50% distilled water, 50% antifreeze).


To prevent antifreeze deterioration,always use the same band. Never mix fdifferent brands unless cooling system is completely flushed and refilled.

CAUTION: To prevent rust formation or freezing condition, always replenish the system with the premixed coolant or with 50% antifreeze and 50% water. Do not use tap water, straight antifreeze or straight water in the system. Tap water contains minerals and impurities which build up in the system. During cold weather, straight water causes the system to freeze while straight antifreeze thickens and does not have the same efficiency. Always use ethylene glycol antifreeze containing corrosion inhibitors specifically recommended for aluminum engines.
Drain the Coolant:

NOTE: Never remove the radiator cap immediately when the engine is hot. Wait for the engine to cool sufficiently before removing the radiator cap. Hot coolant can cause serious burns.

1. Place the vehicle on a level surface.

2. Remove radiator service cover.
3. Remove the radiator cap and the coolant reservoir cap.

4. Place a container under the water pump drain bolt.

5. Remove the water pump drain bolt and washer.
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6. Drain out the coolant.

7. Disconnect the hose on the coolant reservoir side, and drain the residual coolant.

8. Flush the cooling system with clean water. Allow the water to drain completely from the system.

Coolant Replacement

1. Inspect water pump drain bolt and washer for damage. Replace new one if damaged.

2. Reinstall drain bolt, but do not tighten completely at this time.

3. Reinstall hose to the reservoir tank.

4. Add recommended coolant to the radiator until it appears at the top.

5. Loosen the water pump drain bolt and drain coolant until there are no air bubbles in the discharge.

6. Tighten drain bolt to 9~12Nm.

7. Refill coolant until the coolant flow out.

8.Install radiator cover.

9. Start the engine and allow it to idle until the cooling fan turns on, then turn of the engine. After cooling completely, check the coolant level in the radiator and adjust it to the top of radiator. Repeat this step until the coolant level does not change.

10. Add coolant on the reservoir tank to the upper mark.

11.Install reservoir tank cap.

12. Inspect cooling system for leaks. Please contact and authorized dealer if a leak is found.

13.Install engine side cover and radiator service cover.

NOTE: Each year or every 100 hours or when vehicle reaches 3000km, check coolant with proper tester.
4.4 INSPECTION

COOLING SYSTEM TEST

	[image: image139.png]


WARNING

	To avoid potential burns, do not remove the radiator cap or loosen the cooling drain plug if the engine is hot.


Open the water tank cover in the front storage box and remove the radiator cap.

Install the test cap and a small hose pincher on overflow hose.

Using pressure/vacuum pump, pressurize system to 100 kPa.

Check all hoses, radiator and cylinder/base for coolant leaks or air bubbles.
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Inspection

Check general condition of hoses and clamps tightness.

Check the leak indicator hole if there is oil or coolant.

NOTE: Flowing coolant indicates a defective rotary seal. Oil indicates a defective inner oil seal. If either seal is leaking, both seals must be replaced at same time. 
4.5 PROCEDURE
4.5.1 THERMOSTAT

The thermostat is a single action type. 
Removal

The thermostat is located on the top of cylinder head, on intake side.
	CAUTION

	To avoid potential burns, do not remove the radiator cap or loosen the coolant drain plug if the engine is hot.


Drain out cooling system.
Remove radiator inlet hose from thermostat.
Remove:

-thermostat housing screws and pull thermostat cover
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1. Thermostat cover

2. Screws

 –thermostat with gasket out of the hole.

Test

To check thermostat, put in water and heat water.

Thermostat should open when water temperature reaches 65℃(149°F).

Check if the gasket is brittle, hard or damaged. If damaged, replace gasket.
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Installation

For installation, reverse the removal procedure, pay attention to the following details.
	NOTICE

	Take care that the gasket is positioned exactly in the groove when installing the thermostat.


Apply a drop of threadlockerb (Loctite 243(blue)) on the threads of the thermostat cover screws.
Install the thermostat cover then torque screws to 6 Nm.

Check coolant level in radiator and coolant tank and top up if necessary.

Do not forget to bleed the cooling system. Refer to COOLANT REPLACEMENT.
Check for any coolant leakage from radiator and hoses.
4.5.2 RADIATOR AND CAP

Using a pressure cap tester, check the efficiency of radiator cap. If the efficiency is feeble, install a new 100 kPa cap (do not exceed this pressure).  

[image: image445.jpg]



Radiator Inspection

Check radiator fins for clogging or damage.

Remove insects, mud or other obstructions with compressed air or low-pressure water.

Radiator Removal

Drain cooling system.

Ordinary Version

Remove front storage box and cover.
Remove front grille and base.

MUD Version
Remove intake trim panel.
Remove:

- Radiator inlet and outlet hoses

- Overflow hose

- Radiator mounting bolt

Unplug the radiator fan connector.
Remove radiator.

Radiator Installation

For installation, reverse the removal procedure.

Pay attention to the following detail.

Install buffer block and bushing between the radiator and supports.

Fill up the radiator. Refer to COOLANT REPLACEMENT, in this section.

Check for any coolant leakage from radiator and hoses.

Tighten the M6 bolts for retaining radiator to 9~12 Nm.
4.5.3 COOLANT TANK

The coolant expands as the temperature (up to 100~110℃) and pressure rise in the system. If the limiting system working pressure cap is reached 110kPa, the pressure relief valve in the pressure cap is lifted from its seat and allows coolant to flow through the overflow hose into the overflow coolant tank.
Removal

Remove:

· The front storage box and cover.
Remove intake trim panel.(MUD Version)
- The front grille.

- Coolant tank support bolt.

- Overflow hose and clamp.

Tank Installation

The installation is the reverse of the removal procedure.

4.5.4 RADIATOR FAN

Radiator Fan Removal

Unplug radiator fan connector.

Remove bolts.
Separate the radiator and fan.

Radiator Fan Test

NOTE: The ECU controls the radiator fan by the input of the coolant temperature sensor (CTS). The radiator fan should turn on when coolant temperature reaches 98℃ and should turn off when the coolant cools down at 95℃ (203°F).

Connect the vehicle to Diagnostic Tool. Refer to ENGINE MANAGEMNT for procedure and connector location.
	Diagnostic Tool-Delphi
(P/N 2104040000)
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In ACTIVATION folder, press COOLANT FAN button.

If fan turns, check CTS, wiring harness and connectors. If all parts are good, replace the ECU.
U.

If fan does not turn when COOLANT FAN button is pressed, use the following troubleshooting chart to resolve the problem.
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If all of the above test good, replace radiator fan.

Radiator Fan Installation

For the installation, reverse the removal procedure.
4.5.5 COOLANT TEMPERATURE SENSOR(CTS)
Removal
NOTE: The CTS is located on the top of cylinder head near the thermostat.
Install a larger hose pincher on both radiator hoses.
Unplug the CTS then remove it.
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1. Thermostat

2. CTS
Testing the CTS Resistance

1. Disconnect the plug connector from the CTS and check the resistance of the sensor itself.

	CTS Resistance Test

	CTS pin
	Specification @ 20 °C (68 °F)

	1
	2
	2280 - 2720 Ω


2. If resistance is out of specification, replace the CTS.

3. If resistance test is good, reconnect the CTS.

4. Disconnect the engine connector from the ECU.

5. Using a multimeter, recheck resistance from the ECU connector as per table.
	CTS Resistance Test at ECU

	ECU Pin
	Specification @ 20 °C (68 °F)

	22
	39
	2280 - 2720 Ω


6. If resistance value is correct, replace the ECU.

7. If resistance value is incorrect, repair the connectors or replace the wiring harness between ECU connector and the CTS.

Installation
For installation, reverse the removal procedure.
CAUTION: Never use the gasket ring a second time. Always install a new one.
Torque temperature switch to 16 Nm (142 lbf.in).
Check coolant level in radiator and coolant tank and top up if necessary.
4.5.6 WATER PUMP COVER
It is located on the left crankcase cover.

Removal
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WARNING

	To avoid potential burns, do not remove the radiator cap or loosen the cooling drain plug if the engine is hot.


Remove engine side cover and service cover.
Drain cooling system.

Remove radiator outlet hose from water pump cover.

Remove bolts retaining water pump cover.
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1. 5xM6 bolt
2. Water pump cover 

3. Sealing ring 

Pull water pump cover to remove it.

Inspection 

Check if sealing ring is brittle, hard or damage and replace as necessary.

Installation 

The installation is the opposite of the removal procedure.

CAUTION: To prevent leaking, take care that the sealing ring is exactly in groove when you reinstall the water pump cover.

Tighten M6 bolts for water pump cover in the crisscross sequence to 10~12 Nm.
4.5.7 WATER PUMP IMPELLER AND SHAFT
Removal

Remove water pump cover.

Remove left crankcase cover.

Use the expander pliers to remove the retaining ring on the shaft.

Remove the water pump shaft and impeller.
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1. Retaining ring

2. Oil seal

3. Water pump shaft

4. Mechanism seal Assy.
5. Water pump impeller

CAUTION: Water pump shaft and impeller have right-hand threads. Remove by turning counterclockwise and install by turning clockwise. 
Inspection
Check water pump impeller and shaft for wear or damage. Replace if damaged.
Check oil seal and Mechanism seal on the left crankcase for wear or damage. Replace if damaged.
Water pump shaft with seal must rotate freely. Otherwise, replace it.
Installation

The installation is the opposite of the removal procedure. Be careful not damage impeller wings during installation.
Install the water pump shaft to the impeller.

Install the shaft to the left crankcase cover. Then use retaining ring to retain the shaft.
5. FUEL SYSTEM
	FUEL TANK AND FUEL PUMP
5-1
	THROTTLE BODY
5-5


5.1 FUEL TANK AND FUEL PUMP
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Names of components: 
	1. Fuel Tank
	2. M8 Bolt
	3. Fuel Pump
	4. M5 Bolt
	5. Tank Cap
	6. Fuel Filter

	7. Fuel Filter Bracket
	8. M6 Bolt
	9. River Nut
	10. Fuel Hose
	11. Hose Clamp
	


GENERAL
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WARNING

	Fuel is flammable and explosive under certain conditions. Ensure work area is well ventilated. Do not smoke or allow open flames or sparks in the vicinity.
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WARNING

	Always disconnect battery prior to working on the fuel system. Always disconnect battery exactly in the specified order, BLACK(-) cable first. It is recommended to disconnect electrical connections prior to disconnecting fuel lines.


Whenever working on fuel system, always verify for water or dust infiltration in reservoir.

During assembly/installation, use the torque values and service products as in the exploded views.
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WARNING

	Torque wrench tightening specifications must strictly be adhered to.

Locking devices (e.g.: locking tabs, elastic stop nuts, self- locking fasteners, cotter pin, etc.) must be installed or replaced with new ones where specified. If the efficiency of a locking device is impaired, it must be renewed.
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WARNING

	Replace any damaged, leaking or deteriorated fuel lines.


Dismantling 

1. Disconnect wire group plug-in of fuel sensor, separating fuel sensor from wire group. 

NOTE: Do not pull the plug directly when you pull it out. Press the plug by hand and pull it out at both ends.
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WARNING

	Special attention should be paid to explosive gasoline. 


2. Unplug the tubing and tank vent after releasing the hose clamp, and then rotate the oil pump cap in the direction of the arrow. After completing the above steps, the oil pump can be removed from the tank for repair or replacement.
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Note: Clamp should not be used repeatedly; new clamp should be used upon installation.

When pulling out fuel pipe, attention should be paid to pressure inside fuel pipe, splash proof measures should be taken and vessel should be prepared to discharge fuel inside fuel pipe in advance. 

3. Loose the clamp and bolt for the throttle valve, unplug the relevant connector, and remove the throttle valve from the body for maintenance.

[image: image153.png]



Tightening torque of M8 bolt for throttle valve: 22~30 Nm.
Unplug the high voltage coil and remove the spark plug with a tool.

Available overhaul:

Replace and conduct daily maintenance of spark plug.

4. After removing the screw with a screwdriver, open the throttle valve cover and remove the pin of the throttle cable head from the throttle cable. Then separate the throttle cable and throttle valve.

Available overhaul:

Replace and conduct daily maintenance of throttle valve combination and accelerator cable combination.

5. Disconnect cylinder fuel nozzle, crankshaft position sensor and starting motor plug-in separately. 

Remove the hose clamp and pull out the fuel hose connected to the fuel injector.

Available overhaul:

Replace and conduct daily maintenance of fuel pipe. 
INSPECTION

FUEL PRESSURE TEST

The pressure test will show the available pressure at the fuel pump outlet. It validates the pressure regulator, the fuel pump and leaks in the system.

Before proceeding to the pressure test ensure the battery is fully charged. Battery voltage must be over 12 volts.

Ensure there is enough gasoline in fuel tank.
Remove LH side panel.
Disconnect outlet hose.

Install fuel pressure gauge and T-fitting between disconnected hoses.
Using Diagnostic Tool to reactive fuel pump by press button.
Turn ignition key ON and set engine stop switch to RUN and observe fuel pressure. Turn ignition key off then back on. Repeat the test.
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Standard fuel pressure: 350kpa.

A rapid pressure drop indicates leakage is from the fuel rail, if there is not leaking then replace fuel pump.

A slow pressure drop indicates leakage either from the fuel injector or from the fuel pressure regulator. Check fuel injector and the fuel pressure regulator for leaks. If it is not leaking then replace fuel pump module.

If no leakage, start engine and observe fuel pressure. The fuel pressure should be the same as above.

If pressure is within limits, fuel pump and the fuel pressure regulator are working adequately.
Release fuel pressure in the system using Diagnostic Tool.
Remove pressure gauge from inlet hose. Reconnect inlet hose.
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WARNING

	Wipe off any fuel spillage. Fuel is flammable and explosive under certain condition. Allways work in a well-ventilated area.


Reinstall removed parts.
PROCEDURES

FUEL HOSE AND CLAMP
Fuel Hose Replacement
When replaced fuel hoses, be sure to use hoses and clamp as available from ODES parts department. This will ensure continued proper and safe operation.
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WARNING

	Use of improper fuel hoses could compromise fuel system integrity.
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WARNING

	Whenever removing a hose in the fuel system, always use a new clamp at assembly. Then validate fuel tightness by performing a fuel pressure test.


Clamp Replacement
Use pliers to secure or cut clamps on fuel hoses.
FUEL FILTER

Replace fuel filter as per amintenance schedule. 
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Removal
Detach filter from frame.
Remove clamps and pull hoses off. 
Inspection

If fuel filter is suspected to be clogged, it may be checked as follows:

Using low compressed air, check if fuel filter is clogged. Air should flow easily through filter. In doubt, install a new filter.

Installation

Use arrow on filter to position it according to fuel flow.

FUEL TANK

Draining
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WARNING

	Never perform this operation when the engine and/or the exhaust system is/are hot.

Never sue a hose pincher on injection system high pressure hoses.


Remove fuel tank cap and siphon gasoline in an approved fuel container.

Fuel tank removal

Remove the seat.

Remove the LH rear side panel.

Remove fuel pump from fuel tank.

Disconnect fuel hose from fuel tank.

Remove retaining screws, then remove fuel tank.

Fuel tank inspection

Inspect fuel tank for any damage or cracks which may result in fuel leaks. If so replace tank with a new one. Inspect tank and protector attachment points for damage. Inspect protector for damage.

Fuel tank installation
For installation, reverse the removal process but pay attention to the following. 

Reconnect fuel pump connector and fuel hose. 

Tighten retaining M8 bolts to 22～30Nm.

Refuel tank and ensure there are no leaks. 
FUEL PUMP

Fuel pump electrical test

When turning ignition key ON, the fuel pump should run for 5 seconds to build up the fuel pressure in the system.

If the pump does not work, disconnect the connector from the fuel pump.

Install a temporary connector to the fuel pump connector. Apply 12V to this test harness.

CAUTION: Running the fuel pump a few minutes with reverse polarity can damage the pump.

If pump does not run, replace a new pump.

Otherwise, check fuse and if good, probe terminals of fuel pump connector on vehicle harness or its connector, Repair or replace appropriate part.

Removal
Use Diagnostic Tool to release fuel pressure.
	Diagnostic Tool-Delphi
(P/N 2104040000)
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Remove fuel pump, outlet hose and harness.

Remove fuel pump retaining screws.

Gently push pump up.

CAUTION: While pulling out the fuel pump, pay attention to fuel sensor float arm. Float arm can get stuck and bend which can reduce the fuel sensor capabilities.

Installation

For installation, reverse the removal process but pay attention to the following.
Install a new gasket.

Pay attention to pump orientation.

Tighten retaining screws.

Install hose properly on OUT nipples and harness.

FUEL LEVEL SENSOR

The level sensor is part of the fuel pump module mounted inside the fuel tank. 

Inspection

Dismantle the fuel pump module mounted inside the fuel tank (refer to above steps)

Turn on ignition switch.

Use hands to shake fuel sensor’s floating device, locating floating device to see whether it is fit

with indication of fuel meter.

Turn off the ignition switch and disconnect connector, measure resistance:

Lower:Pink/White and Black: 6-9 Ω

Lift: Pink/White and Black: 90-95 Ω

If the resistance is not within empty and full values, replace fuel pump module. If the fuel level sensor is good, try a new multifunction gauge.

Inspection

Install fuel sensor to fuel tank. Connect connector and hose. Turn on fuel supply switch, and check whether functions of fuel meter is normal or not. 

Fuel leakage is not allowed.
5.2 THROTTLE BODY
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Names of components: 
	1. O2 Sensor
	2. Injector Bracket
	3. Fuel Injector
	4. Gasket
	5. M6 bolt
	6. Intake Air Pressure Sensor

	7. M8 bolt
	8. Intake pipe
	9. Rubber Sleeve
	10. Clamp
	11. Throttle body
	


GENERAL
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WARNING

	When electrically disconnecting or removing the throttle body from the intake manifold, always turn off the engine and disconnect the battery.




	[image: image162.png]


WARNING

	Always disconnect battery prior to working on the fuel system. Always disconnect battery exactly in the specified order, BLACK (-) cable first. Electrical connections should be disconnected prior to disconnecting fuel lines.
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WARNING

	Fuel is flammable and explosive under certain conditions. Wear safety glasses and work in a well-ventilated area. Do not smoke or allow open flames or sparks in the vicinity.
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WARNING

	Proceed with care and use appropriate safety equipment when working on the fuel system. Wipe off any fuel spillage in the engine. Do not allow fuel to spill on hot engine parts and/ or on electrical connectors.


Cover the fuel line connection with an absorbent shop rag before disconnecting them. Slowly disconnect the fuel hose to minimize spilling.
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WARNING

	Replace any damaged, leaking or deteriorated fuel lines or connections. After working on the fuel system, always pressurize the fuel system and check for fuel leaks. Refer to FUEL SYSTEM subsection.


ECU (Engine Control Unit)

From input signals, the ECU acknowledges driver demands and converts them to an engine torque requirement through calculation of several variables. Then, the ECU controls the iTC, the injection system and the ignition system to meet the torque requirement.

The ECU manages the engine torque requirements and controls engine operation to ensure it is delivering optimum performance and fuel economy. The ECU also controls idle RPM and limits maximum engine speed through the iTC system.
EFI Sensors
To control the engine, the ECU reads the inputs from the sensors which it compares to predetermined parameters stored in the ECU (fuel and ignition maps), makes computations, and activates the outputs accordingly (injectors, ignition coils etc.).
Signals from sensors are used by the ECU to determine the injection and ignition parameters (referenced to fuel maps) as required to maintain the optimum air-fuel ratio.
To control the injection system, the engine management uses input signals from the following sensors:

- Crankshaft position sensor (CPS)

- Manifold absolute pressure and temperature sensor (MAPTS)

- Throttle position sensor (TPS) which is integrated to the throttle body (Electronic Throttle Control (ETC))

- Throttle accelerator sensor (TAS).

- Coolant Temperature Sensor (CTS)
Air Filter

Air, drawn into the air filter housing, first passes through an inlet duct.

After it passes through the air filter, an air duct) is used to channel the air to the throttle body.
Throttle Body ((ETC) Electronic Throttle Control)

Air for combustion is drawn in by the engine. The air flows through the throttle body (ETC) and is controlled by a throttle plate.
The Electronic Throttle Control (ETC) is a throttle body with throttle position sensors (TPS) and electric throttle actuator (ETA) and is mounted on the intake manifold.
The ETA allows the ECU to electronically control the throttle plate opening which regulates the amount of air that enters the engine, and therefore engine speed.
Fuel Injector
An injector is used to inject fuel into the intake pipe of the engine.
Fuel is injected in accordance with injection signals received from the ECU.
Fuel Pump

An electric fuel pump with an integrated pressure regulator and fuel system filters is used. For more details on the fuel pump unit, refer to Fuel Tank and Fuel Pump subsection.
Idle Speed

Idle speed is not adjustable. The ECU controls the idle speed of the engine primarily through control of the throttle plate position.

The vehicle multifunction gauge can provide an accurate digital readout of the engine's idle speed.

The engine RPM may also be verified using the Diagnostic Tool.

In Diagnostic Tool, go to:

- Measurements page

- ECU button.

NOTE: The gauge and Diagnostic Tool use the same signal to provide the engine RPM indication.

TROUBLESHOOTING

DIAGNOSTIC TIPS

Engine problems are not necessarily related to the fuel injection system.

It is important to ensure that the engine and propulsion system, fuel delivery and electrical systems are functioning normally.

For diagnostics purposes, use Diagnostic Tool.
After a problem has been solved, be sure to clear the fault(s) recorded in the ECU using the Diagnostic Tool.
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WARNING

	Electrical actuators   and electronic modules may be powered up as soon as the START/ STOP switch is depressed. Always disconnect the battery prior to disconnecting any electrical or electronic parts.


Never use a battery charger to temporarily substitute the battery as it may cause the ECU to function erratically, or not at all.

Check related-circuit fuse solidity and condition with an ohmmeter. A visual inspection could lead to a false diagnosis.

Poor Idling

If poor idling is experienced, check the following:

- Poor quality fuel or water in the fuel

- Fault codes using Diagnostic Tool
- Throttle body cleanliness

- Engine leaks or other mechanical problem.

Electrical Related Problems

It is important to check the following in the electrical system:

- Battery voltage

- Fuses

- Ground connections

- wiring and connectors.

Ensure that all electronic components are original recommended components. Any modification to the wiring harness may lead to poor system operation or generate fault codes.

Electrical Connections

Pay particular attention to ensure that terminals and pins are not out of their connectors, corrosion, or out of shape.

When probing terminals, pay attention not to deform the terminals as this could cause a loose or intermittent connection that would be difficult to troubleshoot.

NOTE: Do not apply dielectric grease or other lubricants on the ECU connectors.
PROCEDURES
ENGINE CONTROL UNIT (ECU)
NOTE: As a first troubleshooting step, always check for applicable fault codes using Diagnostic Tool.
ECU Location
The ECU is located on the LH side of air filter housing.
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1. ECU
The ECU connectors have 48 pins.
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NOTE: For connector information, cleaning and probing.
OBD Location
The OBD is located under the operator’s seat.
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1. OBD
1. Remove the operator’s seat, refer to BODY subsection.
2. Pull the OBD cover, then connect the Diagnostic Tool to OBD connector.
ECU Power Circuit Validation

Briefly press START/STOP switch.

This should wake up the ECU. The ECU will then activate relay for approximately 12 seconds after which it will turn off all power.
	QUICK INDICATION THAT ECU IS POWERED (ASSUMING THE OBSERVED COMPONENTIS WORKING)

	Multifunction gauge comes ON.

	Fuel pump turns on for approx. 2 seconds


If ECU does not turn on, check the following:

- Fuse 

- Battery voltage. Refer to CHARGING SYSTEM
- Relay 

- START/STOP switch. Refer to ELECTRICAL

SYSTEM

- ECU power circuit wires and ground wires.

For testing of fuses and relay, refer to ELECTRICAL

SYSTEM subsection.
NOTE: When relay is not working, the EMS
(engine management system) and the complete vehicle electrical system will not be powered.

ECU Wake Up Circuit Test

1. Use a multimeter and select Vdc.
2. While pressing START/STOP switch, read voltage as follows.

	ECU Pin
	Battery
	VOLTAGE

	Pin 5 (Black)
	Positive Terminal
	Battery Voltage


If voltage is as per specification, refer to ECU POWER CIRCUIT TEST.

If voltage is out of specification:

- Test the START/STOP switch, refer to ELECTRICAL SYSTEM subsection.

- If START/STOP switch tests good, test wiring and connectors from battery to ECU. Refer to WIRES DIAGRAM.

ECU Power Circuit Test

1. Remove the operator’s seat.

2. Install an appropriate fused jumper wire between the following terminals on the ECU.

	JUMPERWIRE COORDINATESON ECU

	Pin 14
(Light green/yellow)
	EFI Relay,EFI Fuse


NOTE: When the jumper is installed, the multifunction gauge should come on.

If the multifunction gauge did not come on, check the following:

- Fuses 

- Relay 

- Wiring between ECU contact Pin 14 and fuse 

- ECU ground circuit, refer to CONTINUITY TEST OF ECU GROUND CIRCUITS in this subsection.

For testing of fuses and relay, refer to ELECTRICAL

SYSTEM subsection.

If gauge came on, carry on with the following step.

3. Remove fuse 

4. Set multimeter to Ω.

5. Check resistance as follows.

	ECU
	BATTERY
	READING

	PIN
	TERMINAL
	Ω

	Pin 14
(Light green/yellow)
	Negative

(Ground)
	Close to 0 Ω


If voltage is not measured, check the wiring and connections between ECU and fuse, refer to the WIRES DIAGRAM subsection.

If all items mentioned in this test and in ECU WAKE UP CIRCUIT TEST tested good, try a new ECU.

Continuity Test of ECU Ground Circuits

1. Set multimeter to Ω and probe adapter terminals as per following table.
	OBD
	BATTERY
	READING

	PIN
	TERMINAL
	Ω

	Pin4(Black)
	Negative

(Ground)
	Close to 0 Ω

	Pin5(Black)
	
	


If any measurement is out of specification refer to ELECTRICAL SYSTEM subsection and check the following:
- Wiring and connections

- Engine ground

- Battery ground

- Frame ground.

ECU CAN Line Test

CAN lines link the ECU, multifunction gauge and OBD.

Test CAN wire continuity as follows.

1. Disconnect ECU connector.

2. Disconnect multifunction gauge connector.
Refer to ELECTRICAL SYSTEM subsection.

3. Check wire resistance as follows.
	OBD
	ECU
	MEASUREMENT

	Pin5(Black)
	Pin 5(Black)
	Close to 0 Ω


If continuity is out of specification, repair or replace wiring harness between ECU and OBD.

If continuity is as per specification, carry out the following test.

4. Read wire resistance as follows.

	ECU
	Gauge

Connector
	Measurement

	Pin 29
(Light green)
	Pin 21
(Light green)
	Close to 0Ω


If continuity is out of specification, repair or replace wiring harness between ECU and multifunction gauge.

If continuity is as per specification, CAN lines are functional.

Reconnect connectors and reinstall removed parts.

ECU Removal

NOTE: If a new ECU is to be installed, first read the procedures in ECU REPLACEMENT in this subsection.

1. Disconnect battery cables.

NOTICE: Always disconnect the BLACK negative (-) battery cable first, then disconnect RED positive (+) cable.

2. Refer to BODY subsection and remove the LH side panels.

3. Disconnect ECU connectors from ECU.

4. Remove M6 bolts and remove the ECU from its support.
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ECU Installation
1. Reverse removal procedure. 
Tightening of M6 bolts for ECU to torque: 9-12Nm.
2. Reconnect ECU connectors.
3. Reconnet battery cables.
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WARNING

	Always reconnect the RED positive (+) battery cable first, then reconnect BLACK negative (-) cable.


4. If a new ECU is installed, refer to ECU REPLACEMENT in this subsection.

NOTICE: Always replace ECU by the same part number.
ECU Replacement

NOTE: Prior to replacing an ECU, ensure that all the recommendations in the general introduction of this subsection have been followed and all applicable testing procedures have been carried out.

When the ECU is replaced, data must be entered into the new ECU. 
FUEL INJECTOR

Fuel Injector Removal

1. Refer to BODY subsection and remove both side panels.

2. Refer to AIR INTAKE SYSTEM subsection and remove the following parts:

- Air filter housing
- Air intake hose from throttle body.
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1. Fuel Injectors

2. Fuel Injector connectors

3. M8 bolt

3. Disconnect the fuel injector connectors.
4. Loosen M8 bolt, then remove the fuel injector.
5. Loosen the clamp, separate the fuel injector and fuel hose.
Fuel Injector Operation Test with Diagnostic Tool (Dynamic)

1. Connect Diagnostic Tool to OBD. 
2. Start engine.

3. In Diagnostic Tool, click the following:

- Read Data button

- Monitoring tab.

4. Using the Diagnostic Tool, shut down engine cylinder one at a time by clicking on the button under the applicable cylinder.

If the engine RPM drops when clicking on a cylinder, the injector and the ignition of this cylinder are functioning normally.

If the engine RPM does not drop when clicking on a cylinder, this cylinder is not functioning properly. Check the following:

- Fuel injector operation. Refer to FUEL INJECTOR OPERATION TEST WITH Diagnostic Tool (STATIC).

- Spark plug and ignition coil. Refer to IGNITION SYSTEM.

- Engine condition.

Fuel Injector Operation Test with Diagnostic Tool (Static)

NOTICE: After fuel injector activation using Diagnostic Tool, always crank engine in drowned mode to ventilate engine and prevent a potential backfire due to fuel accumulation in the engine.

1. Connect Diagnostic Tool to OBD. 
2. In Diagnostic Tool, click the Read Data button to read the new ECU.

3. On the Activation page of Diagnostic Tool, energize the fuel injector to be tested.

You should hear the inject or functioning.

This will validate the inject or mechanical and electrical operation.

If the inject or does not function, carry out the FUEL INJECTOR RESISTANCE TEST.

Fuel Inject or Balance Test

NOTICE: After fuel inject or activation using Diagnostic Tool, always crank engine in drowned mode to ventilate the engine of fuel.

1.Install a fuel pressure gauge as described in FUEL PUMP PRESSURE TEST subsection.

2. Connect Diagnostic Tool to OBD. 
3. In Diagnostic Tool. select the following:

- Read Data button

- Activation page tab.

4. In Diagnostic Tool, click on the Fuel Pump button to activate fuel pump.
5. Fuel pressure must be within specification. Refer to FUEL TANK AND FUEL PUMP subsection. Reactivate fuel pump as necessary.

6. In Diagnostic Tool, energize fuel injector.

7. Record the fuel pressure drop for injector.

8. In Diagnostic Tool, click on the Fuel Pump button to activate fuel pump.

9. The maximum fuel pressure drop between injectors should not exceed the following specification:
	Maximum Fuel Pressure Drop Allowed
Between Fuel Injector

	10kPa (1.5 Psi)


If the pressure drop between fuel injectors is greater than the specification, replace the inject or with the least pressure drop, then repeat the test.

11. Using the valve on the fuel pressure gauge, release the pressure in the system (if so equipped).

12. Remove fuel pressure gauge and reinstall removed parts.

13. Set engine emergency off switch to OFF.

14. Crank engine in drowned mode (accelerator held all the way in) to ventilate the engine of the fuel that was injected during the test.
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WARNING

	Always crank engine in drowned mode to ventilate all fuel that was injected during the test. Failure to do so may result in severe engine damage and injury.


Fuel Inject or Leakage Test

Test Setup

1. Ensure there is enough fuel in fuel tank.

2. Ensure fuel pressure from fuel pump is within specification. Refer to FUEL TANK AND FUEL PUMP subsection.

NOTE: Keep the pressure gauge installed for the leakage test.

3. Set engine emergency stop switch to STOP.
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WARNING

	The engine emergency stop switch is set to STOP to prevent any spark in the engine compartment should the engine be cranked. Fuel vapors may ignite in presence of a spark creating a fire hazard.


4. Disconnect the vehicle from Diagnostic Tool by disconnecting the POWER INTERFACE from the vehicle diagnostic connector.

5. Wait for vehicle electrical power to shut off; the multifunction gauge will turn off.

6. Remove fuel hose with injectors from engine. 
7. Position fuel hose so that an appropriate container may be placed under the injectors to collect any fuel leakage.

8. Connect Diagnostic Tool to OBD. 
Leakage Test

1. In Diagnostic Tool, select the following:

- Activation page tab

- ECU page.

2. Click on the Fuel Pump button to activate fuel pump for a few seconds.

3. Check for fuel leakage from the injector nozzles.

4. Monitor fuel pressure at fuel pressure gauge. If pressure drops below 250kPa (36 PSI) during the test, reactivate fuel pump as necessary.
	Fuel Injector Leakage

	Test Duration
	Specification

	2 minutes
	1 drop per minute maximum


If test is not within specification, replace the faulty fuel injector.

5. Reinstall remaining removed components.
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WARNING

	Wipe up any spilled fuel.


Fuel Injector Resistance Test
1. Ensure vehicle electrical power is off, remove fuse.

2. Remove cover from the front fuse box and locate fuse.

3. Check resistance value between fuse box and ECU connector terminals as follows.

	ECU
	Fuse box
	READING

	PIN
	Termianl
	Ω @ 20℃ (68℉)

	Pin8
(Brown/yellow)
	EFI relay


	0Ω


If resistance value obtained is correct, carry out a FUEL INJECTOR INPUT VOLTAGE TEST.
If resistance value obtained is incorrect, remove injector connector and check resistance value between injector pins as follows. Refer to FUEL INJECTOR ACCESS in this subsection.
	INJECTOR
	Resistance

	PIN
	Ω@ 20℃ (68℉)

	PinA
(Brown/yellow)
	PinB
(Grey/yellow)
	12 ±0.6 Ω


If resistance is out of specifications, replace injector.

Fuel Injector Input Voltage Test
1. Ensure ECU connector is properly connected.

2. Disconnect the fuel injector connector. Refer to FUEL INJECTOR CONNECTOR ACCESS in this subsection.

NOTE: Press against tab underneath connector as illustrated to unlock it.

3. Ensure fuse is properly installed.

4. Set engine emergency stop switch to STOP to prevent engine starting.

5. Momentarily press the START/STOP switch to wake up the ECU.

NOTE: It is not necessary to activate the injector since it is continuously powered when the ECU is awake.

6. Use a multimeter and set it to Vdc. Read voltage.
	INJECTOR
	BATTERY
	READING

	WIRE
	TERMINAL
	VOLTAGE

	Brown/yellow
	Battery Ground
	Battery voltage

	
	
	


If inject or input voltage is good, carry out the following:

- Circuit continuity test between injector and ECU, refer to WIRES DIAGRAM subsection.

- FUEL INJECTOR SIGNAL TEST further in this subsection.

If inject or input voltage is not good, check the following:

-Fuse 

-Circuit continuity between fuse and injector. Refer to WIRES DIAGRAM subsections.

Fuel Injector Installation
For the installation, reverse the removal procedure however, pay attention to the following details.

NOTICE: If installing the removed inject or(s), ensure inject or O-rings are in good condition. Replace O-rings as required.

1. Apply a thin film of engine oil to O-rings to ease insertion in rail.

2. Install fuel inject or with your hand. Do not use any tool.

3. Ensure proper positioning of the intake manifold O-ring on inject or as in following illustration.

4. Carefully insert injector in air intake manifold paying attention to the manifold O-ring.

NOTICE: Gently push O-ring in evenly all around while inserting injector. O-ring must be completely inserted and not visible, before completing the insertion of the injector.

5. Firmly push injector until it bottoms out.

6. Install fuel hose.

7. Apply engine oil on O-rings of fuel pressure hose fitting.
Pressurize the fuel system and check for fuel leaks. Refer to FUEL SYSTEM PRESSURIZATION in FUEL TANK AND FUEL PUMP subsection.
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WARNING

	Failure to pressurize the fuel system and checking for fuel leaks may result in severe injury or a life threatening situation should a leak occur.


8. Reinstall all remaining removed parts.
THROTTLE BODY (ETC (ELECTRONIC THROTTLE CONTROL))

Throttle Body (ETC) Description
Electric Throttle Actuator (ETA)

The electric throttle actuator (ETA) is a DC motor on the throttle body that regulates the throttle plate via a drive gear. It receives its control signal from the ECU. Pulse width modulation (PWM) is used to control the motor.

Throttle Plate Operating Positions

Two torsional springs are connected to the throttle plate. A main spring and another one in a plunger mechanism.

When there is no power to the throttle actuator (ETA), the plunger mechanism maintains the throttle plate at a rest position. This also serves as the limp home position.

When the throttle plate is opened by the ETA as commanded by the ECU, it acts against the main spring. If the ETA failed, the return spring would bring the throttle plate back to the limp home position.

Throttle Body (ETC) Faults and Effects

NOTE: Among other things, a weak or broken spring and a sticky throttle plate are validated by the throttle body diagnostic mode.
	FAULT
	EFFECT

	Partial

failure of
TAS sensor

(One
internal

sensor

only)
	Limp home mode. Engine speed limited to idle.

ECU will use the remaining TAS sensor.

Fault code set and beeper activated to emit warning signals. Check engine light is turned ON. Drivability could be reset by releasing and reapplying the throttle.

	Complete failure of
TAS sensor

(Both
internal

sensors)
	Limp home mode. Engine speed limited to 2500 RPM. Fault code set and beeper activated to emit warning signals. Check engine light is turned ON.

	Any

throttle

body

failure
	Limp home mode. Engine speed limited to 2500 RPM.

Engine speed can still be increased up to 3200 RPM using the throttle lever.

Fault code set and beeper activated to emit warning signals. Check engine light is turned ON.


NOTE: Refer to FAULT CODES and INTELLIGENT THROTTLE CONTROL (iTC) subsections for more informations.

Throttle Body (ETC) Access

1. Refer to appropriate subsection to remove:

- LH side panel

- Air filter housing
- Air intake hose.

Throttle Body (ETC) Lubrication

No lubrication is required.

Electric Throttle Actuator (ETA) Test

Electric Throttle Actuator (ETA) Test with Diagnostic Tool 
1. Connect Diagnostic Tool to OBD
2. Press the START/STOP button to wake up the ECU.

3. In Diagnostic Tool, select:

- Read Data button

- Setting page tab.

NOTE: Use the Setting page to confirm ETA movement. The Monitoring page will not read the actual ETA movement.

4. Slowly depress the throttle lever from the idle to WOT. The ETA should go from almost 10%to 100%.

If result is out of specification, carry out a THROFTLE POSITION SENSOR INITALIZATION. Refer to THROTTLE POSITION SENSOR (TPS) in this section.

NOTE: The ETA is reset at the same time as the TPS.

After the reset, test ETA again.

If the result is still out of specification, check wire continuity between ECU and throttle body before assuming the ETA is at fault.
Throttle Body (ETC) Inspection

1. Remove parts required to access throttle body, refer to THROTTLE BODY (ETC) ACCESS.

2. Carry out the following:

- Inspect throttle body for cleanliness.

- Ensure throttle plate opens fully and smoothly.

- Check for corrosion or damaged wiring or damaged ETC connectors.

Throttle Body (ETC) Dynamic Tests

1. Remove the parts required to access the throttle body (ETC), refer to THROTTLE BODY (ETC) REMOVAL.

2. Remove the air inlet hose from the throttle body.

3. Observe the throttle plate with the engine stopped.

NOTE: The throttle plate should be in the rest position (slightly opened).
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WARNING

	Keep your fingers out of the throttle plate area while the ECU turns on. The throttle actuator will cycle. This could cause serious finger injuries as throttle plate quickly moves.


4. As you observe the throttle plate, have someone press the START/STOP switch to wake up the ECU.

NOTE: The throttle plate should cycle quickly from the rest position to a partially open position (approximately 15°), then back to the rest position.

5. As you observe the throttle plate, have someone gradually and evenly pull in the throttle lever, then release it in the same way.

NOTE: The throttle plate should open then close according to throttle lever position however, the movement of the throttle plate may not be linear with the displacement of the throttle lever.

If any test failed, proceed with the THROTTLE BODY (ETC) STATIC TESTS.

Throttle Body (ETC) Static Tests
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WARNING

	First ensure the ECU is off. Do not move the throttle plate using your fingers. Otherwise, should the START/STOP switch be pressed, the ECU would turn on and quickly cycle the throttle plate which could cause serious finger injury.


1. Using a blunt tool, push in on the throttle plate and ensure it opens smoothly within the throttle body.
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1. Push here to open
NOTE: The throttle plate must open fully and return freely to the rest position (slightly opened) when released.

2. Push throttle plate to close throttle body. It must close completely and return freely to the rest position (slightly opened) when released.

If the throttle plate does not move smoothly or does not return freely to the rest position, the problem is mechanical. Check for dirt accumulation on throttle plate shaft. It may also be an actuator or gear problem. Replace throttle body as necessary.

If throttle plate operates normally, the problem is electrical. Check electric throttle actuator (ETA) wiring continuity, throttle position sensor (TPS) and throttle accelerator sensor (TAS).
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WARNING

	If the throttle plate does not return to its rest position properly after a proper cleaning, replace the throttle body.


If the throttle plate does not return to its rest position properly after a proper cleaning, replace the throttle body.

Throttle Body (ETC) Cleaning

1. Remove throttle body from intake manifold. Refer to THROTTLE BODY (ETC) REMOVAL in this subsection.

2. Check throttle body cleanliness using a flashlight. Fully open throttle plate and verify:

- Throttle body bore

- Throttle plate edge.

Look for:

- Dirt

- Oily surfaces

- Carbon and dirt deposits on throttle plate and the surrounding bore.

3. Clean as necessary.

4. Use a throttle body cleaner such as GUNK INTAKE MEDIC or an equivalent.

NOTICE: Only use an appropriate throttle body cleaner that will not damage O-rings and EFI sensors.

CAUTION: Use the product in a well-ventilated area. Refer to product manufacturer's warnings.

5. To avoid getting dirt into engine, spray cleaner on a clean rag then rub rag against throttle plate and bore. A toothbrush may also be used.

CAUTION: Ensure ignition key is removed and battery cables are disconnected so that nobody can activate the electrical system, otherwise the ECU would turn on and the throttle actuator (ETA) would cycle. This could cause serious finger injury as the throttle plate moves quickly.

6. Gently open throttle plate and hold fully open to clean all surfaces.

7. To remove residual dirt, spray cleaner on throttle plate and throttle bore.

8. Reinstall all removed parts.

Throttle Body (ETC) Removal
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WARNING

	When electrically disconnecting or removing the throttle body from the intake manifold, always remove ignition key and disconnect the battery.


1. Remove parts required to access throttle body, refer to THROTTLE BODY (ETC) ACCESS.

2. Detach throttle cable from handlebar.

3. Disconnect ETA and TPS connectors.

4. Loosen M8 bolts, then remove throttle body from intake manifold.
5. Gently move throttle body away to detach throttle cable.
6. Remove throttle body cover.
7. Detach throttle cable.
Throttle Body (ETC) Installation

Installation of the throttle body is the reverse of the removal procedure. However, pay attention for the following details.

1. Properly install cable barrel to throttle cable end.
2. Do not reinstall cover yet.
3. Install throttle body on intake manifold.
4. Install throttle body to handlebar.
5. Depress throttle lever several times to ensure it properly returns.

6. Perform the THROTTLE POSITION SENSOR INITIALIZATION reset procedure.     Refer to THROTTLE POSITION SENSOR (TPS) in this subsection.

7. Install all remaining removed parts, refer to applicable subsections.

8. Start engine and ensure proper idle and throttle control.
THROTTLE POSITION SENSOR(TPS)

TPS Description

NOTE: The TPS is part of the throttle body (ETC).

The throttle position sensor (TPS) is a double potentiometer that sends signals to the ECU that are proportional to the throttle plate angle.

NOTE: As a first troubleshooting step, always check for applicable fault codes using Diagnostic Tool.

Throttle Position Sensor Initialization

NOTE: The TPS initialization procedure must be carried out whenever the throttle body (ETC) is replaced, unless an ECU first initialization reset is carried out.

This operation performs a reset of the TPS basic values in the ECU. This reset is very important as the TPS values are part of the basic parameters for all fuel mapping calculations and control of several settings such as for idle speed and maximum RPM of the engine.

NOTICE: An improperly set TPS may lead to improper idle speed (too low or too high), poor engine performance, poor engine starting and engine stop on deceleration, fault codes and possible engine damage. Emission compliance may also be affected.

1. Connect Diagnostic Tool to OBD.
2. In Diagnostic Tool, select the following:

- Read Data button

- Setting tab

- ECU tab.

3. Ensure the throttle lever is fully released and at the idle position.

4. In the Throttle position sensor initialization field, click on the Throttle Opening Reset button.

A message will be displayed if the operation is successful.

If an error occurred or the TPS is not within the allowed range while resetting, the ECU will generate a fault code and will not accept the setting.

5. If a fault message is displayed, follow the instructions in the message(s).

6. Check for fault codes.

7. If a fault code is generated,

- Carry out the service actions.

- Reset the fault.

- Repeat the reset procedure.

8. Start engine and make sure it operates normally throughout its full engine RPM range.
TPS Wear Test

1. With the engine turned off, slowly press on the throttle lever and pay attention for smooth operation without physical stops.

2. Activate the electrical system to wake up the ECU.

3. Connect Diagnostic Tool to OBD.
4. In Diagnostic Tool, select the following:

- Monitoring tab

- ECU tab.

5. Slowly and regularly move the throttle lever.

6. Observe the Throttle Opening indication movement in Diagnostic Tool.

NOTE: The indication should move gradually and regularly as you move the throttle lever. If the TPS indication is erratic or suddenly drops off, it may indicate a worn TPS that needs to be replaced. An initial slight delay after the throttle lever is moved and before the indication starts to move is normal.

If the indication behavior is not as expected, proceed with the following steps.

7. Manually move the throttle plate in the throttle body using a blunt tool (without sharp tip).

CAUTION: Do not move throttle plate with your fingers. Otherwise, if ECU should turn off, it would quickly close the throttle plate which could cause finger injury.
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1. Push here
8. Check the indication movement again.

- If the indication moves as expected, check the throttle accelerator sensor (TAS). Refer to THROTTLE ACCELERATOR SENSOR (TAS) in this subsection.

- If the indication does not move as expected, perform the TPS RESISTANCE TEST in this subsection.
TPS Voltage Test
Check the ECU voltage output to the TPS.
Disconnect connector from TPS.
Turn ignition key ON and set engine stop switch to RUN.
Check the voltage reading from harness connector as following.
	Connection
	Voltage

	Pin A with battery ground
	5.0V

	Pin B with battery ground
	0 V

	Pin C with battery ground
	4.75~ 5V


If voltage test is not good, check/repair wiring harness. If wiring test good, refer to ECU REPALCEMENT.
If voltage test is good, everything is order(assuming resistance test was performanced).
Replacement
Remove throttle body. Refer to this section.
Loosen two screws retaining TPS.
Remove TPS.
Install the new TPS.
Apply Loctite 243 on the TPS retainscrews, then torque to 9 Nm.
Reinstall remaining removed parts.
CRANKSHAFT POSITION SENSOR (CPS)

CPS TROUBLESHOOTING

When troubleshooting a CPS fault, take into account that a CPS fault can be triggered by bent or missing encoder wheel teeth.

Push START/STOP switch and crank engine. If engine does not start within 15 seconds check for fault codes using Diagnostic Tool.

CPS Access

1. Remove both side body panels, refer to BODY subsection.

2. Remove air filter refer to AIR INTAKE SYSTEM subsection.

3. Remove muffler, refer to EXHAUST SYSTEM subsection.

CPS Resistance Test at ECU connector

1. Remove parts required to access ECU connector, refer to ECU CONNECTOR ACCESS.
2. Disconnect ECU connector from ECU.
3. Set multimeter to Ω.

4. Measure the resistance of the sensor as per following table.
	ECU
	READING

	PIN
	Ω@ 20℃ (68℉)

	42
	43
	775 - 950 Ω


If resistance is as specified, test continuity of wiring between ECU and CPS connectors. Refer to WIRES DIAGRAM subsection.

If resistance value is not as specified, reconnect ECU connector to the ECU and refer to CPS RESISTANCE TEST AT CPS CONNECTOR.

CPS Resistance Test at CPS Connector

1. Cut locking tie securing CPS connector to ECU support and disconnect CPS connector.

2. Probe CPS connector terminals as per following table.
	CPS
	READING

	PIN
	Ω@ 20℃ (68℉)

	1
	2
	775 - 950 Ω


If resistance is not within specifications, replace the CPS.

If resistance tests good, carry out a CPS OUTPUT VOLTAGE TEST.
CPS Output Voltage Test

1. Remove fuse.
2. Cut locking tie securing CPS connector to ECU support and disconnect the CPS connector.
3. Probe CPS connector terminals while cranking engine as per following table.

	CPS
	READING

	PIN
	VOLTAGE

	1
	2
	1 - 2 Vac min.


If voltage is out of specification, inspect wiring/connectors. Replace CPS if wiring is good.

If voltage is within specification, the problem may be related to the ECU.

4. Reconnect CPS connector and install all removed parts.

CPS Replacement

1. Remove parts required to access the CPS, refer to CPS ACCESS in this subsection.

2. Take note of factory CPS wire harness routing for re installation.

3. Cut harness locking ties and disconnect CPS connector.

4. Remove CPS retaining screw and pull on CPS to remove it.

5. Install new CPS.
	CPS INSTALLATION

	O-RING
	SERVICE PRODUCT

	
	APPLY ENGINE OIL ON O-RING

	RETAINING

SCREW
	TORQUE

	
	9~12Nm


6. Route and secure CPS harness using harness clamp and locking ties as noted prior to removal.

MANIFOLD ABSOLUTE PRESSURE AND TEMPERATURE SENSOR (MAPTS)

NOTE: This sensor is a multifunction device. It measures manifold absolute pressure and intake temperature for air flow calculations.

MAPTS Access

To access the MAPTS, remove the LH side panel, air filter housing.
MAPTS Pressure Function

Before the engine is started, when power is applied to the system, the sensor measures the ambient air atmospheric pressure. The ambient pressure is, at that moment, stored in the ECU.

Thereafter, once the engine is started, it measures the air pressure in the intake manifold at operating RPMs.

The sensor must be correctly installed on the intake manifold. Otherwise, the MAPTS could generate a fault code for an unexpected sensor range at idle when it reads the atmospheric pressure. If this is the case, remove sensor and check for oil or dirt on its end and if problem persists, check throttle plate condition/position and the wiring harness. Perform the following tests.

MAPTS Quick Test (Pressure Function)

1. Connect Diagnostic Tool to OBD.
2. In Diagnostic Tool, select the following:

- Read Data

- Monitoring page tab

- ECU page.

3. Look for and take note of the MAPTS pressure reading while the engine is stopped.

NOTE: The indicated intake air pressure in Diagnostic Tool must be within 3.4kPa (0.5PSI) of local atmospheric pressure when the engine is stopped.

	MAPTS PRESSURE FUNCTION QUICK TEST

	RESULT
	SERVICE ACTION

	NO

READING
	Circuit

Continuity

Test of

MAPTS

Pressure
Function
	MAPTS

Input

Voltage
Test
	Repair
or replace wiring

	VALUE IS
OUT OF
RANGE
	Replace MAPTS


4. Perform the same test with a new MAPTS and compare both readings.

MAPTS Input Voltage Test

1. Remove parts required to access the MAPTS, refer to MAPTS ACCESS.

2. Remove electrical connector from MAPTS.

3. Briefly push START/STOP switch.

4. Set multimeter to Vdc, measure for MAPTS input voltage as per following table.
	MAPTS
	READING

	PIN
	VOLTAGE

	A
	D
	5 Vdc


If voltage test is good, replace the MAPTS.

If voltage test is not good, carry out the MAPTS CIRCUIT CONTINUITY TEST (PRESSURE FUNCTION).

MAPTS Circuit Continuity Test (Pressure Function)

1. Remove parts required to access ECU connectors, refer to ECU CONNECTOR ACCESS in this subsection.

2. Disconnect the ECU connector from the ECU.

3. Set multimeter to Ω and check continuity of the following circuits.
	ECU
	MAPTS
	READING

	PIN
	Ω

	Pin 9
	A
	Close to 0 Ω

	Pin 30
	B
	

	Pin 11
	C
	


If resistance is not within specification, repair or replace the wiring harness between ECU connector and the MAPTS. Refer to WIRES DIAGRAM.

MAPTS Temperature Function

The MAPTS also monitors the temperature of the air in the intake manifold.

MAPTS Quick Test (Temperature Function)

1. Connect Diagnostic Tool to OBD.
2. In Diagnostic Tool, select the following:

- Read Data

- Monitoring page tab

- ECU page.

3. Look for the Intake Air temperature reading while the engine is stopped.

NOTE: If the complete vehicle is at room temperature, Diagnostic Tool should display the ambient air temperature at the intake manifold.

4. Perform the same test with a new MAPTS and compare both readings.

If the engine's MAPTS temperature reading is significantly different than the new MAPTS, replace it.

NOTE: Both sensors must feel same ambient air temperature.

If there is no reading, carry out a MAPTS RESISTANCE TEST (TEMPERATURE FUNCTION).

MAPTS Resistance Test (Temperature Function)

1. Disconnect the MAPTS connector.

2. Test MAPTS resistance at the sensor as per following tables.

	MAPTS
	READING

	PIN
	Ω

	A
	D
	Refer to MAPTS

TEMPERATURE SENSOR TABLE


	MAPTS TEMPERATURE SENSOR TABLE

	TEMPERATURE
	Ω

	℃
	℉
	MAPTS

	- 40
	- 40
	40528 to 56935

	- 10
	- 14
	8103 to 10919

	20
	68
	2193 to 2863

	80
	176
	294 to 368

	120
	248
	98 to 122


If resistance is not within specification, replace the MAPTS.

If resistance tests good, reconnect the MAPTS and proceed with the following steps.

3. Using a multimeter, recheck resistance value as per following table.
	ECU
	READING

	PIN
	Ω

	Pin 9
	Pin 10
	Refer to MAPTS TEMPERATURE SENSOR TABLE


	MAPTS TEMPERATURE SENSOR TEST RESULTS

	RESULT
	SERVICE ACTION

	NO

READING
	Circuit

Continuity

Test of

MAPTS

Temperature Function
	MAPTS

Input

Voltage Test
	Repair or replace wiring

	INCORRECTRESISTANCEVALUE
	Check condition of connector pins, replace MAPTS

	CORRECT

RESISTANCEVALUE
	Try a new ECU


MAPTS Circuit Continuity Test (Temperature Function)

	ECU
	MAPTS
	READING

	PIN
	Ω

	Pin 9
	A
	Close to 0Ω

	Pin 10
	D
	


Repair or replace wiring as required.

MAPTS Replacement

1. Disconnect MAPTS connector and remove the MAPTS from the intake manifold.
2. Install new MAPTS as per following table.

	MAPTS Retaining Screw

	Tightening torque
	9 ~12 Nm


COOLANT TEMPERATURE SENSOR (CTS)

Overheat Warning

The CTS will cause the engine overheat warning to come on when the coolant temperature is above 110℃ (230°F).

CTS Access

The CTS is located on the RH side of the engine, between the water pump and oil cooler.

To access the CTS, remove the RH side panel.

CTS Quick Test

1. Connect Diagnostic Tool to OBD.
2. In Diagnostic Tool, select the following:

- Read Data button

- Monitoring page tab

- ECU page.

3. Look for the engine temperature indication.

The engine temperature gauge in Diagnostic Tool should provide an indication of the actual engine coolant temperature. Otherwise, perform the CTS RESISTANCE TEST.

CTS Resistance Test

1. Disconnect the CTS connector.

2. Test the resistance of the sensor as per following tables.

	CTS
	READING

	Wires color
	Refer to CTS

TEMPERATURE SENSOR TABLE

	Green
	Brown/Green
	


	CTS TEMPERATURE SENSOR TABLE

	TEMPERATURE
	Ω

	℃
	LOW
	HIGH

	- 40
	47423
	56157

	- 10
	8260
	10,560

	0
	5423.5
	6119.8

	20
	2280
	2720

	80
	290
	350

	100
	170
	210


NOTE: To test sensor at various temperatures, remove sensor and use a heat gun, ice and a thermometer.

If resistance is out of specification, replace the CTS.

If resistance test is good, proceed with the following steps.

3. Reconnect the CTS connector.

4. Remove parts required to access ECU connectors, refer to ECU CONNECTOR ACCESS in this subsection.

5. Recheck resistance from the ECU connector as per following table.
	ECU
	READING

	PIN
	Refer to CTS

TEMPERATURE SENSOR TABLE

	Pin1
(Green/black)
	Pin 9（Black）
	


If resistance value is correct, refer to ECU REPLACEMENT.

If resistance value is incorrect, repair the connectors or replace the wiring harness between ECU connector and the CTS.

CTS Replacement

1. Drain coolant, refer to PERIODIC MAINTNENANCE PROCEDURES subsection.

2. Cut locking ties of wiring harnesses and move wiring aside for access.

NOTE: Take note of wiring and locking tie position before removal.

3. Disconnect CTS connector.

4. Remove CTS from engine.

5. Install new CTS and torque as specified.

	CTS

	Tightening torque
	16 Nm ± 2 Nm

(142 lbf.in±18 lbf.in)


6. Reinstall remaining removed parts.

NOTE: Ensure to re install wiring harness as noted prior to removal.

7. Refill and bleed the cooling system, refer to PERIODIC MAINTENANCE PROCEDURES subsection.

6.AIR INTAKE AND EXHAUST SYSTEM
	CVT AIR INTAKE AAND EXHAUST SYSTEM
6-3
	AIR INTAKE SYSTEM
6-3

	EXHAUST SYSTEM
6-5
	


CVT AIR INTAKE AND EXHAUST SYSTEM
Ordinary Version
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	1. Front CVT Air Intake Pipe
	2. CVT Air Intake Pipe Joint
	3. Rear CVT Air Intake Pipe
	4. Rear CVT Air Exhaust Pipe
	5. Front CVT Air Exhaust Pipe

	6. M6 Bolt
	7. Clamp
	
	
	


MUD Version
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	1. Front CVT Air Intake Pipe
	2. CVT Air Intake Pipe Joint
	3. Rear CVT Air Intake Pipe
	4. Rear CVT Air Exhaust Pipe
	5. Front CVT Air Exhaust Pipe

	6. M6 Bolt
	7. Clamp
	8. CVT Air Exhaust Pipe Join
	9. Front Section of Front CVT Air Exhaust Pipe
	10. Hose Clamp

	11. CVT Air Exhaust Pipe Connection Bracket
	
	
	


AIR INTAKE SYSTEM (Ordinary Version)
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	1. Air Filter Asse.
	2. Air Filter Exhaust Pipe
	3. Clamp
	4. Air Filter Intake Pipe 1
	5. Air Filter Intake Pipe 2

	6. Air Filter Intake Pipe 3
	7. Clamp
	8. M6 Bolt
	9. M8 Bolt
	10. Air Filter


AIR INTAKE SYSTEM (Ordinary Version)
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	1. Air Filter Asse.
	2. Air Filter Exhaust Pipe
	3. Clamp
	4. Air Filter Intake Pipe 1
	5. Air Filter Intake Pipe 

	6. Air Filter
	7. Clamp
	8. M6 Bolt
	9. M6 Bolt
	


6.1 CVT AIR INTAKE AND EXHAUST SYSTEM
GENERAL
Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e.g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




CVT air intake pipe 

Ordinary Version

1. Remove seat.

2. Remove dash board cover.
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1. Dash board cover

2. Air filter service cover
3. Remove front plastic.
4. Loosen the clamps of the CVT air intake pipe combination at one time. 
5. Remove CVT air intake pipe. 

MUD Version

1. Remove seat.

2. Remove air intake filter and base.

3. Remove air intake mount and top-mount air intake grille.
3. Remove center front plastic component.
4. Loosen the clamps of the CVT air intake pipe combination at one time. 
5. Remove CVT air intake pipe. 
Cleaning
Operators must take necessary protective measures, and wear glasses and masks.
Operation work needs to be in open area.
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1. CVT air filter intake pipe.

2. Blow pipe

Please don’t clean the air intake pipe against the wind, otherwise stuffs will enter into eyes and mouth easily.

Clean the air intake pipe, and make sure there is no other stuffs around.

CVT outlet pipe combination 

Remove the bolts and loosen the clamps. Then the relevant components of outlet pipe combination can be maintained.

Available overhaul: replace CVT air outlet pipe combination. 

Tightening torque of M6 bolts for clamp: 9~12 Nm.
6.2 AIR INTAKE SYSTEM
Air Filter Maintenance Guideline
As with any ATV, air filter maintenance is critical to ensure proper engine performance and life span.

Air filter maintenance should be adjusted according to riding conditions.

Air filter maintenance must be increased in frequency and oil must be added to the foam filter element for the following dusty conditions:

- Riding on dry sand.
- Riding on dry dirt covered surfaces.
- Riding on dry gravel roads or similar conditions.
- Riding in severe snow conditions.
- Riding in areas with high concentration of seeds crop husks.
NOTICE: When riding in dusty conditions or sands, the air box needs to be cleaned before every ride.
NOTE: Riding in a group, under these conditions, increase the frequency of the air filter maintenance.
Air Filter Removal 
NOTICE: Never remove or modify any component in the air filter housing. Otherwise, engine performance degradation or damage can occur. The engine is calibrated to operate specifically with these components.
Remove seat.

Remove dash board cover.

Remove air filter service cover.
[image: image190.png]



1. Air filter service cover

Loosen M6 screws, the remove the air filter housing cover.
Loosen the clamps and then carefully pull air filter out of the air filter housing.
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1. Air filter 

2. Clamp
Air Filter Cleaning and Oiling

CAUTION: Always wear appropriate skin and eye protection. Chemicals can cause a skin rash and eye injury.
NOTE: If vehicle is used in dusty area, inspect more frequently than specified in MAINTENANCE CHART.
Paper Filter Cleaning

1. Ensure that the foam filter element removed from paper filter.

2. Tap out heavy dust from the paper      element.

This will allow dirt and dust to get out of the paper filter.

NOTE: Paper filter has a limited lifespan; replace filter if too dirty or clogged.

NOTE: It is not recommended to blow compressed air on the paper filter; this could damage the paper fibers and reduce its filtration ability when used in dusty environments. If air filter is very dirty and cannot be cleaned following the recommended procedure, it should be replaced.
NOTE: Do not wash the paper filter with any cleaning solution.

Foam Filter Element Cleaning
1. Spray the foam filter element inside and out with a good air filter cleaner and follow manufacturer's instructions.
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2. Dry the foam element completely.
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NOTE: A second application may be necessary for heavily soiled elements.
CAUTION: Do not atart engine if liquip or deposit are found. If there is oil in the air filter housing, check engine oil level. Oil level may be too high.
Air Filter Installation

Put the air filter into the air filter housing. 
Tighten the M6 screws for air filter cover to torque: 9~12 Nm.
Drying the Air Filter Housing After Submersion

If water has been ingested into the air filter housing, drain the air filter housing, remove the air filter, and thoroughly dry the components. Do not use compressed air. Contact your authorized dealer if vehicle performance issues exist.

CUATION: Do not operate the engine without an air filter element. Unfiltered air will enter into the engine and cause engine wear and damage. Driving without an air filter will also decrease performance and can lead to engine overheating.

CUATION: Major engine damage can result if the vehicle if water has been ingested into the air filter housing, and engine. Have the vehicle serviced by your dealer promptly if your vehicle becomes immersed or stalls in water that exceeds the footrest level. It is important to contact your dealer for service before starting the engine, as water may have been ingested in the air filter box and engine.
Inspecting the Engine Air Filter Housing
Check air filter housing dirty chamber for cleanliness.
-If any debris or water are found, clean air filter housing chamber using a vacuum cleaner.
NOTICE: Do not blow compressed air into air filter housing chamber.
6.3 EXHAUST SYSTEM
Structure 
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Names of components: 

	1. Front Cylinder Exhaust Pipe
	2. Locking Nut
	3. Exhaust gasket

	4. Rear Exhaust Pipe
	5. Muffler
	6. M8 Hex Flange Bolt

	7. O2 sensor
	8. Spring
	9. Front Exhaust Pipe Insulation Board

	10. Rear Cylinder Exhaust Pipe Insulation Board-1
	11. Rear Cylinder Exhaust Pipe Insulation Board-2
	12. Rear Cylinder Exhaust Pipe Insulation Board-3

	13. Rear Cylinder Exhaust Pipe Insulation Board-4
	14. Rear Cylinder Exhaust Pipe Insulation Board-5
	15. Rear Cylinder Exhaust Pipe Insulation Board-6

	16. M6 Hex Flange Bolt
	17. Graphite Seal Cartridge
	18. Graphite Seal Cartridge

	19. Muffler Hang Neck Bushing
	20. Muffler Hang Rubber Sleeve
	21. Muffler Top Cushion


GENERAL
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WARNING

	To avoid potential burns, never touch exhaust system components immediately after the engine has been run because these components very hot. Let engine and exhaust system cool down before performing any servicing.



Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e.g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




PROCEDURES
Removal
Remove RH side panels.

Separate the O2 sensor from the front exhaust pipe and the rear exhaust pipe, and then separate the O2 sensor from the connector of the main cable.
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Remove the exhaust pipe insulation board as shown on the right, 23 bolts in total.
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Tightening bolt torque of exhaust pipe insulation board: 9~12Nm.

First remove the tension springs on the hook (remove all four springs at the rear exhaust pipe at the same time), then remove the two bolts at the upper end of the muffler, finally remove the muffler and graphite seal gasket according to the direction of the arrow.
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And then, loose the cover of the rear exhaust pipe, then remove the two M8 lock nuts of the rear exhaust pipe, and finally remove the rear exhaust pipe from the vehicle.

Finally, remove the two M8 locking nuts of the front exhaust pipe and remove the front exhaust pipe from the vehicle.
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Tightening bolt torque of cylinder exhaust pipe: 22~30 Nm.

Remove the three heat insulation plates on the inside of the exhaust pipe, M6 bolts.

Remove muffler trim cover, total four M6 bolts. Remove three countersunk allen screws on muffler tail cover.
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Inspection
Check front exhaust pipe for cracks, bending or other damages. Replace if necessary.
Check muffler/insulation board for cracks or other damages. Replace if necessary.
Check rubber sleeve condition. If hard, brittle or damaged, replace it.
Check neck bushing condition. If crack or damaged, replace it.
Installation 

Conduct reinstallation based on the reversed sequence of dismantling. 
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WARNING

	After dismantling muffler, seal gasket of exhaust pipe should not be used repeatedly; new component should be used upon installation.

To prevent exhaust pipe leakage, high polymer sealant should be applied to cylinder exhaust pipe port and surface of exhaust pipe seal gasket upon muffler assembly installation.


Cleaning the Exhaust System
CAUTION: Never perform this operation immediately after the engine has been running because exhaust system is very hot.
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WARNING

	Debris accumulation could lead to a vehicle fire when the exhaust system is hot and the debris are dried.

In some cases, that could result in serious properly damages, injuries or even death.

Clean often and regularly the area surrounding the exhaust system when riding in swamp, bog, hay or dead leaves.

In other situations, clean as per maintenance schedule requirement.

Also, check all exhaust heat shields for damage regularly and replaced when needed.


1. From the rear of the vehicle, clean the areas around the muffler.

2. Clean the areas around the exhaust pipe and the exhaust manifold.
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WARNING

	Clean also under the heat shields.


Inspection and Cleaning the Muffler Spark Arrester
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TYICAL- REMOVE TAIL PIPE

CAUTION: Never perform this operation immediately after the engine has been running because exhaust system is very hot.

1. Remove exhaust tail pipe, gasket (discard) and spark arrester.
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1. Spark arrester

2. Gasket

3. Exhaust tail pipe

2. Remove carbon deposits from the spark arrester using a soft metallic brush.

NOTICE: Be careful to avoid damaging spark arrester mesh.

CAUTION: Wear eye protection and gloves.

3. Inspect mesh of spark arrester for any damage. Replace as required.

NOTE: Spark arrester mesh replacement is required only when damaged. 

4. Inspect spark arrester chamber in muffler. Clean any debris as required

5. Install new gasket, tail pipe and new retaining screws.

6. Reinstall muffler cover with new retaining screws. Tighten to torque: 22±2 Nm (16.2±1.5 lbf-in).

7.DRIVETRAIN
	FRONT DRIVE
7-2
	REAR DRIVE
 7-7
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	1. Front Differential
	2. Cotter Pin
	3. M10 Bolt
	4. M10 Bolt
	5. M10 Nut

	6. Front Transmission Shaft
	7. M10 Screw
	8. Rear Differential
	9. Rear Reducer Breath Tube
	10. Front Transmission Shaft

	11. Front Tire
	12. Front Rim
	13. Front Wheel-Hub
	14. RH Rear C.V. Shaft
	15. Front Brake Disc

	16. T Bolt M8 
	17. M10 Bolt
	18. Rear Tire
	19. Rear Rim
	20. Rear Brake Disc

	21. Wheel Dust-Proof Cover
	22. Air Valve
	23. Front C.V. Shaft
	24. LH Rear C.V. Shaft
	


7.1 FRONT DRIVE
GENERAL

The procedure explains blow is the same for the RH and LH side unless other instructed.

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e.g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




PROCEDURES
TIRES AND WHEELS
Tire thread
When the tire groove decreases to 3 mm (0.12 in) due to wear, replace the tire.
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WARNING

	When the tires are replaced, never install a bias tire with a redial tire. such a combination could create handling and/or stability problems.

Dot mix tires of different size and/or design on the same axle.

Front and rear tire pairs must be the identical model and manufacturer.

For unidirectional tread pattern, ensure that the tires are installed in the correct direction of rotation.

The radial tires must be installed as a complete set.

In dismantling tires, use special crowbar and rim protection device.


Tire replacement

Use jack to support vehicle and ensure its no dropping.
Remove four M10 nuts, pull along axial direction and remove front wheel combination.

Tightening torque of front wheel nut: 70~80Nm.
After removing the air valve cap, release the tire pressure by depressing the valve.

Dismount the bead from the rim completely.
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Separate the tire from the rim by using a set of tire levers and rim protectors.
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CAUTION: When using the tire lever, do not scratch or hit the sealing portion of the wheel or it may cause air leakage.

Apply tire lubricant to the new tire bead and the flange of the rim. But never apply grease, oil or gasoline to the tire bead because they will deteriorate the tire.
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CAUTION: The standard tire fitted on this vehicle is AT25x8-12 for the front and AT25x10-12 for the rear.

The use of tires other than the standard may cause instability. It is highly recommended to use the specified tire.

Inspect the sealing portion of the rim for contamination and distortion before installing the tire on the rim.
Mount the new tire on the rim. [image: image456.png]



CAUTION: When installing each tire, make sure the arrow on the tire points in the direction of rotation. Also make sure the outer side of the wheel rim is facing outward.
Inflate the tire to seat the tire bead.
Check the rim line cast on the tire side walls. It must 
be equidistant from the wheel rim all the way around. If the distance between the rim line and the wheel rim varies this indicates that the bead is not properly seated. If this is so, deflate the tire completely, and unseat the tire bead on bosh sides. Then coat the bead with clean water and re-seat the tire.

Adjust the tire pressure to specification.
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	Front wheel
	Rear wheel

	Tires pressure
	45kPa(6.5 psi)
	45kPa(6.5 psi)

	Dimension of tire 
	25x8-12
	25×10~12


WHEEL HUB
Removal
Raise the front of vehicle, support it securely on jack stands and remove front wheel.
Apply parking brake or select 4WD position and place shift lever on P position.
 SHAPE  \* MERGEFORMAT 


Remove:
- Cotter pin
- M20 Castle Nut
Remove two screws and brake oil pipe clip, separating front brake oil pipe on upper A-Arm.
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Remove the two M10 installing bolts of the left brake caliper and remove the caliper from the brake disc.
 SHAPE  \* MERGEFORMAT 



NOTE: During dismantling, brake action is prohibited to be conducted, avoiding brake friction plate close or placing spacer between friction plates to avoid friction plate close and to facilitate future installation.
Pull wheel-hub and brake disc out of the shaft.
Loosen M8 bolts to separate the wheel-hub and brake disc.
Inspection
Check wheel hub for cracks or other damages.
Check inner splines for wear or other damages.
If any damages are detected on wheel hub, replace it with a new one.
Installation

For installation, reverse the removal process but pay attention to the following.

Tighten the caste nut M20 on the drive shaft end to 280~300Nm and further tighten until one of its grooves is aligned with a cotter pin hole. Install a new cotter pin and the wheel cap. Fold one pin of cotter pin over drive shaft end.
Front C.V. Shaft

Removal

Remove the wheel and wheel hub, refer to this section.
Remove M10 blots and nuts, then separate the lower A-arms and steering knuckle.
Remove cotter pin and loosen the M12 castle nuts of the upper A-arms at first, then loosen the M10 castle nuts of the steering tie rod, finally take the steering knuckle out of the vehicle.
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Unscrew M10 bolt and nuts for left front shock absorber (one piece for each), separate left front shock absorber and front upper A-arm, and separate front upper A-arm and steering knuckle before removing left steering knuckle assembly along axial direction. 

Pull along axial direction and remove left front C.V. shaft. 

 SHAPE  \* MERGEFORMAT 



Inspection

Inspect the dust-proof sleeves. If there is any damage or evidence of leaking lubricant, replace them. 
Check splines for excessive wear. Replace if necessary. If the splines on plunging joint are worn, a check of differential inner splines should be done.

Check the stop ring at the end of front C.V. shaft. If wear is apparent, replace the stop ring.

Check if the bearing in steering knuckle moves freely and smoothly. If not, replace them.
Installation

Apply synthetic grease to the splines and insert the end of front C.V. shaft in front differential and pull joint a little to make sure that the stop ring is locked in differential side gear groove.
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1. Stop ring
Insert the other side of front C.V. shaft in the steering knuckle and install the knuckle to lower suspension arm. Install and torque the ball joint retaining bolts M10 to 45~59 Nm.
Tighten ball joint retaining bolts M10 to 45~59 Nm.
Tighten ball joint retaining bolts M12 to 78~104 Nm.
Install all other removed parts.
C.V.  Shaft Boot

Removal 
Remove:
- clamps from rubber boot using clamp pliers.
- large end of the boot from plunging joint or CV joint.
Clamp joint housing in a vise.
Align shaft with joint.
Pull hard on shaft to remove from joint.
Remove boot from drive shaft.
Remove and discard the circlip.
Inspection
Check steel ball in plunging joint or CV joint. If steel ball is hard to move, change plunging joint or CV joint.
Check circlip for damage, change as necessary.
Installation
For installation, reverse the removal procedure. Pay attention to the following details.
Insert the small clamp and the small end of boot on shaft.
Install the NEW circlip.
To insert shaft in joint:
- clamp joint in a vise with joint facing up
- center clamp on shaft
- carefully insert shaft into joint
- push hard to engage clamp
Pack steel ball area with grease.
NOTE: Do not use or add other grease.
Front Differential
Removal
Clean the drain plug area. Place an oil pan under the front differential, and then drain oil completely by removing the drain plug.
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Raise the front of vehicle, support it securely on jack stands and remove front wheel.
On both side, remove front C.V. shaft refer to this section.
Loosen M8 bolts, then separate front drive shaft and front differential.
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Loosen M10 bolts and nuts, then separate front differential and mounting bracket.
Disconnect the 2WD/4WD motor wires.

Remove the front differential out of frame from left side.
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Disassembly
Unscrew M10 bolts, then separate half housing.
NOTE: Be careful to keep the spacer shim on the each side of differential case.
- Extract differential case with driven bevel gear out of half housing.
- Unscrew M8 bolts, then separate driven bevel gear from differential case.
- Unscrew M8 bolts, then remove driving bevel gear from half differential housing.
- Unscrew M8 bolts, remove 2WD/4WD motor from half differential housing. Then remove shifting fork shaft, shifting fork, spline housing.

Inspection
Inspect the gear, differential, bearing, oil seals and dust seal for wear or damage. If any damage or wear is found, replace the oil seal or dust seal with a new one.

Check back lash and drag torque.

Check the breather rubber case for wear or damage. Also, check that the joint of rubber case fits tightly.

Assembly
Ring Gear Carrier/Ring Gear
To assemble, reverse the removal procedure. Pay attention to the following details.
Verify condition of half housing seal. Change seal if necessary.
Check all bearings and all oil seals. Change then if necessary.
Pinion Gear
To assemble, reverse the removal procedure. Pay attention to the following details.
Check O-ring for damage. If so, change it. Install the shim then the bearing.
Install the nut. Apply Loctite 277 on the threads nut then torque it to 180 Nm.
Installation

For installation, reverse the removal process but pay attention to the following.
Apply synthetic grease in the lips of new oil and install it.
Tightening M10 bolts torque for front differential: 65~78 Nm.
Tightening M8 bolts torque for front drive shaft: 22~30 Nm.

Front Drive Shaft
Removal
Remove:
- Front wheel

- LH front mud board
Remove the clamp that attach the front drive shaft bellows to front drive shaft. Discard the clamp.
Loosen M10 bolts, then remove front drive shaft.
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Inspection

Check:
- Splines for wear or damage
- If U-joint moves freely in all direction
- Bellows for holes or brittleness
Installation

For installation, reverse the removal process but pay attention to the following.

Tightening M10 bolts torque for front drive shaft: 45~59 Nm.
Front Drive Shaft U-joint
Removal
Remove internal snap ring from bearing caps.
Support inner yoke in vise and drive other yoke 
down with a soft hammer.

Support U-joint in vice and drive inner yoke down toremove remaining bearing caps.
Remove U-joint cross.
Installation

Install new U-joint cross in inner yoke. 
Install new bearing cap by hand.
NOTE: Carefully install U-joint cross with grease
fitting properly positioned.
Tighten vise to force bearing caps in.
Using a suitable tappet, fully seat bearing cap in 
one side. Continually, check for free movement of 
bearing cross as bearing caps are assembled.
Install snap ring.
Repeat procedure for other sides.
Grease U-joint, using a grease gun with synthetic grease.
7.2 REAR DRIVE

GENERAL

The procedure explains blow is the same for the RH and LH side unless other instructed.

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




PROCEDURES
WHEEL HUB
Removal
Raise the rear of vehicle, support it securely on jack stands and remove rear wheel.
Apply parking brake or select 4WD position and place shift lever on P position.
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Remove:
- Cotter pin
- M20 Castle Nut

Remove M6 screws and brake oil pipe clip, separating rear brake oil pipe on upper A-Arm.
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Remove the two M10 installing bolts of the brake caliper and remove the caliper from the disc brake disc.
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NOTE: During dismantling, brake action is prohibited to be conducted, avoiding brake friction plate close or placing spacer between friction plates to avoid friction plate close and to facilitate future installation.
Pull wheel-hub and brake disc out of the shaft.
Loosen M8 bolts to separate the wheel-hub and brake disc.
Inspection
Check wheel hub for cracks or other damages.
Check inner splines for wear or other damages.
If any damages are detected on wheel hub, replace it with a new one.
Installation

For installation, reverse the removal process but pay attention to the following.

Tighten the caste nut M20 on the drive shaft end to 280~300Nm and further tighten until one of its grooves is aligned with a cotter pin hole. Install a new cotter pin and the wheel cap. Fold one pin of cotter pin over drive shaft end.
Rear C.V. Shaft

Removal

Remove the wheel and wheel hub see above.
Remove the M10 nuts for the ball joint. Remove the M6 bolts on the sway bar. There are eight M6 bolts on the left and right sides. After the disassembly, take out the sway bar for maintenance.
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Remove the M10 bolts and nuts for the rear steering knuckle. Then remove the rear steering knuckle.
Remove the M10 bolts of the rear A-arm and take out the shock absorber.
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Pull along axial direction and remove rear C.V. shaft. 

 SHAPE  \* MERGEFORMAT 



Inspection

Inspect the dust-proof boots. If there is any damage or evidence of leaking lubricant, replace them. 
Check splines for excessive wear. Replace if necessary. If the splines on plunging joint are worn, a check of differential inner splines should be done.

Check the ring at the end of rear C.V. shaft. If wear is apparent, replace the wear ring.

Check if the bearing in steering knuckle moves freely and smoothly. If not, replace them.
Installation

Apply synthetic grease to the splines and insert the end of rear C.V. shaft in rear differential and pull joint a little to make sure that the stop ring is locked in differential side gear groove.
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1. Stop ring
The ring should be close to the differential.
Insert the other side of rear C.V. shaft in the steering knuckle and install the knuckle to lower suspension arm. Install and torque the ball joint retaining bolts M10 to 45~59 Nm.
Tighten ball joint retaining bolts M10 to 45~59 Nm.
Tighten ball joint retaining bolts M12 to 78~104 Nm.
Install all other removed parts.
C.V. Shaft Boot

Removal 
Remove:
-Clamps from rubber boot using pliers.
-large end of the boot from plunging joint or CV joint.
Clamp joint housing in a vise.
Align shaft with joint.
Pull hard on shaft to remove from joint.
Remove boot from drive shaft.
Remove and discard the circlip. A new one is included in the boot kit.
Inspection
Check steel ball in plunging joint or CV joint. If steel ball is hard to move, change plunging joint or CV joint.
Check circlip for damage, change as necessary.
Installation
For installation, reverse the removal procedure. Pay attention to the following details.
Insert the small clamp and the small end of boot on shaft.
Install the NEW circlip.
To insert shaft in joint:
- clamp joint in a vise with joint facing up
- center clamp on shaft
- carefully insert shaft into joint
- push hard to engage clamp
Pack steel ball area with grease.
NOTE: Do not use or add other grease.
Rear Differential
Removal
Clean the drain plug area. Place an oil pan under the rear differential, and then drain oil completely by removing the drain plug.
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Raise the rear of vehicle, support it securely on jack stands and remove rear wheel. 
On both side, remove rear C.V. shaft refer to this section.
Loosen M8 bolts, then separate rear drive shaft and rear differential.
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Disconnect the 2WD/4WD motor wires.
Remove the breather rubber hose.
Loosen M10 bolts and upper bracket from the frame, then remove rear differential.
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Disassembly
Unscrew M10 bolts, then separate half housing.
NOTE: Be careful to keep the spacer shim on the each side of differential case.
- Extract differential case with driven bevel gear out of half housing.
- Unscrew M8 bolts, then separate driven bevel gear from differential case.
- Unscrew M8 bolts, then remove driving bevel gear from half differential housing.
- Unscrew M8 bolts, remove 2WD/4WD motor from half differential housing. Then remove shifting fork shaft, shifting fork, spline housing.

Inspection
Inspect the gear case, case cover, bearing, oil seals and dust seal for wear or damage. If any damage or wear is found, replace the oil seal or dust seal with a new one.

Check the breather rubber case for wear or damage. Also, check that the joint of rubber case fits tightly.
Assembly 

Ring Gear Carrier/Ring Gear 

To assemble, reverse the removal procedure. Pay attention to the following details. 
Verify condition of half housing seal. Change seal if necessary. 
Check all bearings and all oil seals. Change then if necessary. 
Pinion Gear 

To assemble, reverse the removal procedure. Pay attention to the following details. 
Check O-ring for damage. If so, change it. Install the shim then the bearing. Install the nut. 
Apply Loctite 277 on the threads nut then torque it to 180 Nm. 
Apply synthetic grease in the lips of the new oil seal and install it.
Installation

For installation, reverse the removal process but pay attention to the following.
Tightening M10 bolts torque for rear differential: 65~78 Nm.
Tightening M8 bolts torque for rear drive shaft: 22~30 Nm.

Rear Drive Shaft

Removal
Remove
- Rear wheel

- RH foot plate

Remove the clamp that attach the front drive shaft bellows to front drive shaft. Discard the clamp.
Loosen M8 bolts, M10 bolts and nuts, then remove front drive shaft.
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Inspection

Check:
- Splines for wear or damage
- If U-joint moves freely in all direction
- Bellows for holes or brittleness
Installation

For installation, reverse the removal process but pay attention to the following.

Tightening M10 bolts torque for rear drive shaft: 45~59 Nm.
Rear Drive Shaft U-joint
Removal
Remove internal snap ring from bearing caps.
Support inner yoke in vice and drive other yoke 
down with a soft hammer.

Support U-joint in vice and drive inner yoke down to remove remaining bearing caps.
Remove U-joint cross.
Installation

Install new U-joint cross in inner yoke. 
Install new bearing cap by hand.
NOTE: Carefully install U-joint cross with grease
fitting properly positioned.
Tighten vise to force bearing caps in.
Using a suitable tappet, fully seat bearing cap in 
one side. Continually, check for free movement of 
bearing cross as bearing caps are assembled.
Install snap ring.
Repeat procedure for other sides.
Grease U-joint, using a grease gun with synthetic grease.
8. STEERING SYSTEM
	GENERAL
8-3
	PROCEDURES
 8-3

	ADJUSTMENT
8-5
	


STEERING SYSTEM(Without EPS)
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Names of components: 
	1.Handle Bar
	2.Combination Switch
	3. Accelerator
	4. LH Rear View Mirror
	5.RH Rear View Mirror,
	6. M6 Nut

	7.Handlebar Grip
	8. Hand Brake Lever
	9. Brake Lever Half Cover
	10. M6 Bolt
	11.Steering Column
	12.Bearing

	13.Steering Column Block
	14.O-ring
	15.Steering Column Block Bushing
	16.Upper Handlebar block
	17.Lower Handlebar block
	18.M8 Screw

	19.Bearing Seat Bracket
	20.Bearing Plate
	21.Steering Rocker Arm
	22.Castle Nut M12
	23.Cotter Pin
	24.M8 Bolt

	25.Washer
	26.Steering Tir Rod
	27. Castle Nut M10
	28.Cotter Pin
	29.Washer
	30. M8 Bolt

	31. M8 Bolt
	32.Washer
	33. M8 Bolt
	34.Throttle Cable
	35.Parking Cable
	36.Harness Clip


STEERING SYSTEM(With EPS)
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Names of components: 
	1. LH Handle Bar Cover
	2. RH Handle Bar Cover
	3. M6 Screw
	4. M6 Screw
	5.Steering Column
	6. EPS

	7.EPS Controller Bracket
	8.EPS Controller
	9.M8 Bolt
	10.M10 Bolt
	11. M6 Bolt
	12. Washer

	13.M8 Bolt
	14.RH Handle Bar Cover Reflective Stripe 
	15.LH Handle Bar Cover Reflective Stripe 
	16.Winch Control Mounting Board
	
	


GENERAL

The procedure explains blow is the same for the RH and LH side unless other instructed.

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.). If the efficiency if a locking device is impaired, it must be renewed.



PROCEDURES

HANDLEBAR GRIP
Removal
Loosen the screw at the end of handlebar grip.
Remove the handlebar grip cover.
Remove the handlebar grip.
Installation
Remove all rubber residues of the old grip before 
installing the new.
Clean the handlebar with pulley flange cleaner or 
alcohol to remove any greasy matter on it.
Install handlebar grip by blowing compressed air 
between handle grip and handlebar.
Install a tapered tip on a bottle of Loctite 406 (glue).
Lift a part of the grip using a small screwdriver and 
inject glue (about 4 spots per side).
NOTE: The glue dries quickly. Do not apply it 
before installing grip.
Apply pressure on the grip for approximately 30 seconds to set the glue.
Install the handlebar grip cap and torque screw 9~12 Nm.
HANDLEBAR COVER
Removal
Loosen M6 screws, then remove the handlebar cover from handlebar.

Inspection 
Check covers for cracks or other damages.

Installation
For installation, reverse the removal process.
HANDLEBAR
Removal
Remove:
- Handlebar grip and handlebar grip cover
- Handlebar cover
- Rearview mirror
- Front windshield
- Throttle and parking brake handles
- Multifunction switch, 2WD/4WD switch, winch switch and brake handles.
NOTE: Remove handlebar grips, throttle handle, brake handle and multifunction switch only if the   handlebar is defective and replace with a new.

Loosen four M8 screws, then remove upper handlebar block.
Remove handlebar.

Inspection
Inspect the handlebar for damage, cracks or 
bending, replace if any of these problems is 
detected.
Installation
For the installation, reverse the removal procedure.
STEERING COLUMN
Removal
Remove:
- LH front mud board
- Handlebar cover and handlebar

- LH front wheel

Steering System (With EPS)

1. Remove two M8 bolts, separating steering column block from steering column.

[image: image232.png]



1. Steering column block

2. Remove cotter pin and M10 castle nut (two pieces for each side), separating left and right steering tie rod from steering rocker arm. 

3. Remove four M10 bolts, cotter pin and M12 castle nut on the steering rocker arm, then lift along axial direction to remove steering column and EPS.

4. Remove M8 bolt and washer, sperate the EPS and steering column. 
5. Pull out steering column.
Steering System (Without EPS)

1. Remove two M8 bolts, separating steering column block from steering column.
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1. Steering column block

2. Remove cotter pin and M10 castle nut (two pieces for each side), separating left and right steering tie rod from steering rocker arm. 

3.  Remove M8 bolt and washer on the steering rocker arm, then lift along axial direction to remove steering column combination.
4. Remove the cotter pin and M12 castle nut, take out the rocker arm.

5. Loosen two M8 bolts, remove and separate bearing and bearing set plate.
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1. Bearing seat plate
2. Bearing plate
3. Bearing
4. M8 Bolt
6. Pull out steering column.
Inspection 
Check steering column for wear, crack or bending, replace if any of these problems is detected.

Check steering column bearing condition. It must turn smoothly and freely. If not, replace it.

Check the splines on steering column and rocker arm for wears, cracks or other damages.
Check the splines on EPS shaft for wears, cracks or other damages.
Installation

For installation, reverse the removal process but pay attention to the following.
Apply synthetic grease on O-ring on bushings.
Install new cotter pins. Both ends of cotter pins must be folds.

Place bearing plate outward.

Install bearing plate on the bearing seat plate. 
Tightening M8 bolts torque: 22~30 Nm.

Tightening M10 castle nut to torque: 45~59 Nm.

Tightening M12 castle nut torque: 78~104 Nm.
TIE ROD
NOTE: Use the same procedure for RH and LH side.
Removal
Place the vehicle on jack stands and remove the appropriate wheel.
Remove the cotter pin (discard it), M10 castle nut from steering rocker arm and steering knuckle.
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1. M10 Castle nut and cotter pin
2. Tie rod ball joint

Remove the tie rod.
Inspection

Check ball joint ends for wear or looseness, if excessive, replace.
Installation

For installation, reverse the removal process but pay attention to the following.
When installing a tie rod, screw threaded end of tie rod into ball joint.

Install new cotter pins. Both ends of cotter pins must be folds.
Tightening M10 castle nut for tie rod: 45~59 Nm.
STEERING KNUCKLE

Removal Front Steering Knuckle

Place the vehicle on jack stands and remove the appropriate wheel.
Remove the cotter pin (discard it) and M10 castle nut, separate the tie rod from steering knuckle.
Remove wheel hub and brake caliper.

Remove the cotter pin and unscrew the upper castle nut (M12), separate the upper A-arm ball joint from steering knuckle.
Using a hammer, hit on the knuckle tip to separate ball joint from knuckle. A ball joint remover can be
used if the ball joint is jammed into knuckle.
CAUTION: Never hit on upper suspension arm.
Permanent damages could be caused to arm and 
its replacement would be necessary.
Remove the cotter pin and unscrew the lower castle nut(M10), separate the lower A-arm ball joint from steering knuckle.
Remove steering knuckle.

Removal Rear Steering Knuckle

Place the vehicle on jack stands and remove the appropriate wheel.
Remove wheel hub and brake caliper.
Remove M10 bolts and nuts, separate the upper/lower ball joint from rear steering knuckle.
Remove rear steering knuckle.
Wheel Bearing
Remove steering knuckle.
Remove retaining ring (discard it).
Using bearing extractor to disassembly the bearing.
CAUTION: Clean all the grease, outside and inside from steering knuckle.
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Inspection
Check steering knuckle for cracks or other damages. Replace if necessary.
Check if wheel bearing turns freely and smoothly.
Check Nylon sleeve and bushing in the rear steering knuckle for cracks or other damages. Replace if worn.
Installation
The installation is the reverse of removal procedure.
Place the bearing in a freezer for 10 minutes beforeinstalling.
Place the knuckle in oven to 100℃ (212℉) for 30 minutes maximum to ease bearing installation.
When knuckle is cold, install the retaining ring.
Tightening M10 castle nut for tie rod: 45~59 Nm.
Tightening M12 castle nut: 78~104 Nm.
MULTIFUNCTION SWITCH
Test
Refer to Electric system.
Removal
Remove handlebar grip and cover.
Remove bolts.
Separate multifunction switch from handlebar.
Unscrew the screw and then remove winch switch.

Unplug the multifunction switch connector.
Installation
The installation is the reverse of removal procedure.
THROTTLE Handle
Test
Refer to Electric system.
Removal
Remove handlebar grip and cover.
Remove bolts.
Separate throttle lever from handlebar. 
Slide rubber protector back to expose throttle cable adjuster.
Loosen lock nut and screw in the throttle cable adjuster.
Remove inner housing protector.
Slide cable in clip slot and remove the end of the cable from clip.

Remove throttle cable from housing.

Unplug the 2WD/4WD switch connector.
Installation
The installation is the reverse of removal procedure.
HAND BRAKE
Removal
Remove handlebar grip and cover.
Remove screws.
Separate hand brake from handlebar
Installation
The installation is the reverse of removal procedure.
EPS Motor and EPS Controller (If equipped)
Removal
Remove:

- LH front mud board
- Handlebar cover and handlebar

- LH front wheel
1. Remove two M8 bolts, separating steering column block from steering column.

2. Remove cotter pin and M10 castle nut (two pieces for each side), separating left and right steering tie rod from steering rocker arm. 

3. Remove four M10 bolts and M8 bolt on the steering rocker arm, then lift along axial direction to remove steering column and EPS.

4. Remove M8 bolt and washer, disconnect the EPS motor connector, then sperate the EPS and steering column. 
5. Disconnet the EPS controller connectors.
6. Loosen M6 bolts and then remove EPS controller from bracket.
Test
Refer to Electric system.
Installation
The installation is the reverse of removal procedure.
ADJUSTMENT
STEERING ALIGNMENT

Keep handlebar in horizontal status on flat ground and check whether the handlebar is loose from four directions (top, bottom, left and right); tighten nut or dismantle steering column for further checking, if any. 

Park vehicle on flat ground and rotate handlebar leftwards and rightwards to check whether it is able to be rotated flexibly. If any stuck, check whether it is caused by installation of main wire ground or other wiring; if not, please check the bottom of steering bar to check whether steering column bearing is damaged.

Park vehicle on flat ground, make sure the tire pressure for right and left tires is same and set to the proper specification, set the front wheels in the straight position, then place a load of 75kg on the seat.
1. Mark both front tire tread centers.
2. Lift the front of vehicle to keep the front wheel from force.
3. Faster the steering forward. Measure the width A between the marks.
4. Rotate the front ties 180º until the marks are exactly oppostite one another.
5. Measure distance B between the marks.
6. Calculate the difference.  
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A: front of front wheel

B: rear of front wheel

Toe-in.: B-A= 5mm

7. If the toe-in is out of range, adjust nut of tie rod.
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CAUTION: After adjusting toe-in, fist rotate steering wheel from center position to the left and right, to ensure that is the same corner, then slowly run vehicle to see whether its direction can be controlled.
1. Mark both tie-rods ends. This reference points will be needed during adjusterment.
2. Loosen the locknut (tie-rod end) on  each tie-rod.
3. The same turns should be given to both the right and left tie-rod until the specified toe-in is obtained. 
4. Tighten the rod end locknut on each tie-rod to: 45~59 Nm.
9. SUSPENSION
	FRONT SUSPENSION
9-1
	REAR SUSPENSION
 9-4


9.1 FRONT SUSPENSION
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Names of components: 
	1. LH Front Upper A-Arm
	2. RH Front Upper A-Arm
	3. RH Front Lower A-Arm
	4. LH Front Lower A-Arm
	5. M10 Bolt
	6. M10 Nut

	7.Grease Zerk
	8. Nylon Sleeve Cover
	9. Nylon Sleeve
	10.Bushing
	11. Ball Joint
	12.Ring

	13. M10 Bolt
	14. Ball Joint
	15.M12 Castle Nut
	16. Cotter Pin
	17. Front Shock Absorber
	18. M10 Bolt

	19. M10 Nut
	20.RH Steering Knuckle
	21. LH Steering Knuckle
	22.Grease Zerk
	
	


GENERAL

The procedure explains blow is the same for the RH and LH side unless other instructed.

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




PROCEDURES

TIRES AND WHEELS
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WARNING

	When the tires are replaced, never install a bias tire with a radial tire. Such a combination could create handling and/ or stability problems.

Do not mix tires of different size and/ or design on the same axle.

Front and rear tire pairs must be the identical model and manufacturer.

For unidirectional tread pattern, ensure that the tires are installed in the correct direction of rotation.

The radial tires must be installed as a complete set.

Severe injury or death can result if these instructions are not followed.


The tires are directional and their rotation must be 
kept in a specific direction for proper operation.
SHOCK ABSORBER
Removal
Loosen wheel nut.
Lift front of vehicle until front shock absorber is fully extended then install a jack stand under the frame to support the vehicle off the ground.
Remove:
- Front wheel 
- M10 bolt and nuts
Remove shock absorber from vehicle.
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1. M10 bolt
2. M10 nut

Disassembly
1. Secure the spring compressor in a vise.
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2. Position the shock absorber in the tool and install the spring compressor hooks.
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1. Spring compressor hooks
3. Tighten the spring compressor tool screw until the spring is sufficiently compressed to remove spring stopper.
4. Release the spring compressor tool screw.
5. Remove spring from shock absorber.
Inspection 

Inspect spring for apparent damage, any defect such as scratches or rust can affect the spring durability.
When the adjustment is at the lowest preload, ensure that adjustment cam and spring stopper are not loose. They must be under spring pressure. Otherwise, the spring stopper might fall off.
Inspect the shock absorber for oil leakage or damage, inspect the bushing for wear or damage. If any damage is found, replace the front shock absorber with a new one.
Extend and compress the piston several times over its entire stroke. Check that it moves smoothly and with uniform resistance with rod up. Any of the following conditions will denote a defective shock:

- A skip or hang up when reversing stroke at mid-travel.

- Seizing or binding conditions except at extreme end of either stroke.

- A gurgling noise after completing one full compression and extension stroke.

Replace shock if any these conditions are found.

Assembly and Installation

For assembly and installation, reverse the disassembly and removal process.

LOWER SUSPENSION ARM PROTECTOR
Removal
Remove M6 screws then remove front C.V. shaft cover.
Inspection 

Check cover for cracks or damages. Replace if necessary.
Installation

For installation, reverse the removal process.

LOWER SUSPENSION ARM
Lubrication
Use suspension grease to lubricate both suspension arm. There are two grease zerk on each arm.
Removal 
Remove wheel.
Remove M6 screws then remove front C.V. shaft cover.
Remove the M10 bolt and nut, separate the lower suspension arm from steering knuckle.
Remove the M10 bolt and nut, separate the lower suspension arm from frame.
Remove the lower suspension arm from frame.
Inspection 

Inspect the suspension arm for cracks, pitting, distortion or other damage. If so, replace the suspension arm with a new one.

Move suspension arm from side to side. There should be no noticeable loose. Replace bushing if necessary.

Move suspension arm up and down. There should be no noticeable loose. Replace bushing if necessary.

The following items are performed when the lower suspension arm is removed.
Inspect the bushing and Nylon sleeve for wearing or damaged. Replace if necessary.
Check ball joint bellows on lower suspension arm for crack or damaged. Ensure it’s moving freely. Replace ball joints as required, see blew for procedure. 
Installation

For installation, reverse the removal process.
LOWER BALL JOINT
Inspection

Check ball joint bellows for crack or damaged. Replace as required.
Check ball joint for damage, pitting, looseness or roughness. If so, replace it. 
Removal 
Remove front wheel and steering knuckle from vehicle.
Remove the snap ring.
Using a press and a small piece of pipe, extract the ball joint. Support the knuckle properly to avoid damaging ball joint location.
Installation

For installation, reverse the removal process.

To install the ball joint properly, use the ball joint installer.
Support the knuckle before pressing the ball joint into its location.
Reinstall the snap ring. If it seems loose, replace it with a new one.
UPPER SUSPENSION ARM
Lubrication
Use suspension grease to lubricate both suspension arm. There are two grease zerk on each arm.
Removal 
Remove front wheel.
Remove screws and brake oil pipe clip, separating front brake oil pipe on upper A-Arm.
Remove the front shock absorber.

Remove the cotter pin and M12 castle nut.
Using a harmmer, hit on the knuckle tip to separate the ball joint and steering knuckle.
CAUTION: Never hit on upper suspension arm. Permanet damages could be caused on arm and its replacement will be nessary.

Remove the M10 bolt and nut, separate the upper suspension arm and frame.
Remove the upper suspension arm from frame.
Inspection 

Inspect the suspension arm for cracks, pitting, distortion or other damage. If so, replace the suspension arm with a new one.

Move suspension arm from side to side. There should be no noticeable loose. Replace bushing if necessary.

Move suspension arm up and down. There should be no noticeable loose. Replace bushing if necessary.

The following items are performed when the upper suspension arm is removed.
Inspect the bushing and Nylon sleeve for wearing or damaged. Replace if necessary.
Check ball joint bellows on upper suspension arm for crack or damaged. Ensure it’s moving freely. Replace ball joints as required, see blew for procedure.
Installation

For installation, reverse the removal process.
Positon the upper suspension arm and install its bolts.

Attach the upper suspension arm to steering knuckle. When retaining ring and castle nut are installed, tighten until one of its grooves is aligned with a cotter pin hole.

Install new cotter pins. Both ends of cotter pins must be folds.

Install the shock absorber lower bolt.
Install front wheel.
Tightening M10 nut : 45~59 Nm.
Tightening M12 castle nut :78~104 Nm.
UPPER BALL JOINT
Inspection

Check ball joint bellows for crack or damaged. Replace as required,
Check ball joint for damage, pitting, looseness or roughness. If so, replace it. 
Removal 
Remove upper suspension arm from vehicle.
Remove the snap ring.
Using a press and a small piece of pipe, extract the ball joint. Support the upper suspension arm properly to avoid damaging ball joint location.
Installation

For installation, reverse the removal process.

To install the ball joint properly, use the ball joint installer.
Support the upper suspension arm before pressing the ball joint into its location.
Reinstall the snap ring. If it seems loose, replace it with a new one.
Install the upper suspension arm.
9.2 REAR SUSPENSION
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Names of components: 
	1.Sway Bar
	2.Blance Bar Clamp
	3. M18 Bolt
	4. Grease Zerk
	5.Sway Bar Lining
	6.Ball Point

	7. RH Rear Upper A-Arm
	8. Ball Point
	9. M10 Nut
	10. RH Steering Knuckle
	11. LH Steering Knuckle
	12. Rear Shock Absorber

	13. M10 Bolt
	14. M10 Bolt
	15.LH Rear Lower A-Arm
	16. RH Rear Lower A-Arm
	17. M10 Bolt
	18. Nylon Sleeve Cover

	19. Nylon Sleeve
	20. Bushing
	21.LH Rear Upper A-Arm
	
	
	


GENERAL

The procedure explains blow is the same for the RH and LH side unless other instructed.

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




PROCEDURES

TIRES AND WHEELS
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WARNING

	When the tires are replaced, never install a bias tire with a radial tire. Such a combination could create handling and/ or stability problems.

Do not mix tires of different size and/ or design on the same axle.

Front and rear tire pairs must be the identical model and manufacturer.

For unidirectional tread pattern, ensure that the tires are installed in the correct direction of rotation.

The radial tires must be installed as a complete set.

Severe injury or death can result if these instructions are not followed.


The tires are directional and their rotation must be 
kept in a specific direction for proper operation.

SHOCK ABSORBER
Removal
Loosen wheel nut.
Lift rear of vehicle until rear shock absorber is fully extended then install a jack stand under the frame to support the vehicle off the ground.
Remove:
- Rear wheel 
- M10 bolt and nuts
Remove rear shock absorber from vehicle.
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Disassembly
1. Secure the spring compressor in a vise.
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Spring compressor
2. Position the shock absorber in the tool and install the spring compressor hooks.
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1. Spring compressor hooks
3. Tighten the spring compressor tool screw until the spring is sufficiently compressed to remove spring stopper.
4. Release the spring compressor tool screw.
5. Remove spring from shock absorber.
Inspection 

Inspect spring for apparent damage, any defect such as scratches or rust can affect the spring durability.
When the adjustment is at the lowest preload, ensure that adjustment cam and spring stopper are not loose. They must be under spring pressure. Otherwise, the spring stopper might fall off.
Inspect the shock absorber for oil leakage or damage, inspect the bushing for wear or damage. If any damage is found, replace the rear shock absorber with a new one.
Extend and compress the piston several times over its entire stroke. Check that it moves smoothly and with uniform resistance with rod up. Any of the following conditions will denote a defective shock:

- A skip or hang up when reversing stroke at mid-travel.

- Seizing or binding conditions except at extreme end of either stroke.

- A gurgling noise after completing one full compression and extension stroke.

Replace shock if any these conditions are found.

Assembly and Installation

For assembly and installation, reverse the disassembly and removal process.

STABILIZER BAR
Removal
Remove M10 nut, then separate the ball joint and rear lower suspension arm.
Remove four M8 bolts and clamps, then remove stabilizer bar from frame.
Inspection 

Remove the stabilizer bar from the frame and the rear swing arm. Check whether the lining of the stabilizer is powdered or cracked. If so, please replace it with a new lining.

Check the transverse stabilizer ball joint for damage, pitting, looseness, etc., and check the ball bellows for cracks, damage, powdering, etc. If so, please replace it with a new one.

Installation

For installation, reverse the removal process.
Use suspension grease to lubricate sway bar. There are two grease zerk on sway bar.
LOWER SUSPENSION ARM
Lubrication
Use suspension grease to lubricate both suspension arm. There are two grease zerk on each suspension arm.
Removal 
Remove rear wheel.
Remove the rear shock absorber.
Remove M10 nut, then separate the ball joint and rear lower suspension arm.
Remove the M10 bolt and nut, separate the lower suspension arm from steering knuckle.
Remove the M10 bolt and nut, separate the lower suspension arm from frame.
Remove the lower suspension arm from frame.
Inspection 

Inspect the suspension arm for cracks, pitting, distortion or other damage. If so, replace the suspension arm with a new one.
Move suspension arm from side to side. There should be no noticeable loose. Replace bushing if necessary.

Move suspension arm up and down. There should be no noticeable loose. Replace bushing if necessary.

The following items are performed when the lower suspension arm is removed.
Inspect the bushing and Nylon sleeve for wearing or damaged. Replace if necessary.
Installation

For installation, reverse the removal process.

UPPER SUSPENSION ARM
Lubrication
Use suspension grease to lubricate both suspension arm. There are two grease zerk on each suspension arm.
Removal 
Remove wheel.
Remove screws and brake oil pipe clip, separating front brake oil pipe and upper A-Arm.
Remove the M10 bolt and nut, separate the upper suspension arm and steering knuckle.
Remove the M10 bolt and nut, separate the upper suspension arm and frame.
Remove the upper suspension arm from frame.
Inspection 

Inspect the suspension arm for cracks, pitting, distortion or other damage. If so, replace the suspension arm with a new one.

Move suspension arm from side to side. There should be no noticeable loose. Replace bushing if necessary.

Move suspension arm up and down. There should be no noticeable loose. Replace bushing if necessary.

The following items are performed when the lower suspension arm is removed.
Inspect the bushing and Nylon sleeve for wearing or damaged. Replace if necessary.
Installation

For installation, reverse the removal process.

Tightening M10 nut : 45~59 Nm.
10. BRAKES
	GENERAL
10-1
	MAINTENACE
10-2

	PROCEDURES
10-3
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	1.Brake Assembly
	2.Hand Brake Master Cylinder
	3. M6 Bolt
	4. M8 Bolt

	5. M8 Bolt
	6. Brake Rod Of Master Cyliner
	7. M10 Bolt
	8. M10 Bolt

	9. Foot Brake Pedal
	10.Washer
	11.Snap Ring
	12. Double Clamp

	13. Clamp for brake oil pipe
	14. M6 Bolt
	15. M6 Nut
	16. Brake Cable Rubber Boot

	17. Brake Hose Clamp
	18.Front Brake Pad
	19. Rear Brake Pad
	20. Brake Master Cylinder

	21. LH Front Brake Caliper
	22. RH Front Brake Caliper
	23. LH Rear Brake Caliper
	24.RH Rear Brake Caliper

	25.Combination Braking System valve
	26. Rear Tee-junction
	27. Front Left Pump Hose
	28. Front Right Pump Hose

	29. Hand Brake Master Cylinder Hose
	30.Parking Brake Cable
	31. Foot Brake Front Master Cylinder Hose
	32. Rear Left Pump Hose

	33. RH Rear Pump Hose
	34. Brake Fluid Reservoir
	35. Foot Brake Front Master Cylinder Oil Pipe
	36. Front Brake Disc

	37. Rear Brake Disc
	38.Washer
	
	


GENERAL

The procedure explains blow is the same for the RH and LH side unless other instructed.

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.).




When storing brake fluid, seal the container completely and keep it away from children.

When replenishing brake fluid, take care not to get dust into fluid.

When washing brake components, use new brake fluid. Never use cleaning solvent.

A contaminated brake disc or brake pad reduces braking performance. Discard contaminated pads and clean the brake disc with high quality brake cleaner or neutral detergent.

CAUTION: Brake fluid may cause damage to surfaces of plastic and rubber parts. Keep it far away from these parts.
CAUTION: To avoid serious damage to the brake system, use only DOT4 brake fuild  from a sealed container. Do not use any brake fluid taken from old, used or unsealed containers. Never reuse brake fluid left over from the last servicing or which has been stored for a long period of time.

CAUTION: Sealing washers must be discarded and replaced with new ones  every time a fitting nut is unscrewed.
Hydraulic Brakes System

The brake system consists of two circuits. Each system has its own master cylinder and reservoir.
Both front and rear brakes are disc type.
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WARNING

	Periodically check the brake hoses for damages or leaks. Repair any damage before operating the vehicle.



Parking Brake
The parking brake operates all brakes. It is activated by a locking mechanism on LH brake lever.
MAINTENANCE
Brake Fluid
Recommended Brake Fluid
Always use brake fluid meeting the specification DOT 4 only.
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WARNING

	To avoid serious damage to the braking system, do not use fluids other than the recommended one, nor mix different fluids for topping up. 


Fuild Level
Place vehicle on a level surface, check brake fuild in reservoir for proper level. It should be above MIN. mark.
Clean filler cap before removing,.
Add fuild as required. Do not overfill.
NOTE: A low level may indicate leaks or worn brake pads.
Hand Brake Reservoir 

Before riding, check that the hand brake fluid is above the lowest level and replenish it if necessary.
Front brake fluid reservoir is located on left handlebar.
Place the ATV on a level surface.

Inspect the brake fluid level window and verify that fluid can be observed.
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1. Brake fluid level window
If brake fluid level cannot be observed in the window or it is too full, add or reduce the brake fluid appropriately.

Insufficient brake fluid can cause air to enter the brake system, potentially causing ineffective braking.

Foot Brake Reservoir 
Foot brake fluid cap is under the dash board cover. Place the vehicle on a level surface.

Remove the dash board cover, and then check the fluid level.
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If fluid level is lower than the “lower” mark, add DOT4 brake fluid until the between two level lines.
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Brake Fluid Replacement
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WARNING

	A contaminated brake disc or pad reduces stopping power. Discard contaminated pads and clean a contaminated disc with a high quality brake degreasing agent.


Brake Fluid Draining

Remove reservoir cover with its diaphragm.

Connect a clear hose to bleeding screw.

Loosen bleeding screw and pump brake lever or brake pedal until no more fluid flows out of bleeding screw.

Brake Fluid Filling and Bleeding
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WARNING

	Never store or use a partial bottle of brake fluid. Brake fluid is hygroscopic, meaning it rapidly absorbs moisture from the air. The moisture causes the drop of boiling temperature of the brake fluid, which can lead to early brake fade and the possibility of accident or severe injury. After opening a bottle of brake fluid, always discard any unused portion.


Close bleeding screws.

Fill reservoirs with DOT 4 brake fluid.

Unscrew the bleeding screw on the braking caliper until brake fluid comes out then close it.
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1. Rear master cylinder

2. Bleeding screw

On each caliper, unscrew the bleeding screw until the brake fluid comes out then close it.

Bleed system as per the following procedure.

With a Vacuum Pump

Using a clear hose, install the vacuum/pressure pump to bleeding screw. Place the pump in vacuum position. See the manufacturer's operating instructions.

Pump vacuum pump loosen bleed. Close bleed and refill reservoir when the fluid level is low.

NOTE: Check fluid level often to prevent air from being pumped into the system.

Repeat the procedure until no more air bubbles appear in hose.

NOTE: For the front brake system, switch to LHand RH caliper. Turn handlebar to full RH side when bleeding right caliper and turn to the LH side for the left caliper. This helps to reach air into the caliper. The front and the rear brakes must be bled at the same time.

Close bleeding screw and operate brake lever or brake pedal. If it still feels spongy, bleed system again.

Repeat the procedures until air bubbles do not appear in hose and lever or pedal is stiff.

Fill reservoirs to the upper level with DOT 4 brake fluid.

Install diaphragms and covers on brake fuild  reservoirs.

Without a Vacuum Pump

If vacuum pump is not available, use the following procedure.

Install a clear hose to bleeding screw.

Open bleeding screw. Fill reservoirs and pump brake lever or brake pedal until fluid freely flows out of the hose.

Close bleeding screw.

Pump up system pressure with brake lever or brake pedal until lever or pedal resistance is felt.

Squeeze brake lever or depress brake pedal, open bleeding screw and then close it.

NOTE: Do not release brake lever or brake ped-al until bleeding screw has been closed. For the front brake system, switch to LH and RH caliper. Turn handlebar to full RH side when bleeding right caliper and turn to the LH side for the left caliper. This helps to reach air into the caliper. The front and the rear brakes must be bled at the same time.

Release brake lever or brake pedal slowly.

Repeat the procedure until no more air bubbles appear in hose and lever or pedal is stiff.
PROCEDURES
BRAKE LIGHT SWITCH

The brake light switch is located on the foot brake master cylinder. It can not be adjusted.
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Inspection

First ensure brake light is good.

Check switch for dirt or corrosion. Make sure it is operating properly.

Depress brake pedal and check for brake light to turn on. Repeat with the brake pedal.

Test

Disconnect switch connectors.

Check switch operation as follows.

	SWITCH POSITION
	PIN
	RESISTANCE

	Firmly pushed
	1
	2
	0.2 Ω max

	Released
	
	
	Infinite


If switch is defective, replace with a new one. If switch tests good, check wiring harness.
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Removal
Disconnect switch connectors.

Drain brake system.

Unscrew brake light switch from master cylinder.

Catch spilled fluid with a rag.

Installation

For installation, reverse the removal procedure.

NOTE: Apply Loctite 657 (pipe sealant) on the threads of brake light switch.
Bleed the brake system.
Check for leaks and make sure the brakes operate normally before driving.

PARKING BRAKE LOCK LEVER
Removal
Remove:
- nut
- screw
- spring
- brake lock lever

Installation

For installation, reverse the removal procedure.
Install the spring properly.
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LH PARKING BRAKE LEVER
Removal
Remove:
- parking brke lock lever
- nut
- screw
- brake lever
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1. Break lever
2. Screw
3. Nut
Inspection
Check brake lever for bending, cracks or other damages. Replace if necessary.
Installation

For installation, reverse the removal procedure.
MECHANICAL PARKING BRAKE LEVER
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Removal
Remove:
- Rearview mirror(RH)

- Handlebar grip cover
- Handlebar grip
- 2WD/4WD switch
- Screw
Remove mechanical parking brake lever from handlebar.
Loosen the screw and remove the lever, then separate braking cable and brake lever.
Inspection
Check spring for bending, cracks or other damages. Replace if necessary.
Check brake lever for bending, cracks or other damages. Replace if necessary.

Installation

For installation, reverse the removal procedure.

FRONT MASTER CYLINDER

Removal
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1. Brake fuild reservoir cap
2. Brake fuild reservoir diaphragm

3. Brake lever
4. Brake rod
5. Dust boot
8. Pin
9. Parking lever
10. Spring
11. Union bolt
12. Washer
13. Brake hose
14. Brake master cylinder hold
15. Brake master cylinder

Remove the handlebar cover, rearview mirror and winch control switch.

Unscrew the screws then remove master cylinder cap and its diaphragm. Drain brake fluid until front master cylinder reservoir is empty.

Remove fitting nut and sealing washers retaining brake hose to front master cylinder.

Remove screws from master cylinder holder and remove master cylinder from handlebar.

Disassembly

Remove brake lever lock and brake lever.

Remove dust boot, snap ring, piston and spring.
Inspection and Lubrication
Discard any remaining fluid inside reservoir.

Clean reservoir, piston and master cylinder thoroughly with clean brake fluid.
Check:

- boot for crack

- spring for damage

- piston cup for wear, deterioration or damages

- master cylinder and piston for scoring, scratches or other damages.

Change part(s) if necessary.

Check if the end cap O-ring is brittle, hard or damaged.
NOTE: If master cylinder housing is damaged or leaking, replace as an assembly.

Assembly
Coat piston and piston cups with clean brake fluid.
Install:

- spring onto piston

- piston into master cylinder

- snap ring into groove in the master cylinder

- boot into master cylinder and the groove in piton.
Apply dielectric grease to the brake lever contacting surface of the piston.

Install brake lever and locking mechanism.

NOTE: Apply dielectric grease on lever pivot bolt.

Installation

For the installation, reverse the removal procedure, pay attention to the following details. Place the brake lever assembly on the handlebar.
Position cylinder holding bracket with the UP mark upward.

Install bolts and tighten loosely.

With the handlebar in straight ahead position, position cylinder reservoir parallel to the ground. Tighten upper bolt first.
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Connect brake hose to master cylinder with fitting nut and new sealing washers.

Bleed brake system.

Check for leaks and make sure the brakes operate normally before driving.

REAR MASTER CYLINDER

Removal

Drain brake fluid.

Remove RH footrests and front mud board.

Unplug brake switch connectors.

NOTE: At this time, check hoses and fittings for damages or leaks.
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1. Brake switch
2. Front brake hose
3. Rear brake hose
4. Reservoir hose
5. M6 Bolt for master cylinder
6. Push rod lock

Disconnect reservoir flexible hose and plug the end to avoid brake fluid spillage.

Unscrew rear hose from master cylinder.

Unhook push rod from brake pedal.

Remove M6 bolts retaining master cylinder to the frame.
Disassembly

Remove:

- end cap

- spring

- piston

- boot 

- snap ring 

- push rod.
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1. End cap
2. Spring
3. Piston

Inspection and Lubrication

Discard any remaining fluid inside reservoirs.

Clean reservoirs, pistons and master cylinders thoroughly with clean brake fluid.

Check:

- boots for crack

- springs for damage

- piston cups for wear, deterioration or damages

- master cylinders and pistons for scoring, scratches or other damages.

Change part(s) if necessary.

Check locking pin for excessive wear, replace if necessary.

Check if the end cap O-ring is brittle, hard or damaged.

NOTE: If master cylinder housing is damaged or leaking, replace as an assembly.

Assembly

Apply synthetic grease on both ends of push rod.

Install:

- push rod

- snap ring

- boot.

If push rod yoke has been removed, reinstall it then adjust push rod length, see the following illustration.
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A. 44±1mm(1.732±0.039 in)
Apply piston and piston cups with clean brake fluid. The spring is conical. Install the smaller end on piston.

Insert piston in the master cylinder.

Install the end cap. Do not forget the O-ring.

Installation

Install master cylinder to frame.

Install push rod on brake pedal.

Connect front and rear hoses on master cylinder.

Connect flexible hose from reservoir.

Fill up reservoir with clean brake fluid.

Bleed brake system.
Connect brake light switch connectors.

Check for leaks and make sure the brakes operate normally before driving.

BRAKE CALIPER

Removal
Loosen wheel nuts.

Raise vehicle and support it securely.

Remove appropriate wheel.

Loosen the M10 bolts then remove the brake caliper from steering knuckle. If the caliper is not being removed from the vehicle as during brake pad replacement, simply hang the caliper with a piece of wire to take the weight off the brake hose.

CAUTION: Do not let caliper hangs by the hose and do not stretch or twist the hose.

If the caliper is being removed for replacement, drain brake system before removing the Banjo fitting and its sealing ring. 
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FRONT CALIPER 
1. Remove banjo fitting and washers

2. Unscrew bolts

Remove spring and loosen the nuts, then remove the parking brake cable from the RH rear caliper.
Drain brake system before removing the Banjo fitting and its sealing ring, then remove the rear caliper.
[image: image268.png]



RH REAR CALIPER 

1. Remove parking brake cable

2. Remove banjo fitting and washers

3. Unscrew bolts

Catch spilled fluid with a rag. Attach the brake hose in a position to prevent the fluid from flowing out.

Disassembly
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1. Brake pad hloding bolt
2. Brake pad
3. Pad spring
4. Caliper bracket
5. Brake caliper piston
6. Dust seal
7. Caliper piston seal
8. Bleed screw

Remove brake pads, see the following section.

Remove:

- caliper bracket
- pad spring.

Place a rag over the caliper piston.

Place caliper body with piston down and apply small squirts of air pressure to the fluid to remove the caliper piston.
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Remove dust seal and piston seal.
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1. Caliper dust seal
2. Caliper piston seal

CAUTION: Be careful not to damage piston sliding surface.

Clean piston grooves, caliper cylinder and piston with clean brake fluid.

Clean slide pins with brake cleaner and a rag.

Inspection
	Recommended brake component replacement schedule:

	Brake pads
	As required

	Piston seals, dust seals
	Every two years

	Brake hoses
	Every four years

	Brake fluid
	Replace when brakes are disassembled
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WARNING

	All internal brake components should be cleaned in new brake fluid only. Do not use solvents as they will cause seals to swell and distort.


If boots are deteriorated or hard, replace with new ones.

Check caliper cylinder for scratches, rust or other damages. If so, replace caliper.

Check piston for scratches, rust or other damages. If so, replace piston.

Assembly

Coat new piston seal with clean brake fluid and install it into piston grooves in caliper.

Coat piston with clean brake fluid and install into cylinder with the closing toward caliper body.

Apply dielectric grease into sliding bores and install slide pins.

NOTE: Make sure that rubber boots are correctly installed in slide pins grooves.

Install pad spring, caliper bracket and pads.

Installation

For the installation, reverse the removal procedure.

Front Brake Caliper
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Install caliper in its original position.

Torque M10 mounting bolts for brake caliper to torque: 48 Nm.
Use new sealing washers when installing banjo fitting retaining brake hose to caliper.

Torque union bolt for brake hose to torque: 22~30 Nm.
Fill the brake reservoir with recommended brake fluid DOT4.
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WARNING

	- Brake fluid may damage painted surface or plastic parts. Always clean up spilled brake fluid immediately.
- Use only the designated quality brake fluid: other brake fluids may deteriorate the rubber seals, causing leakage and poor brake performance.

- Refill with the same type of brake fluid: mixing brake fluids may result in a harmful chemical reaction and lead to poor brake performance.

- Be careful that water does not enter the master cylinder when refilling. Water will significantly lower the boiling point of the brake fluid and may result in vapor lock.


Bleed the brake system.

Check for leaks and make sure the brakes operate normally before driving.
RH Rear Brake Caliper
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Install caliper in its original position.

Torque M10 mounting bolts for brake caliper to torque: 48 Nm.
Install gasket, parking brake cast, bolt and O-ring.
Torque bolt for parking brake hose to torque: 22~30 Nm.
Use new sealing washers when installing banjo fitting retaining brake hose to caliper.

Torque union bolt for brake hose to torque: 22~30 Nm.
Fill the brake reservoir with recommended brake fluid DOT4.
CAUTION: 
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WARNING

	- Brake fluid may damage painted surface or plastic parts. Always clean up spilled brake fluid immediately.
- Use only the designated quality brake fluid: other brake fluids may deteriorate the rubber seals, causing leakage and poor brake performance.

- Refill with the same type of brake fluid: mixing brake fluids may result in a harmful chemical reaction and lead to poor brake performance.

- Be careful that water does not enter the master cylinder when refilling. Water will significantly lower the boiling point of the brake fluid and may result in vapor lock.


Bleed the brake system.

Check for leaks and make sure the brakes operate normally before driving.
Adjust parking brake cable free play.
BRAKE PADS

Removal

Raise vehicle and support it securely.

Remove appropriate wheel.

Loosen brake caliper mounting bolts M10.

Remove caliper from knuckle.

Unscrew brake pad holding bolt then remove pads.

CAUTION: Do not let the caliper hang by the hose and do not stretch or twist the hose.

Push piston all the way in to allow installation of new pads.
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WARNING

	Disc brake components rarely require disassembly. DO NOT:

- Disassemble components unless absolutely necessary;

- Use solvents on internal brake components;

- Use spent brake fluid for cleaning; (use only clean brake fluid)

- Allow brake fluid to come in contact with the eyes, as this may cause eye injury;

- Splash brake fluid onto painted surfaces or plastic parts, as this may cause damage;

- Disconnect any hydraulic connection, as this would require the entire brake system to be disassembled, drained, cleaned, properly filled and bled after reassembly.


Inspection

CAUTION: Do not clean brake pads in petroleum-based solvent. Use brake system cleaner only. Soiled brake pads must be replaced with new ones.

Measure brake pad thickness.

Brake pads must be replaced when pad is 1.5 mm thick or less, or look the hollow places on both sides on the pad lining.

There are three hollow places on one set of brake pads. When the pad wear reaches one of the hollow places, the pad must be changed even if the pad wear does not reach another hollow place.
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	Brake pad wear limit
	1.5 mm
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WARNING

	Avoid getting oil or grease on brake pads. Contaminated brake pads can affect stopping capacities.


CAUTION: Brake pads must always be replaced in pairs.

Installation
[image: image280.png]



1. Brake oil hose
2. Brake caliper bleed screw
- Connect a suitable hose tightly to the brake caliper bleed screw. Put the other end of this hose into an open container. 
- Loosen the brake caliper bleed screw and using a finger push the caliper piston into the brake caliper. 
- Tighten the brake caliper bleed screw to 5 Nm. 
- Install the new brake pads and a new brake pad spring. 
- Tighten the brake pad holding bolts to 17 Nm and brake caliper bolts to 24~28 Nm.
CAUTION: Always install new brake pads and brake pad spring as a set. Do not operate the brake pedal during or after brake pad removal. After replacing the brake pads, pump the brake pedal a few times to check for proper brake operation and then check the brake fluid level.

BRAKE DISC

Inspection

Brake discs can be inspected without removing them from the vehicle.

Raise vehicle and support it securely. Remove wheels and visually inspect disc surfaces for scratches or grooves. Make sure to check both sides of disc.

Measure thickness of the disc.

	Front/Rear Disc Minimum Thickness
	3 mm


Replace disc if out of specifications.

Measure the deflection of brake disc. If the deflection exceeds the service limit, replace the brake disc with a new one.
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Maximum deflection of brake disc: 0.1 mm.
Removal

Apply parking brake and raise the vehicle.

Remove appropriate wheel.

Remove caliper as described previously. Do not disconnect brake hose from caliper.

Remove the cotter pin, the caste nut and the washer. Discard cotter pin.

Pull out wheel hub with brake disc.

Loosen and discard M8 screws for brake disc.
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1. M8 screws

2. Brake disc

Separate brake disc and wheel hub.

Installation

For the installation, reverse the removal procedure.
Aplly threadlocker on the M8 screws for brake disc.

Tighten the screws for brake disc bolts to 30 Nm.
BRAKE PEDAL
Removal

Remove RH foot plate.
Remove pin separate the master cylinder push rod and brake pedal.

Remove washer and snap ring.
Remove bolt retaining the brake pedal to frame.

Inspection

Check brake pedal for cracks or distortion.

Check if ring and washer are brittle, hard or otherwise damaged.

Replace any defective parts.

Installation

For installation, reverse the removal procedure.

Apply synthetic grease on both snap ring and into brake pedal.
BRAKE HOSES

Inspection

Brake hoses should be inspected frequently for leaks and damages.

Check if the hoses are crushed or damaged. Any deformation can restrict the proper flow of fluid and cause braking problems.

Check hoses for cracking or scrapes. This damage can cause hose failure under pressure.

When hoses are removed or disconnected, cleanness must be observed. Clean all joints and connections before disassembly. New hoses should be cleaned with brake fluid before installation to remove any contamination.

Replace any defective parts.

Removal

NOTE: Before removing any hoses, drain brake system.

Remove all necessary parts to reach the hoses.

Thoroughly clean the area around the joints that will be disconnected.

Place a drain pan under the joint that will be disconnected.

Disconnect any retaining clips or brackets holding the hose and remove the defective part(s).

Installation

Install the new hose.

Make sure the piece will not rub against any other part.

When there is a fitting nut securing the hose to the caliper or to the master cylinder, always replace the sealing washers with new ones.

Install any retaining clips or brackets. Refill and bleed the system.
11.BODY AND FRAME
	BODY
11-1
	FRAME
11-8


11.1 BODY

Front panel combination-1
                           Front panel combination-2
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Front panel combination-1
(MUD Version)               Front panel combination-2(MUD Version)
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Foot rest combination                                       Rear plastic part combination
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Seat
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GENERAL

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.). If the efficiency of a locking device is impaired, it must be renewed.



PROCEDURES
SEAT

Cleaning
It is recommended to clean seat with a solution of warm soapy water, using a soft clean cloth.
CAUTION: Avoid use of harsh detergents such as strong soaps, degreasing solvents, abrasive cleaners, paint thinners etc. that may cause damage to the seat cover.
Removal
Rear seat back

Loose three M8 bolts for rear seat back.
Remove the seat back.
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Operator’s Seat
NOTE：Before remove the front seat, it must remove the rear seat back. 

Lift up lock catch at the rear of front seat by the left hand, and pull up and remove front seat by the right hand. 
Inspection

Check the seat and rubber washer for cracks, damage, etc., please replace it in time.
Installation
Insert the front tabs of operator’s seat into frame hooks. When seats in its position, firmly push down to latch.
NOTE: A distinctive snap will be felt. Double check that the seat is secure by giving it a tug to confirm proper latching.
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WARNING

	Make sure seat is securely latched before riding.



Tightening torque of bolt for rear seat back: 22-30 Nm.
REARVIEW MIRROR AND HANDLEBAR GRIP COVER
Removal
Rotate main body of rearview mirror anticlockwise to remove rearview mirror on each side. Loose M6 screws, remove handlebar grip cover.
[image: image293.png]



1. Rearview mirror

2. Handlebar grip cover

3. Handlebar cover mounting board

4. 2xM6 screw

5. 4xM6 screw

Inspection

Check rearview mirror and handlebar grip cover for cracks, damage, etc., please replace it in time.
Installation

For installation, reverse the removal procedure.
Tightening M6 screws of handlebar grip cover to torque: 9~12 Nm.
FRONT PANEL
Removal
Remove center handlebar cover.
Loosen M6 screws, then remove dash board cover.
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Loose M6 screws and remove the dash from the cover.
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Remove push pin then remove inner front mud plate.
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Remove push pin and M6 screws, then remove LH and RH mud plate.
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Remove side panel, foot plate and air filter service cover.
Remove front cargo rack and front bumper.

Remove headlight and grille.
Loosen M6 screws, then remove front side guard.
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Loosen M6 screws and remove grille base.
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Rotate the latch hook then remove front storage box cover.
Loosen M6 screws and remove front cargo box.
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Installation

For installation, reverse the removal procedure.
Tightening M6 screws to torque: 9~12 Nm.

FRONT BUMPER AND WINCH
Removal
Loose and remove the four M8 bolts fixed between the front bumper and frame, and remove front bumper.

Loose and remove the four M6 bolts fixed between front guard board and frame, and remove front guard board.
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Disconnect the winch control connector.

Rotate control handle of winch clockwise, releasing lock-up status of cable. Pull out cable for about 30cm along.
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Remove the four M8 fixed bolts at the behind of the winch, pull out the relevant connector and cable, and finally remove the winch for maintenance.
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Remove four M6 screws and winch relay cover.
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Remove four lock nuts of winch relay, separating positive and negative electrode ① of winch, positive and negative cable ② of battery from wire group. 
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Disconnect switch plug-in of winch and remove winch relay ④.
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Remove the two bolts numbered 1 to remove the winch switch, and remove the bolts numbered 2 to remove the winch switch bracket.
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Inspection

Check front bumper and cover for crack or damaged. Replace it if required.
Check winch for condition refer to Electrical System.
Installation

For installation, reverse the removal procedure.
Tightening M6 bolt to torque: 9~12 Nm.

Tightening M8 bolt to torque: 22~30 Nm.
CARGO RACK
Removal
Loosen M8 bolts, then remove front cargo rack.
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Remove rear seat back.
Loosen M6 screws and M8 bolts, then remove rear cargo rack.
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Inspection

Check front and rear cargo rack for crack or damages. Replace it if required.
Installation

For installation, reverse the removal procedure.
Tightening M6 bolt to torque: 9~12 Nm.

Tightening M8 bolt to torque: 22~30 Nm.
SIDE PANEL
Removal
Remove operator’s seat.

Remove handlebar cover and dash board cover.
Loosen ST4.2 screws, then remove USB holder.
Loosen M6 screws, then remove hand shifting board.
Loosen M6 screws and push pins, then remove LH/RH middle guard plates.
Loosen M6 screws, then remove engine side cover, engine service cover, middle lower guard plates.
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Loosen M6 screws and remove foot plate from frame.
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Inspection

Check side plastics for crack or damages. Replace it if required.
Installation

For installation, reverse the removal procedure.
Tightening M6 screw to torque: 9~12 Nm.

REAR PANEL
Removal
Loosen M6 screws then remove tail trim cover.
Loosen M6 screws and plate nuts, then remove tail plate. Disconnect the tail light wires.
Remove operator’s seat and rear seat back.
Remove rear cargo rack.
Loosen M6 screws and plate nuts, then remove middle rear guard plate.
Loosen M6 screws and plate nuts, then remove rear side cover.
Loosen M6 screws and plate nuts, then remove rear plastic cover and central cover (only for long wheelbase).
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Inspection

Check rear cover for crack or damages. Replace it if required.
Installation

For installation, reverse the removal procedure.
Tightening M6 screw to torque: 9~12 Nm.

Front Windshield
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1. Front windshield
2. RH windshield bracket
3. RH windshield bracket mounting plate

4. LH windshield bracket mounting plate

5. LH windshield bracket
6. Bolt
7. Windshield bushing
8. Windshield sleeve

9.Bolt
10.Nut
Unscrew the bolts and nuts,then separate the winshield bracket and winshield bracket mounting plate.
Remove the front windshield and bracket from handlebar.
Unscrew bolts, sepearte the front windshield and bracket.
Inspection
After prolonged use, the debris flying in the air will cause some damage to the windshield. If the following conditions occur, please replace it immediately.

1. Unclear windshield affects driving.

2. The front windshield is distortion and cracked.

Installation

For installation, reverse the removal procedure.
Tightening M6 bolt to torque: 9~12 Nm.

Tightening M8 bolt to torque: 22~30 Nm.
11.2 FRAME
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	1.Front Cargo Rack
	2.Rear Cargo Rack
	3. M8 Bolt
	4. LH Foot Plate Bracket

	5. RH Foot Plate Bracket
	6. M8 Screw
	7. M8 Bolt
	8. Front Support Frame

	9. Front Bumper
	10.M8 Nut
	11. Front Bumper Plug
	12. M8 Bolt

	13. Rear Bumper
	14. M8 Bolt
	15. Front license plate bracket


GENERAL

Clean thread before applying a thread locker.
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WARNING

	Torque wrench tightening specifications must be strictly adhered to. 

Locking devices must be replaced with new ones when removed (e. g.: locking tabs, elastic stop nuts, self-locking fasteners, cotter pins, etc.). If the efficiency of a locking device is impaired, it must be renewed.



CAUTION: Before performing electrical welding anywhere on the vehicle, unplug the electronic module connector. Also unplug the negative cable and the voltage regulator. This will protect the electronic module and battery against damage caused by flowing current when welding.
PROCEDURES
FOOT PLATE BRACKET
NOTE:  Use the same procedure for RH or LH foot plate bracket.
Removal
Remove the foot plate.
Unscrew M8 bolts and nuts, then remove foot plate bracket from frame.
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Inspection 
Check foot plate bracket for cracks, bending or other damages. Replace if necessary.
Installation

For installation, reverse the removal procedure.
Tightening M8 bolt to torque: 22-30Nm.
FRONT SUPPORT FRAME
Removal
Remove:
- front cargo rack
- front cargo box
- front bumper and winch
- front grille
- radiator
Unscrew M8 bolts.
Remove the front support frame from vehicle.
Inspection
Check front support frame for cracks, bending or other damages. Replace if necessary.
Installation

For installation, reverse the removal procedure.
Tightening M8 bolt to torque: 22~30 Nm.
TRAIL ARM AND BALL HEAD
Removal
Remove the tow ball pin and fixed pin, then remove the trail arm from frame.
Loosen the nut, then remove trail ball head from trail arm.
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Inspection 
Check trail arm and trail ball head for cracks, bending or other damages. Replace if necessary.
Installation

For installation, reverse the removal procedure.
Tightening M8 bolt to torque: 280-300 Nm.
FRAME

Cleaning

Clean frame with appropriate cleaners and rinse with high pressure hose.

NOTE: Clean the draining holes under frame. The drain holes are located at the rear of bottom side of frame.

Touch up all metal spots where paint has been scratched off. Spray all bare metal parts of vehicle with metal protector.

Welding

Steel Frame:

-electric welding

-amperage:70~110 A

-voltage:20~24 V

- rod: E-7014 (3/32 in).

CAUTION: Before performing electrical welding anywhere on the vehicle, unplug the multiple connectors at the electronic module connector. Also unplug the negative cable and the voltage regulator. This will protect the electronic module and battery against damage caused by flowing current when welding.

NOTE: Install the ground as close as possible from the reparation area.

CAUTION: If welding is to be done near plastic material, it is recommended to either remove the part from the area or to protect it with aluminum foil to prevent damage.

12. ELECTRICAL SYSTEM

	Charging System
12-1
	Starting System
12-6

	EFI System
12-9
	Ignition System
12-11

	Light System 
12-15
	Cooling System 
12-16

	Fuse
12-16
	Relay
12-16

	Speedmeter System
12-17
	Gear Position Indication Switch
12-17

	Oil Pressure Sensor
12-17
	2WD/4WD Switch
12-18

	2WD/4WD Motor
12-18
	Multifunction Gauge
12-18

	12-Volt Auxilary Power Outlet
12-21
	12-Volt Power Outlet
12-21

	Multifunction Switch
12-22
	Winch
12-22

	Engine Modes Selector
12-23
	EPS Controller
12-23


Overhauling information
Warning 
Bulb will be very hot after turning on headlamp. Please do not touch it immediately after its off. In operation, bulb needs to be cooled. 

In warning inspection of water temperature, fire or high temperature liquid may be needed, keep it far away from inflammables and do not to be burnt. 

The temperature will be very high in turning of headlamp. For replacement, grease dirt will be splashed to glass in case of operation with bare hands or wearing dirty gloves. As a result, hot spots and glass deformation may be caused with damage to bulb as well. 

Pay attention to the following in replacing bulb: 

- Do not replace bulb when it is on. Turn off ignition switch and replace it after cooling bulb. 

- In order to avoid splashing grease to glass, wear clean gloves in replacing bulb. 

- Use cloth with alcohol or banana water to clean glass to prevent any grease sticking to glass. 

Check battery to confirm whether it is normal. 

Regularly check switch and do not dismantle it from vehicle in inspection. 

12.1 Charging System
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GENERAL

SYSTEM DESCRIPTION

The purpose of the charging system is to keep the battery at a full state of charge and to provide the electrical system with the required electrical power for normal vehicle operation.

Magneto
The magneto is the primary source of electrical energy. It transforms magnetic field into electric current (AC).

The magneto has a 3 phases series stator.
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Voltage Regulator/Rectifier
The rectifier receives AC current from the magneto and transforms it into direct current (DC).

The voltage regulator, included in the same unit, limits voltage to prevent any damage to electrical components.

[image: image319.png][T [T ]





NOTE: If the battery will not stay charged, the probel can be any of the charging system components. If these all check good, try a new voltage regulator.
Battery

The battery supplies DC power to the electric starter for cranking the engine. During engine starting, it also supplies DC power to the entire electrical system.

At low engine RPM operation and high current load conditions, it supplements the magneto output and helps to maintain a steady system voltage.

INSPECTION

Charging System Output
First ensure that battery is in good condition prior to performing the following tests.

Testing the Output Voltage with multimeter.

1. Start engine with the less consumption as possible (no lights, no accessories).

2. Increase engine RPM as specified in the following table and read voltage in the multimeter.

	Output Voltage Test

	Engine Speed
	Voltage (DC)

	4000 RPM
	14.5 ± 0.5V


If voltage is above specification, replace voltage regulator/rectifier.

If voltage is below specification, check stator output and wiring harness prior to concluding that voltage regulator/rectifier is defective.

Stator
Stator Connector Access

The stator is directly connected to the voltage regulator/rectifier.

Testing the Stator Continuity

1. Disconnect the stator connector from the voltage regulator/rectifier.

2. Check resistance between YELLOW wires.
	Required Tool

	MULTIMETER
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3. If any reading is out of specification, replace stator.

4. Re-plug connectors properly.
Testing the Stator Static Insulation

1. Disconnect the stator connector from the voltage regulator/rectifier.

2. Connect multimeter between any YELLOW wire (on stator connector) and engine ground.

	Required Tool

	MULTIMETER
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3. If there is a resistance or continuity, the stator coils and/or the wiring is shorted to ground and needs to be repaired or replaced.

4. Re-plug connectors properly.

Check Battery

1. Connect a battery load tester.

2. Ensure proper test conditions.
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If battery voltage drops below specification during test, replace battery and perform a CHARGING SYSTEM LOAD TEST.

Charging System Load Test
1. Connect a battery load tester.

2. Start vehicle and read voltage on tester.
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If voltage is above specification, replace regulator and continue CHARGING SYSTEM LOAD TEST.

3. Connect an ammeter around RD1-1 wire.
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DC CURRENT TEST WITH INDUCTIVE AMMETER

1. Output connector of voltage regulator

2. Ammeter clamped over RED wire

4. Ensure proper test conditions.

5. Read amperage on ammeter.

  45±5Amps
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NOTE: With a fully charged battery and no electrical loads, specification is less than 10 A.

If amperage or voltage is not within specification, verify magneto and wires. Replace:

· Voltage regulator if magneto test is within specifications.

· Magneto if magneto test is not within specifications.

PROCEDURES
VOLTAGE REGULATOR 
Removal
Remove the LH side panel. Refer to BODY section.
Disconnect the voltage regulator connector.
Loosen M6 bolts, remove voltage regulator.
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1. Voltage Regulator
2. M6 Bolts
Testing the Voltage Regulator Continuity

Due to internal circuitry, there is no static test available.
Voltage Regulator Wire Identification

	FUNCTION
	PIN
	COLOR

	12Vdc output
	RD1-1
	Red

	12Vdc ground
	RD1-2
	Black

	12Vac input
	RD2-1
	Yellow

	12Vac input
	RD2-2
	Yellow

	12Vac input
	RD2-3
	Yellow


Testing the Voltage Regulator Power

1. Check voltage at RD1-1.
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2. Connect a battery load tester.

3. Start vehicle.

4. Ensure proper test conditions.
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5. Measure voltage drop.
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	Backprobe
	Probe
	Specification

	RD1-1
	Bat1(-)
	Under 0.2 Vdc


If voltage drop is above specification, locate and repair damaged connector/wire.
Testing the Voltage Regulator Ground

1. Check ground at RD1-2.
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	Test Conditions

	RD1-2
	Permanent ground


	Backprobe
	Probe
	Specification

	RD1-2
	Bat 1(+)
	Battery voltage


2. Connect a battery load tester.

3. Start vehicle.

4. Ensure proper test conditions.
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5. Measure voltage drop.
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	Backprobe
	Probe
	Specification

	RD1-2
	Bat 2(-)
	Under 0.4 Vdc


If voltage drop is above specification, locate and repair damaged connector/wire.
Installation
Tighten M6 bolts for voltage regulator to torque: 9~12 Nm.

BATTERY

The vehicle is equipped with a maintenance-free type battery. Refer to battery manufacturer's instructions for proper filling, activation and routine charging procedures.
Troubleshooting
Discharged or Weak Battery
- Battery post and /or cable terminal oxidized
- Loose or bad connections
- Faulty battery(does not keep a full charger)
- Main system fuse burnt, fault wiring/connections, voltage regulator or stator.
Battery Removal
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WARNING

	Always respect this order for removal; disconnect BLCAK(-) cable first. Electorlyte or fuel vapors can be presnt and spark may ignite them and positbly cause personal injuries.


The battery is located underneath the driver's seat.


Removing the Battery

1. Remove seat.

2. Remove battery cover.
3. Disconnect BLACK (-) cable first, then the RED (+) cable.
NOTICE: Always respect this order for removal; disconnect BLACK (-) cable first.

4. Remove battery.
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Cleaning the Battery

Clean the battery rack, cables and battery posts using a solution of baking soda and water.

Remove corrosion (if so) from battery cable terminals and battery posts using a firm wire brush.

Rinse with clear water and dry well.

Inspecting the Battery

Visually inspect battery casing for cracks or any other damages. If casing is damaged, replace battery and thoroughly clean battery support with a water and baking soda solution.

Inspect condition of battery posts, battery support, holding strap and strap attachment points and wire terminal lugs.

Battery Storage

It is not necessary to remove the battery during vehicle storage but it is recommended for long term storage.

If the battery is left in the vehicle during storage or used infrequently, disconnect the BLACK (-) negative battery cable to eliminate battery current drain from the electrical equipment.

Recharge the battery once a month with an approved battery charger as per manufacturer's recommendations.

Clean battery, battery support and connections as required. 

For other recommendations during storage, refer to battery manufacturer instructions.
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WARNING

	Ensure battery is stored in a safe place, out of reach for children.


Activating a New Battery

Refer to the instructions provided with the battery.

Charging a Battery
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WARNING

	Always wear safety glasses and charge in a ventilated area. Never charge or boost a battery while it is installed on vehicle. Do not open the sealed cap during charging. Do not place battery near open flame.


NOTICE: If battery becomes hot, stop charging and allow it to cool before continuing.

NOTE: If battery pressure increases due to overcharging, the valve opens to release excess pressure, preventing battery damage.

An automatic charger is a fast and convenient way for error-proof charging.

Always follow the battery manufacturer's charging instructions.

When using a constant current charger, charge battery according to the chart below.

Battery Voltage Below 12.8 V and Above 11.5V.
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Installing the Battery

NOTICE: Always connect RED (+) cable first then BLACK (-) cable.
GROUND
Ensure ground is clean and tight.
12.2 Starting System
GENERAL
System Description
The starting system is composed of an electric starter supplied in current by the battery through a solenoid.

The starter solenoid receives a 12 Vdc input from the ignition switch and the ground signal is provided by the Gear controller.

· Transmission in Park or Neutral position and/or brake pedal held.

· Ignition switch turns to the start position and hold until the engine starts.
Electrical Cables and Connections

Check all connections, cables and wires. Tighten any loosen connections. Replace any cracked wires/cables.
PROCEDURES

FUSES
Make sure the main fuses are in good condition.
BATTERY
To check battery condition, refer to Battery in the CHARGING SYSTEM.
IGNITION SWITCH
To check ignition switch, refer to Ignition Switch in the IGNITION SYSTEM.
START/STOP SWITCH
To check start/stop switch, refer to Start/Stop Switch in MULTIFUCTION SWITCH this section.
STARTER SOLENOID

Starter Relay 

The starter solenoid is located beside the fuse box and the battery, under the front seat.
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Power Signal to Primary Winding
Disconnect small terminals from solenoid.
Turn ignition switch on and set shift in Park position.
Use a multimeter and set it to Vdc.
Press start/stop switch measure the voltage as following.
	Start/Stop Switch
	Wires
	Voltage

	Depressed and held
	Grey red and 
Grey green
	Battery voltage


If voltage is good, test solenoid. See below.
If voltage is not good:
· Bypass ground circuit as follows.
	Start/Stop Switch
	Wires
	Voltage

	Depressed and held
	Grey red and battery ground
	Battery voltage


- If voltage is now good, check ground circuit (White/Red wire) and Gear position switch.
Solenoid Static Test
Disconnect terminals from solenoid.
Use a multimeter and set it to ohm.
Measure primary winding resistance as following.
	Solenoid Terminal
	Resistance
@ 20°C (68°F)

	A
	B
	Approximately 5Ω


Check for stuck solenoid plunger.
	Solenoid Post
	Measurement

	Battery Post
	Starter Post
	Open circuit


If any measurement is out of specification, replace solenoid.
Solenoid Dynamic Test
Turn ignition switch on and set shift in Park position.
Set engine stop switch to OFF to prevent engine starting.
Use a multimeter and set it to Vdc.
Depress start/stop switch and while engine is cranking, measure the voltage drop as follows.
	Solenoid Post
	Measurement

	Post coming from battery
	Post going to starer
	0.2 Vdc max.


If voltage is out of specification, replace start solenoid.
START MOTOR
Starter Test
Remove LH side panel.
Using booster cables, carefully supply current from the battery directly to the starter. Connect the BLACK (-) cable first. Then connect the remaining jumper cable from the battery to the starter.
If starter does not turn, replace it.
Starter Removal
Turn OFF ignition switch.
Disconnect BLACK (-) cable from battery.
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WARNING

	Always disconnect BLACK (-) cable first and reconnect last.


Remove the LH front mud borad.
Disconnect RED (+) cable from starter.
Clean starter area.
Remove starter mount screws.
Pull starter out.
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Disassembly
1. Bracket
2. Brush holder

3. Brush spring

4. O-Ring

5. Washer

6. Motor housing

7. Washer

8. Armature coil

9. Washer supporting tools

10. Inner bracket

11. O-Ring
Brush
- Check the brush on the brush holder whether it is worn abnormal, cracked or not smooth.
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Worn, cracked, or not smooth: → Replace

Rectifier

- Check the rectifier whether it is discolored, abnormal wear or concave.

Abnormal wear or damage: → Replace

- If the rectifier is discolored, grind it with sanding paper, then wipe it with a clean fabric.

- If there is concave, scrape off insulator B, so that the distance with A is d.

d≥1.5mm
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Armature coil
- Test the connection between each wire and the armature coil with the multimeter.

- If they are not connected, replace the armature shaft.

Oil seal
- Check the oil seal lip for damage or leak.

Damage or leakage: →Replace the starter motor.
Starter relay
- Inter-terminal voltage is 12 V. Test the direct connection of positive and negative poles with the multimeter.
- If the starter relay clicks and connected, the starter relay is OK.

- When there is no voltage of 12V, they are not connected, the starter relay is OK.

Note: Do not apply battery voltage on the starter relay for more than 2 seconds. This will result in overheating or damaging the relay coil.
-Measure the coil resistance with the multimeter. If the resistance exceeds the specified value, replace the starter relay.

The multimeter is set to 1x10 Ω.

Starter relay coil resistance: 3-5 Ω.

Starter Installation
Installation is the reverse of removal procedure. However, pay particular attention to the following.
Make sure that starter and engine mating surfaces are free of debris. Serious problem may arise if the starter is not properly aligned.
Torque starter screws to 10 Nm (89 lbf.in).
Connect the RED (+) cable to the starter and torque nut to 6 Nm (53 lbf.in). Apply dielectric grease on terminal and nut.
First connect RED (+) cable to battery then connect the BLACK (-) cable.
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WARNING

	Always connect RED (+) cable first then BLACK (-) cable last. Whenever connecting the RED (+) cable to the starter motor, make sure the battery cables are disconnected to prevent electric shock.


Test starter operation.

12.3 EFI System

Schematic diagram of EFI system
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GENERAL
The function of EFI system includes two parts: fuel injection management and ignition management, which are realized by the following institutions.

(1). ECU: it is responsible for the receiving of sensor signal, the formulation of control strategy, and the issue of control signal.
(2). Oil supply device: it is composed of oil pump, tubing and injector. The pump pressurizes the fuel to 250 KPa. The injector is installed on the engine inlet to control the injection timing and fuel injection amount.
(3). Ignition device: it is composed of ignition module, high voltage wire and spark plug. The ignition module has a DC capacitor igniter and a high voltage ignition coil, which can raise the voltage of the battery from 12V to more than 15000V, which also can be transported to the spark plug by high-voltage wire to generate spark discharge.
(4). Sensors: including: a. The oxygen sensor, which mounted on an exhaust pipe to detect oxygen concentration in exhaust gases, can realize the closed-loop regulation of the mixture concentration, and when the closed-loop adjustment, the output of 0~0.9 V alternating signal can be achieved;

b. Cylinder temperature sensor, which is installed on the engine cylinder head to detect the engine body temperature, will affect the starting thickening amount; 

c. Crankshaft position sensor, which is integrated on magneto to provide crankshaft angle signal, is the time reference for fuel injection and ignition control; 

d. The throttle position sensor is mounted on the throttle body to measure the rotation angle of the throttle valve.

(5). Other: including：a. throttle body, which controls air intake through throttle pull wire; 

b. Fault alarm lamp, which is installed on the dashboard for fault alarm; 

c. Battery, fuse for power supply to EFI system.
INSPECTION
Fuel Gauge /Fuel Level Sensor
Remove fuel tank service cover, and then remove fuel sensor from fuel tank.
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Hold fuel sensor in an upright position after removing it. It is normal if indicator shows “E”, otherwise, circuitry connection, fuel sensor or instrument should be inspected.
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Turn fuel sensor upside down. It is normal if indicator shows “F”, otherwise, circuitry connection, fuel sensor or instrument should be inspected.
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Measure fuel sensor resistance.
	FLOAT POSITION
	RESISTANCE

(20℃/ 68℃)

	Top(Full)
	≥86 Ω

	Bottom(Reserve)
	≤15 Ω


If resistance is not within empty and full values (depending on fuel quantity), check and repair wiring and/or connectors between multifunction gauge and fuel level sender.  
If they test good, replace fuel pump. Refer to FUEL SYSTEM.
If fuel level sender and wiring/ connectors are good, try a new multifunction gauge.

12.4 Ignition System
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TROUBLESHOOTING

No Spark, Weak or Intermittent Spark

- Spark plug gap incorrect

- Fouled spark plug

- Faulty spark plug cap or poor connection to high tension lead

- Related wiring loose, disconnected, shorted, or corroded

- Engine stop switch or ignition switch faulty

- Terminal board or connections wet, corroded

- Poor ignition coil ground (e.g. coil mount loose or corroded)

- Faulty stator (measure resistance of all ignition related windings)

- Incorrect wiring (inspect color coding in connectors etc.)
- Faulty ignition coil winding (measure resistance of primary and secondary) 

- Worn magneto (RH) end crankshaft bearings

- Sheared flywheel key

- Flywheel loose or damaged

- Trigger coil air gap too wide (where applicable) should be 0.030-0.050 in (0. 75-1.25 mm) 

- Excessive crankshaft run out on magneto (RH) end should not exceed 0.005in(0.13mm) 

- Faulty ECU
IF THE IGNITION SYSTEM FAILS TO OPERATE

Inspection
1. Fuse
Check ignition switch for continuity or not. If it not continuity, replace the fuse.
2. Battery
Check the battery condition refer to Battery Inspection in this section. If battery is incorrect, as following:
Clean battery terminals.
Recharge or replace the battery.
3. Spark plug
- Check the spark plug condition.
If it is out of specification, repair or replace the spark plug.
· Check the spark plug type.
	Standard Spark Plug
	DCPR8E / NGK


· Check the spark plug gap.

	Spark Plug Gap
	0.8 to 1.0 mm


4. Ignition spark gap
- Disconnect the spark plug cap from the spark plug
- Connect the ignition test as following
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- Turn the ignition switch to ON position
- Check the ignition spark gap
- Check the spark by pushing the starter switch, and increase the spark gap until a misfire occurs.
If meet specification, the ignition system is not faulty.
5. Resistive cable with Spark Plug cap resistance
- Remove the spark plug cap
- Remove the resistive cable from the ignition coil
- Connect the pocket tester(Ωx 1K) to the spark plug cap and the resistive cable terminal.
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Tester(+) lead        Spark plug side①  
Tester(-) lead        High tesion cord side②
NOTE:

- When removing the spark plug cap, do not pull the spark plug cap from the resistive cable.
- Remove      Pulling
- Connect      Pushing
- Check the resistive cable with spark plug cap
	Resistive cable resistance
	3.68± 0.73KΩ(@20ºC)


If out of specification, replace the resistive cable.
6. Ignition coil resistance
Disconnect the ignition coil connector from the wire harness
- Connect the pocket tester to the ignition coil.

- Check if the primary coil has the specified resistance.
	Primary coil resistance
	0.58± 0.058Ω(@20ºC)
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Tester (+) lead      Right Terminal

Tester (-) lead      Left Terminal

- Remover the resistive cable from the ignition coil 

- Connect the pocket tester (Ω×1k ) to the ignition coil.

- Check the secondary has the specified resistance.
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Tester (+) lead       Connector side (Right )

Tester (- ) lead       Resistive cable side

	Secondary coil resistance
	9.6±0.96KΩ(@20ºC)


If out of specification, replace the ignition coil.
7. Ignition switch
Check ignition switch for continuity or not. If it not continuity, replace the ignition switch.
8. Engine stop switch
Check engine stop switch for continuity or not. If it not continuity, replace the handlebar switch.
9. Wiring connection
- Check the connection of the entire ignition system.
 Refer to the circuit diagram.
If it corrects, replace the ECU.
PROCEDURES 
Safety Precautions
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WARNING

	To prevent powerful electric shocks while cranking engine, neither touch any electronic ignition components (ignition coil, wire harness, etc.) nor tester lead clips. Also make sure that tester leads do not touch any metallic object.


BATTERY

At least 8V is required for proper ignition system operation. Check battery voltage.

IGNITION SWITCH

Quick Test

Turn the ignition switch to the ON position.

- If the taillight turns on, the ignition switch is good.

- If the taillight does not turn on (assuming bulb is good), test it.

Switch Power Supply Test

Remove USB holder and disconnect ignition switch. Measure power supply to switch as follows.
	Ignition Switch Connector
	Voltage

	Black/red and Blue/red
	Battery ground
	Battery voltage


If voltage is inadequate, test wiring harness.

If voltage is good, test switch.

Switch Resistance Test

Use a multimeter and measure the resistance between the following wires.
	Position
	Wire
	Resistance

	OFF
	Black/red
	Infinite (OL)

	
	Blue/red
	

	ON 
(w/lights)
	Black/red
	0.2 ± 0.2 Ω max.

	
	Blue/red
	

	ON 
(w/o lights)
	Black/red
	Infinite (0L)

	
	Blue/red
	0.2 ± 0.2 Ω max.


Replace switch if defective.

Switch Removal

Remove the USB holder and unplug the switch connector.
Switch Installation

For the installation, reverse the removal procedure.

ENGINE STOP SWITCH

Test

If engine crank when pressing the start button and engine stop switch is on RUN position but there is no spark, test the engine stop switch as follows.

Remove the dash cover (refer to BODY) and unplug the multifunction switch connector.

Using a multimeter, measure the resistance between the following wires.

	Position
	Wire
	Resistance

	Switch to OFF
	Black and Black/White
	1 Ω max.

	Switch to RUN
	
	Infinite (0L)


Replace multifunction switch if defective.

TRIGGER COIL

NOTE: The trigger coil is not adjustable.

Static Test: Continuity

Check resistance with a high-sensitivity ohm meter.

1. Remove side panel and disconnect the trigger coil connector.

2. Measure resistance as follows.

	Trigger Coil Connector
(trigger coil side)
	Resistance@ 20°C (68°F)

	Green/Yellow
	Brown/Yellow
	774~946 Ω


Dynamic Test: Voltage

1. Disconnect the trigger coil connector.

2. Connect multimeter and measure voltage as follows.

	Start
Button
	Trigger Coil Connector
(trigger coil side)
	Voltage

	Depressed
	Green/Yellow
	Brown/Yellow
	0.4~0.7 Vac


3. Repeat operation 3 times.

4. If the trigger coil is out of specification, replace it. If it tests good continue the other tests.

IGNITION COIL
Ignition coil is mounted on frame under the operator’s seat.
NOTE: An ignition coil with good resistance measurement can still be faulty. Voltage leak can occur at high voltage level which is not detectable with an ohmmeter. Replacing the ignition coil may be necessary as a test.

Static Test

Primary Winding

Disconnect the wire connector on the primary side of the ignition coil.

Using a multimeter, check the resistance as follows.

	Ignition Coil
(primary winding)
	Resistance
@ 20°C (68°F)

	Coil terminal
	Ignition coil body ground
	0.9~1.2 Ω


If not within specification, check coil grounding and if good, replace the ignition coil.

Secondary Winding

Disconnect spark plug cap.

Measure resistance as follows.
	Ignition Coil
(Secondary winding)
	Resistance
@ 20°C (68°F)

	Spark plug cable cap terminal
	Ignition coil body ground
	9~14 Ω


If resistance is good, continue with the dynamic test.

If test failed, remove spark plug cap to check its resistance.
	Spark Plug Cap
	Resistance
@ 20°C (68°F)

	Cable side
	Spark plug side
	5 kΩ


If cap is not good, replace it.

If cap is good, replace ignition coil.

Dynamic Test

NOTE: The output voltage should not be less than 12 kV (12 000 V).

An ignition coil tester available from aftermarket tool/equipment suppliers can be used.

CAUTION: Do NOT use coil tester on metal work bench. Follow manufacturer instructions.

If the ignition coil is out of specification, replace it. If it tests good ensure the wiring and connectors are in good condition then continue the next tests.

IGNITION TIMING

Ignition timing is not adjustable.

SPARK PLUG

Spark Plug Removal

Unplug the spark plug cable.

Clean the spark plug area with pressurized air.
Unscrew spark plug.
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1. Spark plug cable
2. Spark plug
Troubleshooting Fouled Spark Plug

Fouling of the spark plug is indicated by irregular running of the engine, decreased engine speed due to misfiring, reduced performance, and increased fuel consumption. This is due to a loss of compression. Other possible causes are: prolonged idling or low-speed riding, or running on a too rich mixture due to abuse of choke, a clogged air filter, a faulty carburetor adjustment, incorrect fuel, defective ignition system, incorrect ignition timing, incorrect spark plug gap, lubricating oil entering the combustion chamber, or too cold spark plug. The plug face of a fouled spark plug has either a wet black deposit or a black carbon fouling. Such coatings form a conductive connection between the center electrode and ground.
Spark Plug Analysis

[image: image350.png]



1. Overheated (light grey, white)

2. Normal (light brown, brown)

3. Fouled (black, wet or dry, dark deposits, grey, melted coating)
The plug face reveals the condition of the engine, operating condition, method of driving and fuel mixture. For this reason it is advisable to inspect the spark plug at regular intervals examining the plug face (i.e. the part of the plug projecting into the combustion chamber).

Spark Plug Installation

Prior to installation make sure that contact surfaces of the cylinder head and spark plug are free of grime.

- Using a wire feeler gauge, set electrode gap to 0.7 mm (0.027 in).

- Apply lubricant over the spark plug threads to prevent possible seizure.

- Hand screw spark plug into cylinder head and tighten with a torque wrench and a proper socket.
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1. Proper socket

2. Improper socket
- Torque spark plug to 20 Nm (15 lbf.ft).

12.5 Light System
12.5.1 Headlight 

NOTICE: Poor lighting can result in reduced visibility when driving. Headlight and taillight lenses become dirty during normal operation. Clean lights frequently and replace burned out lamps promptly. Do not operate this vehicle at night or in low light conditions until the headlight is replaced. Always make sure lights are adjusted properly for best visibility.

When servicing a halogen lamp, don't touch the lamp with bare fingers. Oil from your skin leaves a residue, causing a hot spot that will shorten the life of the lamp.

Replacement 

1. Remove the front headlight cover.

2. Locate the bulb on the back side of the headlight housing.

3. Disconnect the harness from the bulb. 


Headlight Beam Aiming

Turn adjustment screw to adjust beam height to your convenience.

NOTE: Adjust headlights evenly.

Headlight Beam Adjustment 

To adjust the headlight beam, do the following:

1. Load the vehicle as per normal use.

2. Position vehicle on a level surface, 7.6 m (25 ft) in front of a test surface (wall or screen) as in first illustration.

3. Measure the distance from the center of each headlight to the ground (high beam and low beam).

4. Trace a line on the test surface parallel to the ground at each measured height (one for high beam and one for low beam).

Low beam aiming is correct when the cutoff at the top of the beam is on the applicable horizontal center line on the test surface.

High beam aiming is correct when the center of the high beam (focus point) is 33 mm (1-5/16 in) above the applicable horizontal center line traced on the test surface as per specification.

NOTE: The headlights can only be adjusted vertically.
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1. High beam focus point

A. Distance between headlight and the test surface

B. Beam aiming specification

5. Turn adjustment screw to adjust the headlight as needed.

Installation

For installation, reverse the removal procedure.

12.5.2 Tail light
Removal
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- Remove the rear cover board from the vehicle. 

- Disconnect light connector.
- Loose the three M6 bolts and nut, then remove the taillights.
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· Loose the 11 screws (ST4.2), then remove the rear penetration light.

Installation

For installation, reverse the removal procedure.

12.5.3 License plate light
Removal
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- Disconnect license plate light connector.

- Loose the two M5 bolts and nut, then remove the license plate light.

Installation

For installation, reverse the removal procedure.

Tightening torque of M6 bolt: 9~12 Nm.

Tightening torque of M5 screw: 5~9 Nm.
12.5.4 Rear fog light (if equiped)
Loose the M6 bolts and nut, then remove therear fog light from frame.
Installation

For installation, reverse the removal procedure.

Tightening torque of M6 screw: 9~12 Nm.
12.5.5 Tailer power
Loose the M5 bolts and nut, then remove the trailer power from frame.
Installation

For installation, reverse the removal procedure.

Tightening torque of M5 screw: 5~9 Nm.
12.6 Cooling System
IF THE FAN MOTOR FAILS TO TURN
Inspection
1. Fan fuse
Check fan fuse. If not continuity, replace the fuse.
2. Battery
Check the battery condition refer to Battery Inspection in this section. If battery is incorrect, as following:
- Clean battery terminals.
- Recharge or replace the battery
3. Fan relay

Check fan relay. If not continuity, replace the relay.

4. Ignition switch
Check ignition switch for continuity or not. If it not continuity, replace the ignition switch.
5. Fan motor
Connect the battery to the fan motor. Check the fan motor operation. If does not move, replace the fan motor.
6. Thermostat switch

Remove the thermostat switch from the radiator.

Connect the pocket tester (ΩX1) to the thermostat switch(.

- Immerse the thermostat switch in the water (
- Check the thermostat switch for continuity.

NOTE: Measure temperatures while heating the coolant with the temperature gauge
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NOTICE:
· Handle the thermostat switch with special care.

Never subject it to strong shocks or allow it to be dropped. Should it be dropped, it must be replaced.

· Do not touch the thermostat switch to the bottom of the heated vessel.

88±3℃--Thermostat switch “ON”

80℃--Thermostat switch “OFF”

If out of specification, replace the thermostat switch.
7. Wiring connection

- Check the connection of the entire cooling system. Refer to the circuit diagram. If incorrect, replace the wiring connection.

12.7 Fuses
Removal
Remove the dash board cover, refer to Dismantling.

Remove the two bolts and fuse box.
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Tightening torque of M6 bolt for fuse box: 9~12 Nm.

Fuse Inspection 

Check fuse condition and replace it if necessary.

To remove fuse from holder, pull fuse out. Check if filament is melted.
Fuse description
	F1
	Ignition Switch
	15 A

	F2
	Combination Switch
	15 A

	F3
	2WD/4WD Switch
	10 A

	F4
	Winch
	5 A

	F5
	Fan
	30 A

	F6
	Backup power
	20 A

	F7
	EFI
	20 A

	F8
	Light power supply
	15 A


12.8 Relay
Ensure to align tabs of relay with terminals of fuse holder at installation.
The easiest way to check a relay is remove it and bypass it with a jumper. If the components then work, replace the relay. See illustration to find where to bypass the relays.
	Relays
	RY 1
	Light Relay

	
	RY 2
	Combination Switch Relay

	
	RY 3
	EFI Relay

	
	RY 4
	2WD/4WD Switch Relay 1

	
	RY 5
	2WD/4WD Switch Relay 2

	
	RY 6
	Fan Relay

	
	RY 7
	Fuel Pump Relay

	
	RY 8
	Handlebar Heating Relay

	
	RY 9
	Overtaking light Relay

	
	RY 10
	Right trailer steering Relay

	
	RY 11
	Left trailer steering Relay

	
	RY 12
	Rear fog light Relay


12.9 Speedmeter System

Operation Of Speed Sensor
Speed sensor on the gearbox output shaft.
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The following is the graphic illustration for sensor installation
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Turn ignition key ON.
Set engine run/ stop switch to RUN.
Use a multimeter and set it to Vdc.
Back-probe connector and read voltage as follows.
	Speed Sensor Conntector
(harness side)
	Voltage

	White/Blue
	Red
	Battery voltage


If voltage is not good, check/ repair wiring/connectors.
If voltage is good, do the following test.
Lift rear of vehicle so that rear wheels are off the ground.
Set transmission to 2WD and to Neutral.
Back-probe connector and read voltage while slowly rotating rear wheels with your hands.
If voltage is appropriate, check/repair wiring/ connector between sensor and BCM. If it is good, try a new BCM.
If voltage is wrong, try a new sensor.
12.10 Gear Position Indicator Switch 
Check the gear position sensor as following:
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The gear position sensor fuction:
	
	E
	P
	R
	N
	H
	L

	P
	●
	●
	
	
	
	

	R
	●
	
	●
	
	
	

	N
	●
	
	
	●
	
	

	H
	●
	
	
	
	●
	

	L
	●
	
	
	
	
	●

	Wires color
	
	Pink
	R/W
	Lg/R
	L/R
	G/B


12.11 Oil Pressure Sensor
Switch Activation
When oil pressure is high than 13kPa, the switch is cut off. 
When oil pressure is lower than 13kPa, the switch is connected. 
Removal

Unplug and unscrew the oil pressure sensor. This  sensor is located in the area between cylinder head and gearbox shift shaft.
Installation 
Apply Loctite 234(blue) and torque switch to
9~12 Nm.

12.12 2WD/4WD Switch/Diff Lock Switch
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1. The rider shifts by the Switch on handlebar.

2. The Switch gives signal to Controller.

3. The controller gives power to the solenoid.

During this time, the 4WD/Diff lock indicator is not on, this requires the rider to back or move (ride) the ATV a little to allow the Dog change position for engagement. 
The switch position sensor fuction:

[image: image363.png]Wire
olor

Functio

Grey / white

Blue / Black

Brown / re

Blue / Green

Light gree
/ Brown

Brown /
Green

black

dh

yellow

HOCK

alla]

red

WD

O

O

O

O

[allla]

yellow

AW,

dh

red

F2W0

()
/

[l

vellow

A WQ

e}

red

HAWQ

Olo

O

O 10





Troubleshooting

Inspection

1. Fuse
Check 2WD/4WD switch for continuity or not. If it not continuity, replace the fuse.
2. Battery
Check the battery condition refer to Battery Inspection in this section. If battery is incorrect, as following:
Clean battery terminals.
Recharge or replace the battery.
3. Ignition switch
Check ignition switch for continuity or not. If it not continuity, replace the ignition switch.
4. 4WD/Diff lock switch
Check the operation of 4WD/Diff lock switch.
If not continuity, replace the switch.
5. Solenoid Switch

Disconnect solenoid switch from the wire harness
Connect the solenoid to the battery.
Battery(+) lead        Red/brown terminal  
Battery(-) lead       Black ground

If the switch does not move, replace the solenoid switch.
6. Wiring connection
- Check the connection of the entire ignition system.
Refer to the wires diagram.
If it correct, replace the ECU.
12.13 2WD/4WD Motor
Use a multimeter and set it to Vdc.
Measure the voltage as following.
	Wires
	Voltage

	Light green/Red and White/Red
	Battery voltage


12.14 Multifunction Gauge

GENERAL

Most of the electrical tests require the following tool.
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Refer to Wires Diagram subsection for diagnostic tips on troubleshooting electrical problems.

NOTICE： It is recommended to always disconnect the battery when replacing any electrical component. Always disconnect battery as specified, BLACK (-) cable first.

INDICATOR LAMPS DESCRIPTION
Important information about vehicle condition is displayed on the multifunction gauge. When starting the engine, always look at the gauge for any indicator lamps or special messages.

Important information messages can also be displayed by assist indicator lamps.
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NOTE: Depending on the vehicle, not all the indicator lamps and messages will be applicable.
	Item
	Function
	Icon

	1
	Left turn
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	2
	Right turn
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	3
	Position light
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	4
	High beam
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	5
	Low beam
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	6
	Engine fault
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	7
	EPS
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	8
	ABS fault
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	9
	Brake fault
	[image: image374.png]




	10
	Oil change
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	11
	Trailer indicator light
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	12
	Handbrake activation
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	13
	Speed limit
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TROUBLESHOOTING 

DIAGNOSTIC TIPS 
IMPORTANT: When solving an electrical problem, the first thing to do is to check the battery condition as well as its cables and connections. Make sure the battery is fully charged or install a power pack for any tests that involves a prolonged "key ON" period. If battery voltage gets too low, not only test results can be altered, but the vehicle electrical system may not operate normally. Pay attention to ground wires. They could become loose or corroded which causes them to act as an additional load in a circuit, dropping voltage and reducing current to components. Some components may be grounded through their outer casing and mounted hardware. This should also be considered. 

Electrical Connectors
Pay particular attention to ensure that pins are not out of their connectors, loose, or damaged. The troubleshooting procedures may not cover problems resulting from one of these causes.

NOTICE: Ensure all terminals are properly crimped on wires and connect or housings are properly fastened. When replacing any electric or electronic part(s), always check electrical connections. Make sure that they are clean, 

corrosion-free, tight and make good contact. The voltage and current might be too weak to go through dirty or corroded connector pins or terminals.

MULTIFUNCTION GAUGE TROUBLESHOOTING 
GAUGE FUNCTIONS INOPERATIVE OR WORKING INTERMITTENTLY             
1. Power supply or ground problem

- Check power supply and ground circuits.

PROCEDURES
Testing the Multifunction Gauge
Before beginning any troubleshooting, test or repair, always check for fault codes.

1. Check for fault codes using DELPHI DIAGNOSTIC TOOL.

2. Record all fault codes, then erase them.

3. Perform a complete shutdown of the electrical system and reactivate it.

4. Check fault codes. If a previous fault code reappears, perform the required service actions.

Testing the Multifunction Gauge Using DELPHI DIAGNOSTIC TOOL
Connect the DELPHI DIAGNOSTIC TOOL to OBD.

In DELPHI DIAGNOSTIC TOOL, go to:

- Functions page

- Cluster button

- Routines-Execute Cluster WOW test.

All indications will come and stay ON so that you can verify each indication.

NOTE: The WOW Test only tests the gauge LEDs and LCD. It does not test the actual circuit functions related to each indication.

Testing the Multifunction Gauge Power Input
If the multifunction gauge is inoperative, first check for fault codes with DELPHI DIAGNOSTIC TOOL, record all faults then erase them. Reactivate the electrical system and recheck for faults. If any fault code appears, perform service actions required. 

1. Remove multifunction gauge.

2. Perform the test at multifunction gauge connector as per following illustration and tables.

If there is no power at pin 9(Black), check fuse and the related circuit.

If the power test is within specification, continue with TESTING THE MULTIFUNCTION GAUGE GROUND CIRCUIT.

Testing the Multifunction Gauge Ground Circuit
Test as per the following table.
If the ground at pin 9 (Black) is not within specification, check the related circuit.

If the ground tested to specification, continue with TESTING THE MULTIFUNCTION GAUGECAN WIRE CIRCUIT.
Testing the Multifunction Gauge CAN Circuit
1. Remove the front service cover for access to the OBD. Refer to BODY subsection.
2. Test as per the following table.

	Multifunction Gauge CAN WIRE TEST

	CL Connector
	OBD
	Results

	Pin7 Pink
 (CAN L)
	Pin 4 (Black)
	Close to 0.4Ω

	Pin8 Purple
(CAN H)
	
	Close to 0.4Ω


If the CAN wire verification test fails, check the related circuit.

If the multifunction gauge functions, however there is a suspected communication problem with another component, perform this test between the multifunction gauge and that component.

If the multifunction gauge power, ground and CAN verification tests are all to specifications and the multifunction gauge is inoperative, replace the multifunction gauge.

Removing the Multifunction Gauge
Remove gauge cover. Refer to procedure in BODY subsection

Disconnect the gauge connector. Remove following fasteners.

1. Loosen two M6 screws, disconnect the wires from gauge. 
2. Remove gauge cover from gauge cover bracket. 
3. Loosen M6 screws, separate gauge cover and gauge. 
Installing the Multifunction Gauge
The installation is the reverse of the removal procedure. However, pay attention to the following.
	TIGHTENING TORQUE

	Gauge screws
	9~12 Nm


If the multifunction gauge was replaced, connect the vehicle to the DELPHI DIAGNOSTIC TOOL and apply any available updates. Also set the odometer reading, engine hours, time language the menu on the gauge.
Menu settings
Buzzer alarm: Sound alarm is triggered based on the vehicle status.

Text-based alarm: Text-based alarms include:

	Item
	Text-based alarm

	1
	Reset maintenance mileage

	2
	The parking brake is released.


Reset Maintenance Mileage:

When the remaining maintenance mileage is 0 km, a pop-up window prompts for a reset operation. Clicking the "Yes" button resets the maintenance mileage; clicking the "No" button does not reset the maintenance mileage (the pop-up window is canceled), and a pop-up window will prompt again after restarting the device.
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SETTING

Menu entry and exit: Click the area within the square on the screen to display the menu settings items.
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In the menu area, simply swipe up and down to scroll through the menu options.

Click on any area other than the menu to exit the menu.
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Backlight: Backlight adjustment mode, backlight brightness value setting.

The backlight adjustment modes are: manual/automatic.
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In automatic mode, the backlight brightness of the screen is automatically switched.

In manual mode, the manual adjustment range of brightness is: 1~100. 1 is the darkest and 100 is the brightest.

In manual mode, the backlight brightness values when the near light is turned on and off can be set and memorized separately. [image: image384.png]Backlight A
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Tire diameter: You can set the option for tire diameter. After setting, it will be remembered.
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EPS gear position: EPS gear position options can be set. After setting, it will be memorized.
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Clock: Set and remember the clock mode (24-hour format, 12-hour format); adjust the time.
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Language: Settings and memory for Chinese, English, or other languages.
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Unit: Set and memorize metric and imperial units.
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Fault Code: When the vehicle has a specific fault, the fault code will be displayed.
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Maintenance Information: Displays the remaining mileage until the next scheduled maintenance. The reminder for the first maintenance is at 500 km, and the subsequent intervals are 2000 km.
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Vehicle Information: Displays the total working time since the vehicle was started.
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Version: Displays the current software (MCU, APP) version and hardware (HW) version number of the instrument.
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12.15 12-Volt Auxilary Power Outlet
The 12-volt auxiliary power outlet allows the installation of additional accessories.

Test

The wires are located on the USB holder.
NOTE: Turn ignition key ON.

Using a multimeter, measure the voltage between White/Green and Black wires.

The obtained value should be between 12 and 14.5 Vdc.

- No voltage:

● Check wiring condition.

- Voltage is good:

● Check accessories.
12.16 12-Volt Power Outlet
Removal

Remove USB holder. Refer to BODY.

Unplug the connectors of the power outlet.

Unscrew the retaining nut.

Installation

Reverse the removal procedure.

Test

NOTE: No key required.

Remove the USB holder.
Unplug the power outlet connectors.

Using a multimeter, measure the voltage between White/Blue and Black wires.

The obtained value should be between 12 and 14.5 Vdc.

- No voltage:

Check accessories fuse (15 A) and wiring condition.

- Voltage is good:

Change power outlet.
12.17 Multifunction Switch
Apply parking brake lever, place shift lever to NETURAL position and start engine.

Low/Hi Beam Switch
Select low beam position on switch.

Using a multimeter, measure the voltage between GREEN and BLACK wires.

The value should be between 12 and 14.5 Vdc.
Select low beam position on switch.

Using a multimeter, measure the voltage between BULE and BLACK wires.

The value should be between 12 and 14.5 Vdc.
- No voltage 

●Check switch and wiring condition.

- Voltage is good:

●Change headlight bulb.
Using a multimeter, measure the resistance between the following wires.
	Switch Position
	Wire Color
	Resistance

	Hi Beam
	White/
Brown
	Black/Brown
	0.2±0.2Ωmax.

	Lo Beam
	Bule/
Brown
	Black/Brown
	0.2±0.2Ωmax.


Replace Low/Hi beam switch if defective.
Start/Stop Switch
Using a multimeter, measure the resistance between the following wires.
	Ignition Switch 
	Wire Color
	Resistance

	ON position
	Black/White

 And 
Grey red
	 0.2±0.2Ωmax.

	OFF position
	
	Infinite (0L)


Replace power switch if defective.
Horn Switch

Using a multimeter, measure the resistance between the following wires.
	Switch 
	Wire Color
	Resistance

	ON position
	Black/Brown
 And
 Light green
	 0.2±0.2Ωmax.

	OFF position
	
	Infinite (0L)


Replace horn switch if defective.
Override Switch
Using a multimeter, measure the resistance between the following wires.
	Switch 
	Wire Color
	Resistance

	Override switch pushed
	Blue and White/blue
	 Infinite (0L)

	Override switch released
	Grey/Black and White/blue
	0.2±0.2Ωmax.


Replace driving light switch if defective.
Steering signal switch
Using a multimeter, measure the resistance between the following wires.
	Switch 
	Wire Color
	Resistance

	Left position
	Orange
 And Grey
	0.2±0.2Ωmax.

	Right position
	Orange

 And Light blue
	0.2±0.2Ωmax.


Replace steering signal switch if defective.
Warning lights switch
Using a multimeter, measure the resistance between the following wires.

	Switch 
	Wire Color
	Resistance

	ON position
	Black

 And Grey/Black
	 0.2±0.2Ωmax.

	OFF position
	
	Infinite (0L)


Replace warning light switch if defective.
12.18 Winch
Test
Winch Motor

Using boosting cables, connecter pore to IN post of winch the to OUT post.

If motor does not turn in any test, replace motor. If it works, continue testing.
Voltage Supply to Switch

Remove front panel and dashboard. Refer to BODY.
Disconnect the winch control switch connector.
Using a multimeter, measure the resistance as follows.
	Winch Switch Connector

(harness side)
	Voltage

	Pin A
	Battery ground
	12 Vac


If there is no voltage, check fuses, relay and wiring condition.
If there is voltage, test switch as follows.
Winch Control Switch
Removal

Remove screws retaining winch control switch to handlebar.
Remove steering cover, refer to BODY.
Disconnect the winch control switch connector.
Remove steering cover, refer to BODY.
Disconnect the winch control switch connector.
Using a multimeter, measure the resistance.
	Position
	Connector Pin
	Resistance

	Switch to IN
	Blue and Brown
	< 5Ω

	Switch to OUT
	Brown and yellow
	< 5Ω


If the resistance is above 5 Ω, replace the winch control switch. 
Installation

For the installation, reverse the removal procedure.
Winch Relay

Reconnect terminals at winch relay.
Measure voltage drop between relay and motor as follows.
	Position
	Relay terminal
	Voltage Drop

	Switch pressed to IN and held
	Battery post and IN cable
	0.2 Vdc max.

	Switch pressed to OUT and held
	Battery post and OUT cable
	0.2 Vdc max.


If voltage drop read is higher than specification in either test, check wiring/connectors. If they are good, replace winch relay.
If voltage read is battery voltage, the relay does not close. Replace with a new one.
Removal

Disconnect, the battery BLACK (-) cable first, then the RED (+) cable.
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WARNING

	Always respect this order for disassembly; disconnect BLACK (-) cable first. Electrolyte or fuel vapors can be present in engine compartment and a spark may ignite them and possibly cause personal injuries.



Disconnect the winch power cables.
NOTE: Note the position of the power cables for reinstallation.
Remove:
- locking pin
- hook
- bolts retaining the winch from both LH and RH sides.
Remove winch.
Installation
For the installation, reverse the removal procedure.
12.19 Engine Modes Selector
Steering signal switch
Using a multimeter, measure the resistance between the following wires.
	Switch 
	Wire Color
	Resistance

	STND position
	Purple/Red
 And Black
	Infinite (0L)

	SPRT position
	
	0.2±0.2Ωmax.


Replace engine modes selector if defective.
12.20 EPS Controller
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1. Motor drive module(Motor side)
2. Motor drive module(Battery side)
3. Analog/digital conversion
4. Control module
The wires diagram is as following:
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TEST

EPS Power Test

Using a multimeter, measure the voltage as follows.
	EPS Connector
	Voltage

	Control Module
	Motor Drive Module
	

	Pin 1 (Red)
	Pin1 (Black)
	12 Vac


If there is no voltage, check fuses, relay and wiring condition.
EPS CAN Resistance Test

Using a multimeter, measure the resistance as follows.
	EPS Connector
	Resistance

	Control Module
	

	Pin 4 (Blue/red)
	Pin8 (Pink)
	55Ω


13. TROUBLESHOOTING
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ELECTRICAL SYSTEM

Symptom: NO SPARK OR POOR SPARK
1. Refer to ignition system.
Symptom: STARTER DOES NOT TURN
1.
Refer to starting system.
Symptom: STARTER TURNS BUT DOES NOT CRANK THE ENGINE
1.
Refer to starting system.

2.
Check gear condition on electric starter.


Worn and/or damaged starter gear. Replace electric starter and/or starter drive.

3.
Check condition of starter pinion gear.


Worn and/or damaged starter pinion and/or ring gear. Replace starter drive and/or drive pulley fixed sheave.

4.
Check splines on starter drive.


Poor movement of pinion gear on splines. Clean and/or replace starter drive.

Symptom: STARTER TURNS BUT STARTER DRIVE DOES NOT MESH WITH RING GEAR

1.
Refer to Starting System.

Symptom: STARTER KEEPS RUNNING

1.
Refer to Starting System.

COOLING SYSTEM

Symptom: HIGH ENGINE OPERATING TEMPERATURE

1.
Check coolant level.


Coolant level lower than recommended. Refill (refer to Cooling System).

2.
Check for air bubbles in cooling system.


Air in cooling system. Refill and bleed cooling system (refer to Cooling System).

3.
Check temperature sensor for electrical/mechanical failure.


Temperature sensor defective. Replace.

4.
Check thermostat.


Thermostat defective (does not open when engine gets hot). Replace (refer to Cooling System).

5.
 Check leak indicator hole (in crankcase MAG side-water pump housing area) if coolant leaks.


Coolant leaking from indicator hole means a damaged water pump rotary seal. Replace rotary seal (refer to Cooling System).

6.
Check condition of hoses and hose clamps fixation.


Hoses are brittle and/or hard. Replace.


Hose clamps are loose. Retighten clamps.

7.
Check condition of impeller located on the water pump shaft.


Impeller wirings broken and/or impeller threads are damaged. Replace (refer to cooling system).

8.
Check gasket on water pump housing.


Gasket on water pump housing leaks. Retighten screws and/or replace gasket.

9.
Check cylinder head and/or cylinder base gasket.


Worn out gasket(s) is (are) causing coolant leakage. Replace.

10.
Check coolant drain screw on water pump housing MAG side.


Copper ring on drain screw leaks. Retighten screw and/or replace copper ring.

11.
Check intermediate gear(s) behind of PTO cover.


Worn out and/or broken gear(s) is/are causing less coolant supply. Replace worn out and/or broken gear(s) (refer to Bottom End).

12.
Check if water pump shaft is seized.


Water pump shaft does not turn. Replace defective part(s).

13.
Check cooling fan and connection.


Fan motor faulty. Replace.


Wire harness is brittle or hard (no connection). Replace.

14.
Check radiator fan switch and fuse.


Faulty fan switch and/or faulty fuse. Replace defective part(s).

15.
Check radiator condition for leakage.


Radiator cracked or deformed. Replace radiator.

16.
Check mud/dust in radiator fins.


Radiator fin obstructed, hard air cooling. Clean radiator fins.

MAGNETO SYSTEM

Symptom: BATTERY NOT CHARGING OR CHARGING VOLTAGE INADQUATE

1.
Check battery


Battery shows less power. Reload battery.

2.
Check magneto for damage and/or electrical failure.


Radial position of rotor wrong due to broken woodruff key. Replace woodruff key.


Coating on stator winding is damaged. Replace stator.


Resistance value is out of specification (refer to technical specifications). Replace magneto.


Connector on magneto is damaged and/or has electrical failure. Repair and clean contacts of connector.

3.
Check voltage regulator/rectifier.


Refer to Charging System.

4.
Check wiring harness for cracks or other damages.


Harness shows electrical failure and/or other damages. Replace/repair wiring harness.

LUBRICATION

Symptom: LOW OR NO OIL PRESSURE/HIGH OIL CONSUMPTION

1.
Check oil level and search for leakage on crankcase and/or sealing parts.


Crankcase is leaking due to damage. Rebuild engine with new crankcase and gasket parts. Use recommended oil (refer to Technical Specifications).


Crankcase is leaking due to loosen screws. Retighten screws with recommended torque


Sealing rings, O-rings and/or gaskets are brittle, hard or damaged. Replace damaged parts.


Poston rings worn out (blue colored engine exhaust emission). Replace piston rings (refer to Cylinder and Head).


Piston rings are broken (low compression). Replace piston rings (refer to Cylinder and Head).


Valve stem seal damaged and/or sealing lip is hard and/or brittle. Replace all valve stem seals.

2.
Check oil filter for contamination.


Oil filter clogged. Replace oil and oil filter at the same time. Use recommended oil (refer to Technical Specifications).

3.
Check oil drain plug on engine bottom.


Plug is loose and/or gasket ring is missing. Retighten the plug and/or place gasket ring.

4.
Check leak indicator hole if oil leaks (in crankcase MAG side-water pump housing area).


Oil leaking from leak indicator hole means a damaged oil seal on water pump shaft. Replace oil seal (refer to Cooling System).

5.
Check oil pressure switch function.


Oil pressure switch damaged. Replace oil pressure switch.

6.
Check oil orifice(s) on the oil pump suction side.


Oil orifice(s) is (are) clogged. Clean from contamination. Replace oil and oil filter if necessary (refer to maintenance or lubrication system).

7.
Check oil pump function.


Oil pump rotor is out of wear limit. Replace oil pump (refer to lubrication system).


Oil pump seized due to oil leakage and/or air inclusion. Replace oil pump (refer to lubrication system).


Gears driving oil pump are broken or otherwise damaged. Replace gears.


Incorrect oil being used. Use recommended oil (refer to technical specifications).

8.
Check oil pressure regulator valve (spring) function.


Valve spring damaged (valve always open). Replace spring.


Valve piston is worn or broken. Replace valve piston (refer to lubrication system).


Valve piston stays open due to contamination. Clean or repair valve piston.

9.
Check plain bearings in crankcase for heavy wear.


Plain bearings out of specification (increased clearance). Replace plain bearings (refer to bottom end).

10.
Check engine oil strainer in crankcase.


Oil strainer is clogged due to contamination. Clean or replace strainer and diagnose causes. Replace possible damaged parts (refer to bottom end).

Symptom: OIL CONTAMINATION (white appearance)

1.
Check leak indicator hole (in crankcase MAG side-water pump housing area) if water and oil leaks.


Leakage of oil/water mixture from indicator bore means damaged water pump seal ring and rotary seal. Replace sealing ring, rotary seal and change oil, oil filter and/or coolant (refer to lubrication system, cooling system and bottom end).

2.
Check cylinder head and/or cylinder base gasket.


Gasket damaged or leaking. Retighten cylinder head with recommended torque and/or replace gasket.

3.
Check tightening torque of cylinder head screws.


Screws not properly tightened. Retighten screws to recommended torque and replace oil. 

4.
Check oil for particles (may indicate possible engine internal damages).


Oil contamination due to metal or plastic particles. Replace possibly damaged part(s) including oil and oil filter. Use recommended oil (refer to technical specifications).

CYLINDER AND HEAD

Symptom: UNUSUAL ENGINE NOISE AND/OR VIBRATION

1.
Check noise coming from cylinder head area.


Improper valve clearance adjustment. Readjust valve clearance and/or replace defective part(s).


Faulty chain tensioner. Replace spring and/or mechanism.


Chain guide worn out. Replace chain guide.


Stretched chain and/or worn-out sprockets. Replace chain and sprockets.


Sprocket screws got loose. Retighten screws with recommended torque. 


Rocker arm(s) is (are) worn out (valve adjustment). Readjust valve clearance and/or replace rocker arm(s).


Incorrect camshaft timing adjustment. Replace damaged components and readjust camshaft timing (refer to cylinder and head).

Symptom: OIL CONTANMINATION ON CYLINDER AND/OR HEAD

1.
Check screws for torque.


Loose screws. Retighten screws with recommended torque.


Gaskets are brittle, hard, worn out or otherwise damaged. Replace damaged gaskets, O-rings.
CRANKSHAFT AND BALANCER SHAFT
Symptom: UNUSUAL ENGINE NOISE AND/OR VIBRATION

1.  Check noise coming from crankshaft area.


Crankshaft plain bearings are damaged. Replace crankshaft plain bearings.


Connecting rod plain bearings are damaged. Replace connecting rod plain bearings.


Magneto rotor got loose. Replace damaged components and retighten rotor retaining screw with recommended torque (refer to MAGNETO SYSTEM).
           2. Check ball bearing on balancer shaft end
                      Ball bearing do not move freely. Replace bearing.
           3.Check that mark on blance shaft aligned with crankshaft position mark.
GEARBOX

Symptom: UNUSUAL GEARBOX NOISE AND/OR VIBRATION

1.
Check oil level in gearbox.


Oil leakage from gearbox. Replace damaged gasket(s) and/or oil seal(s), torque screws and refill with oil up to specified level (refer to TECHNICAL SPECIFICATIONS and GEARBOX)

2.
Check bearings in the gearbox for free movement.


Bearing(s) do(es) not move freely. Replace bearing(s)

3.
Check for knocking noise.


Tooth of gears are damaged and/or worn. Replace respective gears.

Symptom: GEAR INDICATION FAILS.

1.
Check contact screws on gear housing center.


Check contact screw outside for contamination and wetness. Clean contact screw and screw for wiring harness.


Contact(s) is (are) corroded and/or contact screw for wiring harness got loose. Clean contact surface and retighten contact screw(s) with recommended torque.


Wiring harness has broken cables. Replace wiring harness.


Shifting indicator switch(es) pin(s) is (are) worn and/or damaged. Replace shifting indicator switch(es).

Symptom: GEAR(S) IS (ARE) HARD TO SHIFT

1.
Check shift shaft splines and/or shift forks for wear and/or damages.


Shift shaft is worn out and/or shows damaged splines. Replace shift shaft.


Shift drum track(s) and/or splines is (are) worn out or damaged. Replace shift drum and damaged part(s).


Shift fork(s) is (are) worn out and/or engagement pins are damaged. Replace shift fork(s).


Shift fork(s) is (are) worn out and/or fork(s) is (are) damaged. Replace shift fork(s).


Shift gear(s) is (are) worn out. Replace shift gear(s).


Shifting indicator switch(es) pin(s) is (are) worn out (no rounding on top of pin). Replace shifting indicator switch(es).

2.
Check engine idle speed.


Check throttle cable and throttle adjustment.


Check bypass idle valve and connectors.

3.
Check CVT one way clutch on drive pulley.


CVT one way clutch was not lubricated correctly. Lubricate CVT one way clutch (refer to CONTINUOUSLY VARBRIABLE TRANSMISSION (CVT)).


CVT one way clutch is worn out or damaged. Replace defective part(s) (refer to CONTINUOUSLY VARBRIABLE TRANSMISSION (CVT)).


Check if friction washer at one way clutch is worn. Replace friction washer (refer to CONTINUOUSLY VARBRIABLE TRANSMISSION (CVT)).

4.
Check transmission lever and connecting rod.


Ball joint and/or ball joint nut is (are) loose. Retighten or replace the ball joint.

5.
Check spring on shift shaft in gearbox.


Broken spring. Replace the spring (refer to GEARBOX).

6.
Check for any mud intrusions.
CVT parts dirty. Clean all CVT parts.

COUPLING UNIT

Symptom: 4 WHEEL DRIVE INDICATION FAILS

1.
Check contact screw on gear housing right side for damage and/or wear.


Shifting indicator switch pin is worn and/or damaged. Replace shifting indicator switch.


Contact is corroded and/or contact screw for wiring harness got loose. Clean contact surface and retighten contact screw with recommended torque.


Wiring harness has broken cable. Replace wiring harness.

Symptom: 4 WHEEL DRIVE DOES NOT ENGAGE OR DISENGAGE

1.
Check actuator and/or actuator shifting fork for wear and/or damages.


Check if selector works properly. If so, check actuator.


If selector is out of specifications, check wires, connectors and/or replace selector.


Actuator shifting fork is worn out and/or damaged. Replace shifting fork of actuator.


Check function of actuator. Replace if actuator is not turning, refer to GEARBOX.

2.
Check shifting sleeve splines and/or shifting fork for wear and/or damages.


Check sleeve shows damaged splines. Replace shifting sleeve (refer to GEARBOX).


Shifting fork is worn out and/or engagement pin is damaged. Replace shifting fork.

CVT 

Symptom: UNUSUAL ACCELERATION BEHAVIOR

1.
Check drive belt condition.


Belt is too narrow (drive belt engagement is higher in drive pulley). Replace belt if width is less than specified.

2.
Check lever condition on drive pulley sliding sheave and/or roller(s) on governor cup.


Lever(s) on drive pulley sliding sheave is (are) worn and/or damaged. Replace all levers at the same time (lever kit).


Roller(s) is (are) worn and/or damaged. Replace governor cup assembly.

3.
Check drive/driven pulley sliding sheave for free axial movement.


Sliding sheave is stuck. Replace damaged part(s).

4.
Check condition of drive/driven pulley spring.


Drive pulley spring tension is too smooth and/or damaged. Replace spring.


Driven pulley spring tension is too stiff. Replace spring.

5.
Check if cam of driven pulley is worn.

Replace if out of specifications.

6.
Check condition of fixed and sliding sheaves (drive and driven pulley).


Check surface of fixed and sliding sheaves (drive and driven pulley) for grooves or other damages.

7.
Check valve adjustment.


Intake and/or exhaust valves are not adjusted correctly. Adjust valves.

8.
Check engine condition.


Low engine compression.

9.
Check ignition condition.


Faulty spark plug. Install new spark plug(s).

10.
Check differentials operation.


Vehicle on Neutral is hard to move. Repair or replace defective part(s).
11. Check with Diagnotisc Tool for failure.
                    Repair or replace defective part.

Symptom: ENGINE MAXIMUM RPM IS TOO HIGH AND VEHICLE TOP SPEED IS NOT REACHED.

1.
Check drive/driven pulley area for contamination and/or water intrusion.


CVT area is contaminated with water, dirt or oil. Clean CVT system and replace damaged part(s).

2.
Check drive/driven pulley spring tension.


Drive pulley spring tension is too stiff. Replace spring.


Driven pulley spring tension is too smooth and/or damaged. Replace spring. 
3.  Check drive/driven pulley area for contamination and/or water intrusion.
          CVT area is contaminated with water, dirt or oil. Clean CVT system and replace damaged parts.
Symptom: DRIVE PULLEY NOISE IN IDLE SPEED

1.
Check slider shoes (drive pulley).


Worn slider shoes (increased clearance between governor cup and drive pulley sliding sheave). Replace all slider shoes at the same time (slider shoes kit).

2.
Check driven pulley sliding mechanism (between driven pulley outer and inner sheave).


Mechanism is stuck and/or damaged. Replace driven pulley assembly.

3.
Check roller(s) and/or levers for wear (located on sliding sheave of drive pulley).


Roller(s) on governor cup is (are) worn out and/or damaged. Replace governor cup assembly.


Lever(s) on drive pulley sliding sheave is (are) worn out and/or damaged. Replace all levers at the same time (lever kit). 

4.
Check drive pulley screw for torque.


Loose screw. Retighten screw with recommended torque.

5.
Check one-way clutch condition on drive pulley sliding sheave.


Bearing(s) do(es) not move freely. Replace damaged part(s) and lubricate inside of one-way clutch.


Spring sleeve(s) inside one-way clutch is (are) worn out. Replace both sleeves and springs and lubricate inside of one-way clutch.


Spring(s) inside one-way clutch is (are) worn out. Replace both pins and springs and lubricate inside of one-way clutch.

Symptom: DRIVE PULLEY NOISE WHEN ACCELERATING/DECELERATING

1.
Check if belt runs in dry condition.


Drive pulley area is wet/contaminated due to water/dirt intrusion. Clean driven pulley area and/or drain water out of CVT cover.

2.
Check drive/driven pulley screw for torque.


Loose screw on drive pulley. Retighten screw with recommended torque.

3.
Check cam and driven pulley fixed sheave for wear.


Cam and/or drive pulley fixed sheave out of wear limit and/or damaged. Replace damaged part(s).

4.
Check torque gear fixed in driven pulley sliding sheave for wear.


Torque gear out of wear limit and/or damaged. Replace torque gear).

5.
Check for foreign particles in CVT area (stones, dirt, etc.).


Small particles damaged belt and/or pulley surface(s). clean system and replace damaged parts.

Symptom: VIBRATIONS ORIGINATING FROM DRIVE PULLEY

1.
Check tightening torque of drive pulley screw.


Moving sliding sheave. Retighten screw.

2.
Check fixed sheave bushings.


Excessive gap between bushings and fixed sheave shaft, thus restraining sliding sheave movements. Replace fixed sheave assembly.

3.
Check if slider shoes are present and/or placed in correct position.


Slider shoe(s) is (are) missing and/or damaged. Replace all slider shoes at the same time (slider shoes kit).

Symptom: VIBRATIONS ORIGINATING FROM DRIVEN PULLEY

1.
Check fixed and sliding sheave bushings on driven pulley.


Excessive gap between bushings and CVT shaft, thus restraining sliding sheave movements. Replace fixed and/or sliding sheave of driven pulley, polish CVT shaft area with fine emery cloth and wipe clean with a cloth.

Symptom: PULLEYS DO NOT DOWN/UP SHIFT PROPERLY.

1.
Check drive pulley bushings (cleanliness, wear, etc.)


Check items 1 and 2 of UNUSUAL ACCELERATION BEHAVIOR.


Bushings stick to fixed sheave pulley shaft. Clean or replace.


Spring seat sticks to sliding sheave pulley bushing. Clean system and/or replace sliding sheave pulley.


One-way clutch does not operate properly. Clean system and/or replace damaged part(s).

2.
Check driven pulley spring tension.


Driven pulley spring tension is too weak or broken. Replace.


Driven pulley cam is worn or damaged. Replace.

Symptom: BELT GLAZED EXCESSIVELY OR HAVING BAKED APPEARANCE

1.
Check if CVT air intake and/or outlet is clogged.


CVT area heats up due to contamination. Clean air intake and/or outlet from contamination.


Fans located on drive pulley is worn or damaged. Replace.

2.
Check if pulley sheaves are clean.


Oil on pulley surfaces. Clean pulley sheaves and replace belt.


Water intrusion in CVT area. Find root cause and repair. Drain water and replace belt.

Symptom: BELT WORN EXCESSIVELY IN TOP WIDTH.

1.
Check drive belt width.


Considerable wear. Replace belt if narrower than specified (refer to CONTINUOUSLY VARIABLE TRANSMISSION (CVT) OR TECHNICAL SPECIFICATIONS)。

2.
Check driver belt identification number.


Wrong type of belt. Replace belt with an appropriate drive belt.

3.
Check for localized belt wear caused by belt slippage.


Localized wear. Replace belt.

Symptom: BELT DISINTEGRATION.

1.
Check drive belt lifetime is exceeded.


Clean CVT system and rebuild with a new drive belt.

2.
Check drive belt identification number.


Excessive belt speed. Using unspecified type of belt. Replace belt with proper type of belt.

3.
Check if pulley sheaves are clean.


Oil on pulley surfaces. Clean pulley surfaces with fine emery cloth and wipe clean using pulley flange cleaner and a cloth.


Drive/driven pulley sheaves are damaged through stones inside CVT area. Clean pulley surfaces with fine emery cloth, wipe clean with a cloth or replace drive/driven pulley sheaves and belt.

Symptom: BACK BETWEEN COGS

1.
Check drive belt condition.


Considerable use, belt wearing out. Replace.


Brittle belt condition through aging. Replace belt.
ENGINE GENERAL

Symptom: ENGINE CRANKS BUT FAIL TO START

1.
Check if spark plug connectors fit on spark plugs (refer to IGNITION SYSTEM).

2.
Check spark plugs.


Define spark plugs (no spark) or wrong spark plug gap. Readjust gap and clean spark plugs or replace.

3.
Check for fuel on spark plugs.


Flooded engine (spark plugs wet when removed). Activate engine drowned mode and crank engine with rags over the spark plug holes.

4.
Check battery voltage.


Battery is discharged and starter works not properly. Charge battery.

5.
Check fuel level in fuel tank and fuel pressure. Ensure fuel pump was not disabled.

Low or no fuel pressure. Replace defective part(s).

6.
Check fuel injectors.


Plugged or faulty injector(s). Replace defective part(s).

7.
Check idle bypass valve.


Stuck or defective.

8.
Check encoder wheel.


Bent tooth. Refer to MAGNETO SYSTEM.

9.
Check engine compression.


Insufficient engine compression. Replace defective part(s).

10.
Check fault codes in DIAGNOSTIC TOOL system.


Check if actuator(s) is/are defective. Replace defective part(s) (refer to COMPONENT INSPECTION AND ADJUSTMENT).

Symptom: ENGINE DOES NOT START

1.
Electrical problem.


                  Determine if the electrical system works correctly (fuse(s), battery, wiring harness, etc.).
 Refer to IGNITION SYSTEM.

2.
Problem with fuel system (carburetor, fuel pump, hoses, etc.).


Clean, inspect, repair or replace defective parts. 

3.
Check engine compression.


Insufficient engine compression. Replace defective parts.


Valve seat worn and/or damaged. Repair by performing valve guide procedure (refer to CYLINDER AND HEAD). Readjust valve clearance.

4.
Internal engine problem.


Overhaul engine to find defective parts. Refer to the appropriate section in ENGINE.

Symptom: ENGINE HARD TO START

1.
Check idle bypass valve.


Stuck or defective. Refer to ENGINE MANAGEMENT.

2.
Check closed throttle and idle actuator with DIAGNOSTIC TOOL

Wrong TPS zero setting/idle bypass valve reset. Refer to ENGINE MANAGEMENT.

3.
Check engine compression.


Wrong adjustment (likely too tight). Refer to ENGINE MANAGEMENT.

4.
Check engine compression.


Insufficient engine compression. Replace defective part(s) refer to LEAK TEST.

5.
Verify spark plug condition.


Defective, improperly set, worn out, fouled. Identify source of problem and correct. Replace.

6.
Check fuel level in fuel tank and fuel pressure.


Low or no fuel pressure. Replace defective part(s) refer to FUEL TANK AND FUEL PUMP.

7.
Check CAPS (camshaft position sensor).


Defective sensor/wiring. Refer to ENGINE MANAGEMENT.

Symptom: ENGINE SUDDENLY TURNS OFF

1.  Perform engine leak test.


Damaged head gasket and/or seal and/or leaking inlet/exhaust valve(s). replace and/or repair defective parts.

2.
Check spark plugs condition and/or gap.


Fouled spark plugs or wrong spark plug gap. Readjust gap and clean spark plugs or replace.

3.
Piston seizure.


Spark plugs heat range is too hot. Install spark plugs with appropriate heat range (refer to TECHNICAL SPECIFICATIONS).


Compression ratio is too high. Install genuine parts.


Poor oil quality. Use recommended oil.


Leaks at air intake manifold (engine gets too lean). Retighten screws or replace air intake manifold gasket.


Snow/water intrusion through intake system into combustion chamber. Clean intake system and replace defective part(s).

4.
Melted and/or perforated piston dome; melted section at ring end gap.


Spark plugs heat range is too hot. Install recommended spark plugs (refer to TECHNICAL SPECIFICATIONS).


Coolant less than recommended level (engine gets too hot). Repair cooling circuit and/or refill with recommended liquid.


Poor quality and/or wrong fuel. Clean from contamination and use appropriate fuel (refer to TECHNICAL SPECIFICATIONS).

5.
Piston color is dark due to seizure on intake and exhaust side.


Cooling system leaks and lowers coolant level. Tighten clamps or replace defective parts. Add antifreeze in cooling system until appropriate level reached. Replace damaged parts. 

6.
Cracked or broken piston.


Cracked or broken piston due to excessive piston/cylinder clearance or engine overheating. Replace piston. Check piston/cylinder clearance (refer to CYLINDER AND HEAD).

7.
Check piston rings and cylinder surface for grooves.


Poor oil quality. Use recommended oil.


Contamination through engine intake. Replace defective part(s) and use new air filter.

8.
Check crankshaft, rocker arms movement.


Oil pump failure due to lack of oil. Repair and replace defective parts and use new recommended oil.


Oil contamination due to clogged oil filter/oil strainer. Replace oil and oil filter at the same time, replace defective part(s).

9.
Check valve springs exhaust/intake.


Broken valve spring damages the cylinder head, valve(s), rocker arm(s), piston, piston rings and connecting rod. Replace defective part(s).

10.
Check if fuel supply is sufficient.


Low fuel level.


Clogged fuel filter or fuel injector filter.


Fuel line is contaminated and/or bent. Clean and/or replace defective part(s).
          11. Check fault codes in Diagnostic Tool.
                    Check if electrical actuators is defective. Replace defective parts.

Symptom: ENGINE BACKFIRES

1.
Check spark plugs.


Carbon accumulation caused by defective spark plugs. Replace spark plugs.

2.
Check leakage on intake manifold.


Air leak on intake system. Retighten screws and/or replace intake manifold gasket.

3.
Check exhaust air leaking.


Exhaust gasket is leaking. Retighten screws and/or replace exhaust gasket.

4.
Check intake valve(s) for leaking.


Intake valve(s) is (are) leaking. Repair or replace valve(s).

5.
Check if fuel supply is sufficient.


Fuel line is contaminated and/or bent (engine gets lean). Clean and/or replace defective part(s).

6.
Check engine ground.


Poor engine ground. Clean.
7.  Check fault codes in Diagnostic Tool.
                    Check if electrical actuators is defective. Replace defective parts.
Symptom: ENGINE DOES NOT OFFER MAXIMUM POWER AND/OR DOES NOT REACH MAXIMUM OPERATING RPM

1.
Check spark plugs condition and/or gap.


Fouled spark plugs or wrong spark plug gap. Readjust gap and clean spark plugs or replace.

2.
Check spark plugs type.


Improper spark plugs heat range. Install recommended spark plugs (refer to TECHNICAL SPECIFICATIONS).

3.
Perform engine leak test.


Damaged head gasket and/or seal and/or leaking intake/exhaust valve(s). replace and/or repair defective parts.

4.
Check for water in fuel (wrong fuel).


There is water in fuel or wrong fuel. Drain fuel system, search for leakage and refill it with appropriate fuel.

5.
Check engine compression.


Worn piston(s) and/or piston ring(s). Replace defective part(s).

6.
Check fuel pressure.


Low fuel pressure. Perform fuel pressure test (refer to FUEL SYSTEM).

7.
Check air intake system.


Air filter is clogged due to contamination. Replace air filter.

8.
Check if EMS (engine management system) is in limp home mode. Check fault codes in DIAGNOSTIC TOOL system.


Check if electrical actuator(s) is/are defective. Replace defective part(s).

9.
Check drive belt.


Worn. Replace belt if its width is less than specified.

Symptom: HIGH ENGINE OPERATING TEMPERATURE

1.
Check if cooling system shows any failure (see COOLING SYSTEM).


System is leaking. Repair and/or replace damaged part(s).

2.
Check function of lubrication system (see LUBRICATION SYSTEM).


Lubrication is not working properly. Repair and/or replace damaged part(s).

3.
Check condition and heat range of spark plugs.


Melted spark plug tip or inadequate heat range. Replace.

4.
Check air leakage on engine intake.


Leakage causes overheating. Replace/repair damaged part(s).

5.
Check air inlet and outlet of the CVT cover.


Air circulation is clogged (overheating). Clean air circulation from contamination.


Drive belt worn and/or damaged. Replace belt with an appropriate drive belt (refer to TECHNICAL SPECIFICATIONS).

14.SPECIFICATIONS

	Item
	Parameter

	Dimensions
	Long 
	Short

	Overall length (mm)
	2215
	2055

	Overall width (mm)
	1172
	1172

	Overall height (mm)
	1260
	1260

	Wheelbase (mm)
	1460
	1300

	Ground clearance (mm)
	265
	265

	Engine

	Type
	Single cylinder, Four-stroke, liquid-cooled, SOHC

	Number of valves
	4 (mechanical adjustment)

	Cylinder diameter
	91 mm

	Piston stroke
	ATV525 
	76.2 mm

	
	ATV625
	89.2 mm

	Compression ratio
	10.7:1

	Displacement
	ATV525 
	495 cm3

	
	ATV625
	580 cm3

	Maximum power
	ATV525 
	28 kW/6800 rpm

	
	ATV625
	31 kW/6500 rpm

	Maximum torque
	ATV525 
	46 Nm/5800 rpm

	
	ATV625
	51 Nm/5000 rpm

	Idle speed
	1500±100rpm

	Lubrication
	Type
	Wet tank lubrication, oil filters can be changed

	
	Oil pressure
	0.25~0.35 MPa at 1500 rpm

	
	Type of oil
	SAE5W-40 SJ

	
	Oil quantity
	2800 mL

	
	Replacement of capacity
	2500 mL

	Fuel
	Type
	Unleaded gasoline only 92# or higher

	
	Fuel pressure
	350 KPa

	
	Fuel tank capacity
	20 L

	Valve clearance
	Intake
	0.08 to 0.1 mm

	
	Exhaust
	0.08 to 0.1 mm

	Spark plug
	Type/manufacturer
	CR8EKB

	
	Gap
	0.8 to 1.0 mm

	Transmission type
	CVT (Continuously Variable Transmission)

	Continuously variable ratio
	0.646 to 2.87

	Drive belt width
	Service limit
	30.00 mm

	Gearbox type
	Dual range(H/L) with park, neutral and reverse

	Gear ratio
	H
	ATV525 
	3.5

	
	
	ATV625
	1.35

	
	L
	ATV525 
	6.562

	
	
	ATV625
	2.53

	
	R
	ATV525 
	5.369

	
	
	ATV625
	2.07

	Capacity of cooling liquid
	Type
	Ethyl glycol/water mix (-35℃)

	
	Maximum load
	3200 ml (General version)

	
	
	3600 ml (MUD version)

	
	Capacity of water tank
	300 ml

	Cooling liquid temperature thermostat
	Valve opening
	65℃

	
	Fan opening
	88℃

	Tire

	Type
	Tubeless

	Pressure
	45 KPa

	Size Front
	AT25x8-12 (Rim12x6)

	Size Rear
	AT25x10~12 (Rim12x7)

	Brake

	System
	Front and rear unified

	Type Front
	Dual disc brake

	Type Rear
	Dual disc brake

	Operation
	Foot/hand operation

	Suspension and shock absorber

	Front suspension
	Double A-Arm independent 

	Rear suspension
	Double A-Arm independent with 

external stabilizer bar

	Front shock absorber
	Airbag shock absorption / oil damper

	Front shock absorber travel
	180 mm

	Rear shock absorber
	Airbag shock absorption / oil damper

	Rear shock absorber travel
	220 mm

	Drive train

	Front differential
	Shaft driven/single auto-lock differential

	Front differential ratio
	3.67:1

	Rear axle
	Shaft driven/single differential

	Rear axle ratio
	3.67:1

	Front differential oil capacity
	230 mL (GL-5 80W90)

	Rear differential oil capacity
	230 mL (GL-5 80W90)

	Electrical

	Ignition system
	EFI

	Battery
	Type
	Maintenance Free

	
	Voltage
	12 V

	
	capacity
	20 AH

	Fuses
	F1
	Ignition Switch
	15 A

	
	F2
	Combination Switch
	15 A

	
	F3
	2WD/4WD Switch
	10 A

	
	F4
	Winch
	5 A

	
	F5
	Fan
	30 A

	
	F6
	Backup power
	20 A

	
	F7
	EFI
	20 A

	
	F8
	Light power supply
	15 A

	Relays
	RY 1
	Light Relay
	-

	
	RY 2
	Combination Switch Relay
	-

	
	RY 3
	EFI Relay
	-

	
	RY 4
	2WD/4WD Switch Relay 1
	-

	
	RY 5
	2WD/4WD Switch Relay 2
	-

	
	RY 6
	Fan Relay
	-

	
	RY 7
	Fuel Pump Relay
	-

	
	RY 8
	Handlebar Heating Relay
	-

	
	RY 9
	Overtaking light Relay
	-

	
	RY 10
	Right trailer steering Relay
	-

	
	RY 11
	Left trailer steering Relay
	-

	
	RY 12
	Rear fog light Relay
	-
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Brake light switch
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